{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Disclaimer","Parameter->PN","PN->Parameter","Film Data","Utility"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":1,"defined_names":21,"comments":1,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Disclaimer","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Parameter->PN","index":1,"n_rows":7134,"n_cols":66,"rows_kept":1125,"cut":true,"hidden":false,"merged":[[0,57,1,58]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["Panasonic Standard Film Capacitor Quick Search",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"COUNTA(BC:BC)-1","v":7129}]
["Please select parameters below to find the capacitors to match your requirements."]
["Filters",null,null,null,null,"Last data update - 29.Sep.2023",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Output"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"V",null,"C",null,null,"L","W","H","P1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tolerance ddd","Type","Rated \nVoltage (V)","Voltage type","Capacitance\n(uF)","Tolerance on capacitance\n(%)","Tangent\nof Loss \nAngle\n(at 1kHz / 20°C)","Body length / dia\n(mm)","Body width\n(mm)","Height\n(mm)","Lead Space P1\n(mm)","Category Temperature Range \n(°C)","MOQ\n(pcs)","Dielectric Material","Automotive grade","Series","PartNumber",null,null,"URL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"box",250,"AC",12,"±10","(空白)",48.5,22,36,45.6,"-25 to 85",200,"PP","No","EZPQ","EZPQ25126LTA",null,null,{"$f":"IF(BC6=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC6,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25126LTA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,"±10","(空白)",57.5,30,45,52.5,"-25 to 85",50,"PP","No","EZPQ","EZPQ25226LTA",null,null,{"$f":"IF(BC7=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC7,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25226LTA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,"±10","(空白)",57.5,35,56,52.5,"-25 to 85",50,"PP","No","EZPQ","EZPQ25366LTA",null,null,{"$f":"IF(BC8=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC8,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25366LTA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,450,"DC",0.1,"±10","(空白)",13,5,10.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W104K",null,null,{"$f":"IF(BC9=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC9,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W104KA",null,null,{"$f":"IF(BC10=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC10,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W104Q5",null,null,{"$f":"IF(BC11=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC11,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104Q5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W104QD",null,null,{"$f":"IF(BC12=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC12,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104QD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",13,5,10.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W104J",null,null,{"$f":"IF(BC13=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC13,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104J"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W104JA",null,null,{"$f":"IF(BC14=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC14,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104JA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W104P5",null,null,{"$f":"IF(BC15=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC15,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104P5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W104PD",null,null,{"$f":"IF(BC16=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC16,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104PD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,"±10","(空白)",13,5,10.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W154K",null,null,{"$f":"IF(BC17=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC17,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W154KA",null,null,{"$f":"IF(BC18=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC18,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W154Q5",null,null,{"$f":"IF(BC19=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC19,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154Q5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W154QD",null,null,{"$f":"IF(BC20=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC20,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154QD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",13,5,10.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W154J",null,null,{"$f":"IF(BC21=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC21,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154J"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W154JA",null,null,{"$f":"IF(BC22=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC22,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154JA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W154P5",null,null,{"$f":"IF(BC23=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC23,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154P5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W154PD",null,null,{"$f":"IF(BC24=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC24,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154PD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.22,"±10","(空白)",13,6,12,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W224K",null,null,{"$f":"IF(BC25=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC25,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W224KA",null,null,{"$f":"IF(BC26=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC26,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W224Q5",null,null,{"$f":"IF(BC27=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC27,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224Q5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W224QD",null,null,{"$f":"IF(BC28=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC28,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224QD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",13,6,12,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W224J",null,null,{"$f":"IF(BC29=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC29,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224J"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W224JA",null,null,{"$f":"IF(BC30=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC30,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224JA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W224P5",null,null,{"$f":"IF(BC31=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC31,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224P5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W224PD",null,null,{"$f":"IF(BC32=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC32,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224PD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.33,"±10","(空白)",13,6,12,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W334K",null,null,{"$f":"IF(BC33=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC33,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W334KA",null,null,{"$f":"IF(BC34=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC34,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W334Q5",null,null,{"$f":"IF(BC35=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC35,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334Q5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W334QD",null,null,{"$f":"IF(BC36=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC36,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334QD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",13,6,12,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W334J",null,null,{"$f":"IF(BC37=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC37,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334J"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W334JA",null,null,{"$f":"IF(BC38=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC38,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334JA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W334P5",null,null,{"$f":"IF(BC39=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC39,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334P5"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W334PD",null,null,{"$f":"IF(BC40=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC40,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334PD"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.47,"±10","(空白)",13,7,12.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W474Q1",null,null,{"$f":"IF(BC41=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC41,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474Q1"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W474QA",null,null,{"$f":"IF(BC42=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC42,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474QA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,6,11.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W474K",null,null,{"$f":"IF(BC43=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC43,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W474KA",null,null,{"$f":"IF(BC44=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC44,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",13,7,12.5,10,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W474P1",null,null,{"$f":"IF(BC45=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC45,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474P1"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W474PA",null,null,{"$f":"IF(BC46=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC46,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474PA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,6,11.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W474J",null,null,{"$f":"IF(BC47=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC47,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474J"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W474JA",null,null,{"$f":"IF(BC48=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC48,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474JA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.68,"±10","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W684K",null,null,{"$f":"IF(BC49=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC49,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W684K"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W684KA",null,null,{"$f":"IF(BC50=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH('Parameter->PN'!BC50,'Film Data'!G:G,0))))","v":"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W684KA"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W684J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W684JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"±10","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W105K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W105KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2W105J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W105JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,"±10","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2W155KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2W155K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,9,19,27.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2W155QL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWFE","ECWFE2W155Q8"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2W155JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2W155J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,9,19,27.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2W155PL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWFE","ECWFE2W155P8"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"±10","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2W225KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2W225K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,11,21,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W225Q8"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W225QL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2W225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2W225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,11,21,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W225P8"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W225PL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"±10","(空白)",26,10,17,22.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2W335KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWFE","ECWFE2W335K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,13,23,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W335Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W335QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,10,17,22.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2W335JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWFE","ECWFE2W335J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,13,23,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W335P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2W335PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"±10","(空白)",26,12,19,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W475KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWFE","ECWFE2W475K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,15.5,25.5,27.5,"-40 to 105 (85)",100,"PP","No","ECWFE","ECWFE2W475QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","No","ECWFE","ECWFE2W475Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,12,19,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2W475JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWFE","ECWFE2W475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,15.5,25.5,27.5,"-40 to 105 (85)",100,"PP","No","ECWFE","ECWFE2W475PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","No","ECWFE","ECWFE2W475P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66,"±15","(空白)",32.5,90,24,27.5,"-25 to 70",50,"PP","No","EZPE [Low profile]","EZPE45666MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"DC",10,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE50106LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE50156LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE50206LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE50256LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE50306MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50356MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50406MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50456MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50506MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50556MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE50606MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50656MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50706MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50756MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,80,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50806MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50856MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50906MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50956MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50107MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE50117MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,525,"DC",29,"±15","(空白)",37,48.5,23.5,34,"-25 to 70",100,"PP","No","EZPE [Low profile]","EZPE52296MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,575,"DC",12,"±15","(空白)",41.5,24.5,19.5,37.5,"-25 to 70",200,"PP","No","EZPE [Low profile]","EZPE57126LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,630,"DC",0.1,"±10","(空白)",17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J104K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J104KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J104QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J104Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,5,10.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J104J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J104JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J104PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J104P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15,"±10","(空白)",17.5,6,11.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J154K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J154KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J154QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J154Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,6,11.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J154J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J154JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J154PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J154P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.22,"±10","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J224K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J224KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J224QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J224Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,7,12.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFE","ECWFE2J224J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J224JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,6,13,22.5,"-40 to 105 (85)",700,"PP","No","ECWFE","ECWFE2J224PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWFE","ECWFE2J224P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.33,"±10","(空白)",17.5,8.5,14.5,15,"-40 to 105 (85)",800,"PP","No","ECWFE","ECWFE2J334KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2J334K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,7,14,22.5,"-40 to 105 (85)",500,"PP","No","ECWFE","ECWFE2J334QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"PP","No","ECWFE","ECWFE2J334Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,8.5,14.5,15,"-40 to 105 (85)",800,"PP","No","ECWFE","ECWFE2J334JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2J334J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,7,14,22.5,"-40 to 105 (85)",500,"PP","No","ECWFE","ECWFE2J334PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"PP","No","ECWFE","ECWFE2J334P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.47,"±10","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2J474KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2J474K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,8,15,22.5,"-40 to 105 (85)",400,"PP","No","ECWFE","ECWFE2J474QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,"PP","No","ECWFE","ECWFE2J474Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,10,15.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2J474JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFE","ECWFE2J474J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,8,15,22.5,"-40 to 105 (85)",400,"PP","No","ECWFE","ECWFE2J474PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,"PP","No","ECWFE","ECWFE2J474P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.68,"±10","(空白)",17.5,11,17.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2J684K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J684KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",17.5,11,17.5,15,"-40 to 105 (85)",600,"PP","No","ECWFE","ECWFE2J684J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J684JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"±10","(空白)",26,10,17,22.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2J105KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWFE","ECWFE2J105K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,10.5,19,22.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG2J105QA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG2J105Q1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,9,19,27.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2J105QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWFE","ECWFE2J105Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,9.5,18,27.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG2J105KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG2J105K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,10,17,22.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2J105JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWFE","ECWFE2J105J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,10.5,19,22.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG2J105PA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG2J105P1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,9,19,27.5,"-40 to 105 (85)",300,"PP","No","ECWFE","ECWFE2J105PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWFE","ECWFE2J105P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,9.5,18,27.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG2J105JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG2J105J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,"±10","(空白)",26,12,19,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J155KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWFE","ECWFE2J155K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,12,21,22.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG2J155Q1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J155QA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,11,21,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J155Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J155QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG2J155K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J155KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,12,19,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J155JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWFE","ECWFE2J155J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,12,21,22.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG2J155P1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J155PA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,11,21,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J155P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J155PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG2J155J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J155JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"±10","(空白)",26,16,23,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J225K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J225KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,15.5,24,22.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG2J225Q1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG2J225QA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,13,23,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J225Q5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J225QD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG2J225K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG2J225KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,16,23,22.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,15.5,24,22.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG2J225P1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG2J225PA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,13,23,27.5,"-40 to 105 (85)",200,"PP","No","ECWFE","ECWFE2J225P5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFE2J225PD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG2J225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG2J225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"±10","(空白)",27,17.5,26.5,22.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG2J305Q1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J305QA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG2J305K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J305KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",27,17.5,26.5,22.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG2J305P1"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J305PA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG2J305J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J305JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"±10","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG2J475K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J475KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG2J475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG2J475JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"±15","(空白)",41.5,24.5,19.5,37.5,"-25 to 70",200,"PP","No","EZPE [Low profile]","EZPE63106LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"DC",2,"± 5","(空白)",31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG80205J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80205JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"± 5","(空白)",31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG80225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG80275J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG80275JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG80305J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG80305JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG80335J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG80335JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.9,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG80395JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80395J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG80475JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.6,"± 5","(空白)",31.5,16,29.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80565JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80565J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.8,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80685JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80685J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"±10","(空白)",31,20.5,41.5,27.5,"-40 to 105 (85)",200,"PP","Yes","EZPV","EZPV80106LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80106MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80106LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80106MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE80106LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV80106LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80106LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"±10","(空白)",31,20.5,41.5,27.5,"-40 to 105 (85)",200,"PP","Yes","EZPV","EZPV80126LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80126MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80126LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80126MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80126LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80126LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE80156MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80156MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80156MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE80206MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,26,40.5,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80206MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80206MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE80256MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80256MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80256MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80256MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80256MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE80306MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80306MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80306MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80306MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80306MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"±10","(空白)",41.5,30,56,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80356MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80356MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80356MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80356MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE80356MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"±10","(空白)",57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80406MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80406MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE80406MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,38,52.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80406MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80406MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"±10","(空白)",57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80456MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80456MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE80456MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,38,57,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80456MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80456MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"±10","(空白)",57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80506MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80506MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE80506MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,43,58,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV80506MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80506MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE80556MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80556MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80556MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"±10","(空白)",57.5,35,56,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80606MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80606MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE80606MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,"±10","(空白)",57.5,35,64.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV80656MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80656MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG80405J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80405JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"± 5","(空白)",31.5,16,29.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80505JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80505J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV80805LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80805LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80805JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80805J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"±10","(空白)",31,20.5,41.5,27.5,"-40 to 105 (85)",200,"PP","Yes","EZPV","EZPV80905LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80905MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80905LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80905MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV80905LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80905LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"± 5","(空白)",31.5,16,29.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80605JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80605J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80705JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80705J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"±10","(空白)",31,22,53.5,27.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80186LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80186MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80186LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80186MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG80355J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG80355JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,"±10","(空白)",31,26,41,27.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80146LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80146MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80146LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80146MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG80755JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG80755J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,"±10","(空白)",31,20.5,41.5,27.5,"-40 to 105 (85)",200,"PP","Yes","EZPV","EZPV80116LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80116MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80116LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80116MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,"±10","(空白)",31,26,41,27.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV80136LTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80136MTU"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV80136LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPV80136MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"DC",3,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1A305LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A305LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1A475LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A475LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"±10","(空白)",41.5,23.5,43.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A106MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A106MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"±10","(空白)",41,26,40.5,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1A126MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A126MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A156MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A156MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1A156MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A156MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",41.5,30,56,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A206MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A206MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.5,35.5,45.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1A206MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A206MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",57.5,35.5,45.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1A256MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A256MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,38,52.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A256MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A256MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"±10","(空白)",57.5,35,50,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1A306MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A306MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,43,58,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A306MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A306MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"±10","(空白)",57.5,35,56,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1A356MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A356MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"±10","(空白)",57.5,35,56,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1A406MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A406MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1A405LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A405LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1A505LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A505LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1A805MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A805MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1A905MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A905MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1A605LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A605LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1A705MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A705MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"±10","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1A186MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1A186MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1100,"DC",1,"± 5","(空白)",31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG1B105J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG1B105JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG1B155J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG1B155JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG1B205J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG1B205JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG1B225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG1B225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1B305LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B305LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,16,29.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG1B305JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG1B305J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"± 5","(空白)",31.5,16,29.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG1B335JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG1B335J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1B475LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B475LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,18.5,35,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG1B475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG1B475JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"±10","(空白)",41.5,20,42,37.5,"-25 to 70",150,"PP","No","EZPE","EZPE1B106MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,43.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B106MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B106MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"±10","(空白)",41,26,40.5,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1B126MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B126MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE1B156MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B156MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B156MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1B156MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B156MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE1B206MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B206MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B206MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.5,35.5,45.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1B206MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B206MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE1B256MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35.5,45.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1B256MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B256MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,38,52.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B256MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B256MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE1B306MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,50,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1B306MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B306MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,43,58,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B306MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B306MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"±10","(空白)",57.5,35,56,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1B356MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B356MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE1B356MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"±10","(空白)",57.5,35,56,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV1B406MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B406MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-25 to 70",50,"PP","No","EZPE","EZPE1B406MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1B405LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B405LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG1B405J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG1B405JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1B505LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B505LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,18.5,35,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG1B505J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG1B505JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1B805MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B805MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1B905MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B905MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV1B605LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B605LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV1B705MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B705MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,"±10","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV1B186MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV1B186MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,"DC",10,"±10","(空白)",41.5,30,51,37.5,"-25 to 70",100,"PP","No","EZPE","EZPE1D106MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE1D156MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",57.5,30,51,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE1D206MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",57.5,35,56,52.5,"-25 to 70",50,"PP","No","EZPE","EZPE1D256MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,600,"DC",2,"± 5","(空白)",31.5,8,17,27.5,"-40 to 110",400,"PP","Yes","ECWFG","ECWFG60205J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG60205JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"± 5","(空白)",31.5,8,17,27.5,"-40 to 110",400,"PP","Yes","ECWFG","ECWFG60225J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG60225JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7,"± 5","(空白)",31.5,9.5,18,27.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG60275JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG60275J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,"± 5","(空白)",31.5,9.5,18,27.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG60305JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG60305J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"± 5","(空白)",31.5,9.5,18,27.5,"-40 to 110",350,"PP","Yes","ECWFG","ECWFG60335JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","Yes","ECWFG","ECWFG60335J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.9,"± 5","(空白)",31.5,10.5,21,27.5,"-40 to 110",300,"PP","Yes","ECWFG","ECWFG60395JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG60395J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG60475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG60475JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.6,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG60565J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG60565JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.8,"± 5","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG60685J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG60685JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.1999999999999993,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG60825J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG60825JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV60106LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60106LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,13.5,28.5,27.5,"-40 to 110",150,"PP","Yes","ECWFG","ECWFG60106J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFG60106JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"±10","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV60126LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60126LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",31.5,17.5,32.5,27.5,"-40 to 110",100,"PP","Yes","ECWFG","ECWFG60126JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,"PP","Yes","ECWFG","ECWFG60126J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"±10","(空白)",41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV60156LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60156LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60206MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60206MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"±10","(空白)",41,22,36,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60256MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60256MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"±10","(空白)",41,26,40.5,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60306MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60306MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"±10","(空白)",41,26,40.5,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60356MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60356MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,"±10","(空白)",41.5,27.5,42,37.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60406MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60406MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60406MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60406MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"±10","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV60456MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60456MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60456MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60456MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,50,"±10","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV60506MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60506MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,25,40,52.5,"-40 to 105 (85)",150,"PP","Yes","EZPV","EZPV60506MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60506MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,55,"±10","(空白)",57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV60556MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60556MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV60556MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60556MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"±10","(空白)",41.5,30,56,37.5,"-40 to 105 (85)",100,"PP","Yes","EZPV","EZPV60606MTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60606MTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV60606MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV60606MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,75,"±10","(空白)",57.5,30,51,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV60756MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,100,"±10","(空白)",57,40,51.5,52.5,"-40 to 105 (85)",50,"PP","Yes","EZPV","EZPV60107MTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG60505JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,"±10","(空白)",41.5,17,34.5,37.5,"-40 to 105 (85)",300,"PP","No","EZPQ","EZPQ60155LTD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,"±10","(空白)",57.5,45,62,52.5,"-40 to 105 (85)",50,"PP","No","EZPQ","EZPQ60126MTD"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,35,"± 5","(空白)",57.5,45,62,52.5,"-40 to 105 (85)",50,"PP","No","EZPQ","EZPQ33356MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"± 5","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","No","EZPQ","EZPQ38205LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EZPQ38106MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,"± 5","(空白)",41,30,50.5,37.5,"-40 to 105 (85)",100,"PP","No","EZPQ","EZPQ38905LTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5,"± 5","(空白)",41,15,29,37.5,"-40 to 105 (85)",300,"PP","No","EZPQ","EZPQ38255LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,250,"PP","Yes","ECWFG","ECWFG70205KA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"±10","(空白)",31.5,12,24.5,27.5,"-40 to 110",200,"PP","Yes","ECWFG","ECWFG70225K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,17,34.5,37.5,"-40 to 105 (85)",300,"PP","Yes","EZPV","EZPV70106LTT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV70126LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV70356MTC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV70805LTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No","EZPV","EZPV70905MTA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"chip",16,"DC",1E-4,"± 5","(空白)",1.6,0.8,0.7,"'-","-55 to 125",4000,"PPS","No","ECHU(X)","ECHU1C101JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",1.6,0.8,0.7,"'-","-55 to 125",4000,"PPS","No","ECHU(X)","ECHU1C181GX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",1.6,0.8,0.7,"'-","-55 to 125",4000,"PPS","No","ECHU(X)","ECHU1C821GX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",2,1.25,0.9,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1C562GX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.2000000000000007E-3,"± 5","(空白)",2,1.25,1.1000000000000001,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1C822JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.6000000000000001E-2,"± 5","(空白)",3.2,2.5,1.5,"'-","-55 to 125",2000,"PPS","No","ECHU(X)","ECHU1C563JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",3.2,2.5,2.1,"'-","-55 to 125",2000,"PPS","No","ECHU(X)","ECHU1C104GX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",2,1.25,0.9,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1H391GX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.1999999999999998E-4,"± 5","(空白)",2,1.25,0.9,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1H821JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5999999999999999E-3,"± 5","(空白)",3.2,1.6,0.9,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1H562JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7E-2,"± 5","(空白)",3.2,2.5,1.5,"'-","-55 to 125",2000,"PPS","No","ECHU(X)","ECHU1H273JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",4.8,3.3,1.5,"'-","-55 to 125",3000,"PPS","No","ECHU(X)","ECHU1H473GX9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",6,4.0999999999999996,2.8,"'-","-55 to 125 (105)",2000,"PPS","No","ECHU(X)","ECHU1H224GX9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3E-3,"± 5","(空白)",3.2,1.6,1.5,"'-","-55 to 105",2000,"PEN","No","ECWU(X)","ECWU1332JX5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",4.8,3.3,2,"'-","-55 to 105",3000,"PPS","No","ECHU(C)","ECHU1183GC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 2","(空白)",6,4.0999999999999996,2,"'-","-55 to 105",3000,"PPS","No","ECHU(C)","ECHU1393GC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,4.0999999999999996,2.8,"'-","-55 to 105",2000,"PPS","No","ECHU(C)","ECHU1563JC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",6,4.0999999999999996,2.8,"'-","-55 to 125 (85)",2000,"PEN","No","ECWU(C)","ECWU1154JC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.18,"±10","(空白)",7.1,5,2,"'-","-55 to 125 (85)",1500,"PEN","No","ECWU(C)","ECWU1184KC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5E-3,"±10","(空白)",4.8,3.3,1.4,"'-","-55 to 125 (85)",3000,"PEN","No","ECWU(C)","ECWU2152KC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",4.8,3.3,1.4,"'-","-55 to 85",3000,"PEN","No","ECWU(V16)","ECWU2392V16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-55 to 125 (85)",3000,"PEN","No","ECWU(C)","ECWU2562JC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.01,"±10","(空白)",4.8,3.3,1.4,"'-","-55 to 125 (85)",3000,"PEN","No","ECWU(C)","ECWU2103KC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",4.8,3.3,2.4,"'-","-55 to 85",2000,"PEN","No","ECWU(V16)","ECWU2273V16"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.1,"±10","(空白)",6,5,3.8,"'-","-55 to 125 (85)",1500,"PEN","No","ECWU(C)","ECWU2104KC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.12,"±10","(空白)",6,5,4.5,"'-","-55 to 125 (85)",1500,"PEN","No","ECWU(C)","ECWU2124KC9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1684KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE1824KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.8,5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE1125KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.399999999999999,5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE1185KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.399999999999999,6.5,19.399999999999999,5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE1185JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1275KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.5,5,"-40 to 105 (85)",400,"PET","No","ECQE(F)[DC]","ECQE1335KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE1475KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",26,10,20,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE1825JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE1106JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",7.9,4.2,7.1,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2103JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2103JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,"PET","No","ECQE(B)[DC]","ECQE2123KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,"PET","No","ECQE(B)[DC]","ECQE2123JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(F)[DC]","ECQE2153RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 105 (85)",1500,"PET","No","ECQE(T)[DC]","ECQE2153JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.3,4.4000000000000004,7.5,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2183KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.8,4.4000000000000004,7.5,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2183JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(T)[DC]","ECQE2183RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE2223JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2273KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",7.9,4.3,7.2,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2273JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2333KF9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(F)[DC]","ECQE2333RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(B)[DC]","ECQE2393KB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(F)[DC]","ECQE2393RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 105 (85)",1500,"PET","No","ECQE(T)[DC]","ECQE2393JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.3,4.5,7.5,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2473KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2473JF9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2563KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.9,5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE2563JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2683KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",7.9,5.0999999999999996,8,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2683JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.6,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2823KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2823JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2104KB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2104JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.8,5.8,8.4,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2104JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.8,6,9,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2124KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2124JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2124HAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2154JB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2154JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2184KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.3,5,"-40 to 105 (85)",800,"PET","No","ECQE(T)[DC]","ECQE2184KT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",13,5.9,15.1,7.5,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2184HAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",1000,"PET","No","ECQE(B)[DC]","ECQE2224RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,5.5,10.5,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2224JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,6,11.5,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2274KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE2274RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2274JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.33,"±10","(空白)",10.3,6.4,11.3,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2334KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2334JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2394KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE2394KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,4.9000000000000004,12,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2394JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.47,"±10","(空白)",12.3,6.2,11.4,10,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2474KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",1000,"PET","No","ECQE(B)[DC]","ECQE2474RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2474JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",800,"PET","No","ECQE(T)[DC]","ECQE2564RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",800,"PET","No","ECQE(T)[DC]","ECQE2564RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[DC]","ECQE2684KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWF(A)","ECWF2684JAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,6,13.5,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2684JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",15.3,6.3,13.3,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2824JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18.100000000000001,8,17.600000000000001,7.5,"-40 to 105 (85)",400,"PP","No","ECWF(A)","ECWF2824RHA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.4,15,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2105KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.3,15,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2105JAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2105JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.600000000000001,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2125JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18.8,9.5,14.6,15,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2125HA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",300,"PET","No","ECQE(B)[DC]","ECQE2155RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.8,5,"-40 to 105 (85)",400,"PET","No","ECQE(T)[DC]","ECQE2155KT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,9,16.8,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2155JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.8,7.6,14.6,17.5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[DC]","ECQE2185JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,7.5,15.5,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2185JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.6,15,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2225JAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26.5,8.5,16.3,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2225JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",300,"PET","No","ECQE(B)[DC]","ECQE2275RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26.5,10.3,18,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2335KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PP","No","ECWF(A)","ECWF2335JAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2395KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.3,12.5,"-40 to 105 (85)",500,"PP","No","ECWF(A)","ECWF2395JAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2475KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,11.8,21,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE2565KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2565JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2685JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28.5,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE2825KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2106JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2A103KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.5,6,11.5,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A123JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.5,5.5,14.9,7.5,"-40 to 85",1000,"PET","No","ECQE(F)[AC]","ECQE2A153RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.3,9.9,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE2A153JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A223KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.5,5,"-40 to 85",700,"PET","No","ECQE(T)[AC]","ECQE2A223KT6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",1000,"PET","No","ECQE(F)[AC]","ECQE2A273RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",1000,"PET","No","ECQE(F)[AC]","ECQE2A333RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.399999999999999,7.5,"-40 to 85",1000,"PET","No","ECQE(F)[AC]","ECQE2A393RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.5,6.5,14.4,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A473JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE2A473JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A683KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,6.3,12,15,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE2A823KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,6.3,12,15,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE2A823JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,6.3,14,15,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE2A104KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE2A124KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.399999999999999,5,"-40 to 85",500,"PET","No","ECQE(T)[AC]","ECQE2A154JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,5,"-40 to 85",500,"PET","No","ECQE(T)[AC]","ECQE2A184KT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",18.5,9,16.899999999999999,15,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A224JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.27,"±10","(空白)",26,7,16.5,22.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A274KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,15,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A334JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,15,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE2A474JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4103KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(T)[DC]","ECQE4103RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.8,4.4000000000000004,7.5,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4123KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.8,4.4000000000000004,7.5,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4153KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4183KF9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(T)[DC]","ECQE4183RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(F)[DC]","ECQE4223RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4223JF9"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7E-2,"±10","(空白)",10.3,5.5,8,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4273KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4273KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",12.5,6.2,9,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4273HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,5,"-40 to 105 (85)",1000,"PET","No","ECQE(T)[DC]","ECQE4333KT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",12.5,6.7,9.5,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4333HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE4393RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,4.9000000000000004,8,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4393KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.2999999999999997E-2,"± 5","(空白)",12.5,6,8.8000000000000007,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4433JL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.3,5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE4473KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.3,5,"-40 to 105 (85)",900,"PET","No","ECQE(T)[DC]","ECQE4473JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4563KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",900,"PET","No","ECQE(T)[DC]","ECQE4563RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWF(L)","ECWF4623RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE4683RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4683JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.4999999999999997E-2,"± 5","(空白)",13,7.3,10.1,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4753JL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4823JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.7,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4913HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4104KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4104JLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWF(L)","ECWF4114RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4124JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE4154RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",15.5,7.6,12.2,12.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4154JL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.399999999999999,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4164JLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE4184RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.8,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4184HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4224KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4224JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.600000000000001,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4224HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4274KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.899999999999999,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4304HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.899999999999999,5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE4334KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,9.6,14.3,15,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4334HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.7,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4364HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",400,"PET","No","ECQE(F)[DC]","ECQE4394RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4474KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",500,"PET","No","ECQE(T)[DC]","ECQE4474RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",20.5,10.3,16.8,17.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4514HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4564KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.9,12.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4624HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,"PP","No","ECWF(L)","ECWF4754RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26.5,7.9,17.3,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4824KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",23,12.4,19.2,20,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4914HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE4105KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"±10","(空白)",26,9.5,18.899999999999999,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4125KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4125JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE4155JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,11,20.5,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE4185JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"± 5","(空白)",28,16,23.1,25,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4205JL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",28,17.5,24.8,25,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF4245HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W104KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.6,4.5999999999999996,14,5,"-40 to 110",1500,"PP","No","ECWFD","ECWFD2W124J3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1400,"PP","No","ECWFD","ECWFD2W154J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1300,"PP","No","ECWFD","ECWFD2W184K4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W224JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,6.5,15.6,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W224JAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W334KQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"PP","No","ECWF(A)","ECWF2W394RKA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"PP","No","ECWF(A)","ECWF2W394RJA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFD","ECWFD2W474PB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W474JAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.100000000000001,7,11.5,15,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W564JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 110",700,"PP","No","ECWFD","ECWFD2W684Q4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFD","ECWFD2W684PB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.100000000000001,7.5,12.1,15,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W684JA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFD","ECWFD2W824JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWF(A)","ECWF2W105RKA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W105PQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.7,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W125KAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWFD","ECWFD2W125JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.8,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W155JAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.3,15,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W185JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.3,7.5,"-40 to 110",200,"PP","No","ECWFD","ECWFD2W225K4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7,"±10","(空白)",25.3,9,13.7,22.5,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W275K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",25.3,9,13.7,22.5,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W275J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.5,22.5,"-40 to 105 (85)",100,"PP","No","ECWF(A)","ECWF2W335JAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.399999999999999,15,"-40 to 110",1000,"PP","No","ECWFD","ECWFD2W395KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFD2W475JC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE6562JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6682KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6103KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 105 (85)",900,"PET","No","ECQE(T)[DC]","ECQE6103KT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6103HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1200,"PP","No","ECWF(L)","ECWF6113RHL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE6123JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.2,5,"-40 to 105 (85)",1000,"PET","No","ECQE(F)[DC]","ECQE6153KF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6153KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1100,"PP","No","ECWF(L)","ECWF6153RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.9,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6163JLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J183KQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,4.9000000000000004,10,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6183JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14.3,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6203HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5.3,10.5,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6223JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.6,6.4,14.4,7.5,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J223JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE6273KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12,5.5,10.9,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6273JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWF(L)","ECWF6303RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12,6,11.9,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6333JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.899999999999999,5,"-40 to 105 (85)",700,"PET","No","ECQE(T)[DC]","ECQE6333JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PP","No","ECWF(L)","ECWF6363RHL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,6,13.4,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6393KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"PP","No","ECWF(L)","ECWF6393RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,6.5,13.5,10,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6473KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12,6.5,13.5,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6473JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,5,"-40 to 105 (85)",600,"PET","No","ECQE(T)[DC]","ECQE6473JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6513HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,5.4,10.5,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6563JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6563JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",500,"PET","No","ECQE(F)[DC]","ECQE6683RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.6,5,8.4,7.5,"-40 to 105 (85)",1200,"PP","No","ECWFD","ECWFD2J683J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.8,7.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6683HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.6,5.4,8.6999999999999993,7.5,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J823J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.5,8,12.4,12.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6823JL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWF(L)","ECWF6913RHL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.100000000000001,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6104JLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,6.3,14,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6104JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWF(L)","ECWF6114RHL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,6.3,14.5,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6124KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFA2J124JC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6124JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,10,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6134HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",400,"PET","No","ECQE(F)[DC]","ECQE6154RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",400,"PET","No","ECQE(F)[DC]","ECQE6154RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.18,"±10","(空白)",12.6,7.4,10.7,7.5,"-40 to 105 (85)",700,"PP","No","ECWFD","ECWFD2J184K4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE6184KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,8,16,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6184JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 105 (85)",400,"PET","No","ECQE(T)[DC]","ECQE6184RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6224KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWF(A)","ECWFA2J224JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.5,5,"-40 to 105 (85)",400,"PET","No","ECQE(T)[DC]","ECQE6224JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.5,15,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6274KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.5,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6274KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.7,12.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6274HLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J334KQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J334J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWF(A)","ECWFA2J334JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,12.5,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6364JLB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.2,9.1999999999999993,14.3,15,"-40 to 105 (85)",1000,"PP","No","ECWF(A)","ECWFA2J394J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,"PP","No","ECWF(L)","ECWF6394RJL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J474K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26.5,9.3000000000000007,18.5,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6474KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE6474JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J564J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PP","No","ECWF(A)","ECWFA2J564JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J684K"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26.5,11.5,21,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6684KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,15,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6684JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J824J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.5,"-40 to 105 (85)",1000,"PP","No","ECWF(A)","ECWFA2J824JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWFD2J105QC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,12.5,21.9,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6105KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,12.5,21.9,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6105JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31.5,12.5,21.9,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(T)[DC]","ECQE6105JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.3,22.5,"-40 to 105 (85)",1000,"PP","No","ECWFD","ECWFD2J125JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",28,17.600000000000001,24.4,25,"-40 to 105 (85)",100,"PP","No","ECWF(L)","ECWF6135HL"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,29.7,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6155KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,22.5,"-40 to 105 (85)",900,"PP","No","ECWFD","ECWFD2J185KQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE6185KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,31,19.5,29,27.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE6225KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.7,15,"-40 to 105 (85)",800,"PP","No","ECWFD","ECWFD2J225JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,700,"PP","No","ECWFD","ECWFD2J275JC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PP","No","ECWFD","ECWFD2J475KC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",25.3,18.3,23.9,22.5,"-40 to 105 (85)",300,"PP","No","ECWFD","ECWFD2J475J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PP","No","ECWH(A)","ECWH8123HAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWH8183HAC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.8,12.5,"-40 to 105 (85)",100,"PP","No","ECWH(A)","ECWH8333HAQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PP","No","ECWH(A)","ECWH8473RHA"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10122JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH10162RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10182HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH10222RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10272HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH10392RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10472HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5999999999999999E-3,"± 5","(空白)",18,6.5,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10562JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH10682RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10752HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE10103JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE10123KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10123JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE10153JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10153HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10183HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10203JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10243JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE10273KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10303HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10363HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE10393KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE10473KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH10473RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE10563JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,7.5,"-25 to 105 (85)",300,"PP","No","ECWH(V)","ECWH10683RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10753JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9.0999999999999998E-2,"± 5","(空白)",23,11.5,20.5,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH10913JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,7.5,"-40 to 105 (85)",300,"PET","No","ECQE(F)[DC]","ECQE10104RKF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE10124KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE10154KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1250,"DC",1E-3,"± 5","(空白)",18,6.5,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12102JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH12122RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12132HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,7,14,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12182HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH12202RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.0000000000000001E-3,"± 5","(空白)",18,7.5,14,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12302JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12332JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,6,12.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12362HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,6,13,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12432HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7000000000000002E-3,"±10","(空白)",15.5,7,12.5,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12472KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5999999999999999E-3,"±10","(空白)",15.5,7.5,13,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12562KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12622JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE12682KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12682JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12822JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12103JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12103JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12123JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12133JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH12153RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH12183RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12203HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH12243RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE12273KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3000000000000002E-2,"±10","(空白)",26,6.5,16,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12333KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE12393KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",23,10.5,19.5,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12393HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12433HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",23,12,21,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12513HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",28,12.5,21.5,25,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12683JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.5,22.5,"-40 to 105 (85)",100,"PET","No","ECQE(F)[DC]","ECQE12683JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",28,14.5,23,25,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH12913HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE12124KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE12154KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,6.5,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16102JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",17.8,5.2,13,7.5,"-40 to 105 (85)",600,"PP","No","ECWH(A)","ECWHA3C102H4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C122JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",17.8,5.7,13.4,7.5,"-40 to 105 (85)",500,"PP","No","ECWH(A)","ECWHA3C132H4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C152JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,7,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16162HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.8E-3,"± 5","(空白)",17.8,6.4,14.1,7.5,"-40 to 105 (85)",500,"PP","No","ECWH(A)","ECWHA3C182J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C202HQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,6.5,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16222JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C242HB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C272JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",17.8,5.5,13.2,7.5,"-40 to 105 (85)",500,"PP","No","ECWH(A)","ECWHA3C302H4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C362JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,7,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16362HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C432JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C432HQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.1000000000000004E-3,"± 5","(空白)",17.8,6.6,9.4,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C512J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5.5999999999999999E-3,"± 5","(空白)",17.8,6.8,9.6,15,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C562J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16562JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16622JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,7.5,"-25 to 105 (85)",500,"PP","No","ECWH(V)","ECWH16622RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.399999999999999,7.5,"-40 to 105 (85)",400,"PP","No","ECWH(A)","ECWHA3C752J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.7,7.5,"-40 to 105 (85)",400,"PP","No","ECWH(A)","ECWHA3C822J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWHA3C822HC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWHA3C912HC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.01,"± 5","(空白)",20.3,6.4,12.3,17.5,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C103J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C113JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16113JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C123HB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,7.5,"-40 to 105 (85)",400,"PP","No","ECWH(A)","ECWHA3C133J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,"-40 to 105 (85)",400,"PP","No","ECWH(A)","ECWHA3C153J4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,7.5,"-25 to 105 (85)",300,"PP","No","ECWH(V)","ECWH16163RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECWHA3C163HC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,10.5,19.5,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16183HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21.6,17.5,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C203JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,17.5,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C223JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 105 (85)",1000,"PP","No","ECWH(A)","ECWHA3C243HB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.5,17.5,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16243HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,11,20,25,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16303JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,11,20,25,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16303HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.5999999999999997E-2,"± 5","(空白)",20.6,11.7,17.5,17.5,"-40 to 105 (85)",800,"PP","No","ECWH(A)","ECWHA3C363J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",20.6,11.7,17.5,17.5,"-40 to 105 (85)",800,"PP","No","ECWH(A)","ECWHA3C363H"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,17.5,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH16393HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"PP","No","ECWH(A)","ECWHA3C473JC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,800,"PP","No","ECWH(A)","ECWHA3C473HC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20102JVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,6.5,13.5,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20112HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20152HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",18,8,15,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20202HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000001E-3,"± 5","(空白)",18,8.5,15,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20222JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.5,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH20332RJV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.5,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH20332RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7000000000000002E-3,"± 5","(空白)",23,7,15.5,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20472JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,7.5,"-25 to 105 (85)",400,"PP","No","ECWH(V)","ECWH20562RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20622HVB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.4999999999999997E-3,"± 5","(空白)",23,9.5,18,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20752JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,7.5,"-25 to 105 (85)",300,"PP","No","ECWH(V)","ECWH20912RHV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2999999999999999E-2,"± 5","(空白)",23,12,21,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20133JV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 3","(空白)",23,12,21,20,"-25 to 105 (85)",100,"PP","No","ECWH(V)","ECWH20133HV"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.2,23,"-40 to 105 (85)",1000,"PP","No","ECWH(C)","ECWHC3F432JQ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.01,"± 5","(空白)",25.8,8.1999999999999993,16.100000000000001,22.5,"-40 to 105 (85)",1000,"PP","No","ECWH(C)","ECWHC3F103J"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",7.9,4.2,7.1,5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A103JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.5,4.4000000000000004,7.5,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A123KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,"PET","No","ECQE(B)[AC]","ECQE1A123JB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 85",1500,"PET","No","ECQE(T)[AC]","ECQE1A153KT6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1A153KFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2000,"PET","No","ECQE(B)[AC]","ECQE1A183KB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(F)[AC]","ECQE1A183JFZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A223KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A223JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(F)[AC]","ECQE1A223RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1700,"PET","No","ECQE(T)[AC]","ECQE1A273RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.5,5,"-40 to 85",1000,"PET","No","ECQE(F)[AC]","ECQE1A273JF6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,4.5,7.8,7.5,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A333JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1700,"PET","No","ECQE(T)[AC]","ECQE1A393RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",7.9,4.5,7.4,5,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A393JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.5,5.5,8,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A473KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A473KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.5,5,"-40 to 85",1000,"PET","No","ECQE(T)[AC]","ECQE1A563KT6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.5,5.9,8.5,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A563JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(B)[AC]","ECQE1A683KB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(F)[AC]","ECQE1A683JFZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1A683JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,"PET","No","ECQE(B)[AC]","ECQE1A823RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.5,6.5,9.8000000000000007,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A823JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10.5,6.5,11.8,7.5,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A104KF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",10.3,5.0999999999999996,7.7,5,"-40 to 85",1500,"PET","No","ECQE(B)[AC]","ECQE1A104JB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.12,"±10","(空白)",10.3,5.3,8.4,5,"-40 to 85",1500,"PET","No","ECQE(B)[AC]","ECQE1A124KB2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[AC]","ECQE1A124RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,5.9,11.5,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A124JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,6.5,12,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A154KT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13.9,5,"-40 to 85",1500,"PET","No","ECQE(B)[AC]","ECQE1A154JB6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.3,5,"-40 to 85",1500,"PET","No","ECQE(B)[AC]","ECQE1A184KB6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.5,5,"-40 to 85",500,"PET","No","ECQE(F)[AC]","ECQE1A184JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A184JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",800,"PET","No","ECQE(T)[AC]","ECQE1A224RKT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[AC]","ECQE1A224RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A274KFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1A274JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.2,5,"-40 to 85",700,"PET","No","ECQE(B)[AC]","ECQE1A334KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.2,5,"-40 to 85",700,"PET","No","ECQE(B)[AC]","ECQE1A334JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A334JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A394KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.600000000000001,5,"-40 to 85",600,"PET","No","ECQE(B)[AC]","ECQE1A394JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.47,"±10","(空白)",12.3,7,12.2,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A474KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A474KTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.3,7,12.2,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A474JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A474JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.2,5,"-40 to 85",500,"PET","No","ECQE(B)[AC]","ECQE1A474JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A474JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PET","No","ECQE(B)[AC]","ECQE1A474RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.5,7.5,15.3,15,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A474JF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(F)[AC]","ECQE1A474JFZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.3,5,"-40 to 85",500,"PET","No","ECQE(F)[AC]","ECQE1A474JF3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",400,"PET","No","ECQE(F)[AC]","ECQE1A474RJF"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(F)[AC]","ECQE1A474JFB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECQE1A474JFW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,7.5,15.3,15,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A474JT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.3,5,"-40 to 85",500,"PET","No","ECQE(T)[AC]","ECQE1A474JT3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",400,"PET","No","ECQE(T)[AC]","ECQE1A474RJT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(T)[AC]","ECQE1A474JTB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.56000000000000005,"±10","(空白)",12.3,6.7,11.9,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A564KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A564KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.899999999999999,5,"-40 to 85",600,"PET","No","ECQE(B)[AC]","ECQE1A564KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A564KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[AC]","ECQE1A564RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.3,6.7,11.9,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A564JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A564JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16.899999999999999,5,"-40 to 85",600,"PET","No","ECQE(B)[AC]","ECQE1A564JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A564JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000,"PET","No","ECQE(B)[AC]","ECQE1A564RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.68,"±10","(空白)",12.3,7.3,12.7,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A684KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A684KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.7,5,"-40 to 85",500,"PET","No","ECQE(B)[AC]","ECQE1A684KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A684KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PET","No","ECQE(B)[AC]","ECQE1A684RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"±20","(空白)",12.3,7.3,12.7,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A684MB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",12.3,7.3,12.7,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A684JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A684JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.7,5,"-40 to 85",500,"PET","No","ECQE(B)[AC]","ECQE1A684JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A684JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,900,"PET","No","ECQE(B)[AC]","ECQE1A684RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.82,"±10","(空白)",15.3,6.3,13.3,12.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A824KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A824KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.3,5,"-40 to 85",600,"PET","No","ECQE(B)[AC]","ECQE1A824KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A824KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A824RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",15.3,6.3,13.3,12.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A824JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A824JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.3,5,"-40 to 85",600,"PET","No","ECQE(B)[AC]","ECQE1A824JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A824JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A824RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"±10","(空白)",15.3,7,14,12.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A105KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A105KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,5,"-40 to 85",500,"PET","No","ECQE(B)[AC]","ECQE1A105KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A105KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A105RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",15.3,7,14,12.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A105JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A105JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,5,"-40 to 85",500,"PET","No","ECQE(B)[AC]","ECQE1A105JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A105JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A105RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.2,"±10","(空白)",20.8,7.1,14.1,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A125KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A125KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.100000000000001,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A125RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A125KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A125KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",20.8,7.1,14.1,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A125JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A125JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19.100000000000001,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A125RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A125JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A125JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.5,"±10","(空白)",20.8,8,15.1,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A155KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A155KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.100000000000001,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A155RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A155KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A155KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",20.8,8,15.1,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A155JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A155JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.100000000000001,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A155RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A155JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,"PET","No","ECQE(B)[AC]","ECQE1A155JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.8,"±10","(空白)",20.8,8.6999999999999993,15.9,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A185KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A185KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.9,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A185RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A185KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A185KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",20.8,8.6999999999999993,15.9,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A185JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A185JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20.9,7.5,"-40 to 85",400,"PET","No","ECQE(B)[AC]","ECQE1A185RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A185JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A185JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.2000000000000002,"±10","(空白)",20.8,9.6999999999999993,17.100000000000001,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A225KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A225KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.1,7.5,"-40 to 85",300,"PET","No","ECQE(B)[AC]","ECQE1A225RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A225KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A225KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",20.8,9.6999999999999993,17.100000000000001,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A225JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A225JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22.1,7.5,"-40 to 85",300,"PET","No","ECQE(B)[AC]","ECQE1A225RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A225JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,"PET","No","ECQE(B)[AC]","ECQE1A225JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.7,"±10","(空白)",20.8,10.9,23.2,7.5,"-40 to 85",300,"PET","No","ECQE(B)[AC]","ECQE1A275RKB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A275KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PET","No","ECQE(B)[AC]","ECQE1A275KB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.2,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A275KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A275KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",20.8,10.9,23.2,7.5,"-40 to 85",300,"PET","No","ECQE(B)[AC]","ECQE1A275RJB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A275JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"PET","No","ECQE(B)[AC]","ECQE1A275JB3"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18.2,17.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A275JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A275JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.3,"±10","(空白)",25.8,9.6,18.7,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A335KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A335KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.7,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A335KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",25.8,9.6,18.7,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A335JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A335JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23.7,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A335JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.9,"±10","(空白)",25.8,10.6,19.7,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A395KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A395KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.7,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A395KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",25.8,10.6,19.7,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A395JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A395JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24.7,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A395JBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.7,"±10","(空白)",25.8,11.8,20.8,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A475KB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A475KBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25.8,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A475KBB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"± 5","(空白)",25.8,11.8,20.8,22.5,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A475JB"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-40 to 105 (85)",100,"PET","No","ECQE(B)[AC]","ECQE1A475JBZ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25.8,15,"-40 to 85",100,"PET","No","ECQE(B)[AC]","ECQE1A475JBB"]

{"sheet":"PN->Parameter","index":2,"n_rows":137,"n_cols":23,"rows_kept":137,"cut":false,"hidden":false,"merged":[]}
["Panasonic Film Capacitor Quick Search"]
[]
[]
[]
[]
[null,"e1","e2","e3","#","Part Number","Voltage Cap.","Cap Tolerance","Size (mm)","Mounting","Temp. Range","Product","Series","Automotive Grade","V","Vtype","uF","Tol.","L (mm)","W (mm)","H (mm)","URL"]
[null,null,null,null,{"$f":"\nIF(F7<>\"\",COUNTIF($F$7:F7,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(O7,\"V \",P7,\" \",Q7,\"uF\"))","v":""},{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(\"Tol. \",R7,\"%\"))","v":""},{"$f":"\nIF(F7=\"\",\"\",CONCATENATE(\"L\"&S7,\"x W\",T7,\" x H\",U7))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F7,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F7=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F7,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F8<>\"\",COUNTIF($F$7:F8,\"*\")&\".\",\"\")","v":""},null,"","",{"$f":"\nIF(F8=\"\",\"\",CONCATENATE(\"L\"&S8,\"x W\",T8,\" x H\",U8))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F8,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F8=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F8,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F9<>\"\",COUNTIF($F$7:F9,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F9,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F9=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F9,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F10<>\"\",COUNTIF($F$7:F10,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F10,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F10=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F10,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F11<>\"\",COUNTIF($F$7:F11,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F11,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F11=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F11,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F12<>\"\",COUNTIF($F$7:F12,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F12,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F12=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F12,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F13<>\"\",COUNTIF($F$7:F13,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F13,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F13=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F13,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F14<>\"\",COUNTIF($F$7:F14,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F14,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F14=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F14,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F15<>\"\",COUNTIF($F$7:F15,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F15,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F15=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F15,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F16<>\"\",COUNTIF($F$7:F16,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F16,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F16=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F16,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F17<>\"\",COUNTIF($F$7:F17,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F17,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F17=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F17,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F18<>\"\",COUNTIF($F$7:F18,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F18,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F18=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F18,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F19<>\"\",COUNTIF($F$7:F19,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F19,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F19=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F19,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F20<>\"\",COUNTIF($F$7:F20,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F20,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F20=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F20,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F21<>\"\",COUNTIF($F$7:F21,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F21,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F21=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F21,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F22<>\"\",COUNTIF($F$7:F22,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F22,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F22=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F22,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F23<>\"\",COUNTIF($F$7:F23,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F23,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F23=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F23,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F24<>\"\",COUNTIF($F$7:F24,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F24,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F24=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F24,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F25<>\"\",COUNTIF($F$7:F25,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F25,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F25=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F25,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F26<>\"\",COUNTIF($F$7:F26,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F26,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F26=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F26,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F27<>\"\",COUNTIF($F$7:F27,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F27,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F27=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F27,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F28<>\"\",COUNTIF($F$7:F28,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F28,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F28=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F28,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F29<>\"\",COUNTIF($F$7:F29,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F29,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F29=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F29,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F30<>\"\",COUNTIF($F$7:F30,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F30,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F30=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F30,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F31<>\"\",COUNTIF($F$7:F31,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F31,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F31=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F31,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F32<>\"\",COUNTIF($F$7:F32,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F32,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F32=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F32,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F33<>\"\",COUNTIF($F$7:F33,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F33,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F33=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F33,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F34<>\"\",COUNTIF($F$7:F34,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F34,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F34=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F34,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F35<>\"\",COUNTIF($F$7:F35,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F35,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F35=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F35,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F36<>\"\",COUNTIF($F$7:F36,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F36,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F36=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F36,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F37<>\"\",COUNTIF($F$7:F37,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F37,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F37=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F37,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F38<>\"\",COUNTIF($F$7:F38,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F38,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F38=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F38,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F39<>\"\",COUNTIF($F$7:F39,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F39,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F39=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F39,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F40<>\"\",COUNTIF($F$7:F40,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F40,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F40=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F40,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F41<>\"\",COUNTIF($F$7:F41,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F41,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F41=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F41,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F42<>\"\",COUNTIF($F$7:F42,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F42,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F42=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F42,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F43<>\"\",COUNTIF($F$7:F43,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F43,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F43=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F43,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F44<>\"\",COUNTIF($F$7:F44,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F44,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F44=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F44,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F45<>\"\",COUNTIF($F$7:F45,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F45,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F45=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F45,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F46<>\"\",COUNTIF($F$7:F46,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F46,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F46=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F46,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F47<>\"\",COUNTIF($F$7:F47,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F47,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F47=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F47,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F48<>\"\",COUNTIF($F$7:F48,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F48,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F48=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F48,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F49<>\"\",COUNTIF($F$7:F49,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F49,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F49=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F49,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F50<>\"\",COUNTIF($F$7:F50,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F50,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F50=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F50,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F51<>\"\",COUNTIF($F$7:F51,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F51,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F51=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F51,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F52<>\"\",COUNTIF($F$7:F52,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F52,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F52=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F52,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F53<>\"\",COUNTIF($F$7:F53,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F53,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F53=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F53,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F54<>\"\",COUNTIF($F$7:F54,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F54,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F54=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F54,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F55<>\"\",COUNTIF($F$7:F55,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F55,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F55=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F55,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F56<>\"\",COUNTIF($F$7:F56,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F56,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F56=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F56,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F57<>\"\",COUNTIF($F$7:F57,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F57,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F57=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F57,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F58<>\"\",COUNTIF($F$7:F58,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F58,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F58=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F58,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F59<>\"\",COUNTIF($F$7:F59,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F59,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F59=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F59,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F60<>\"\",COUNTIF($F$7:F60,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F60,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F60=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F60,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F61<>\"\",COUNTIF($F$7:F61,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F61,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F61=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F61,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F62<>\"\",COUNTIF($F$7:F62,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F62,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F62=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F62,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F63<>\"\",COUNTIF($F$7:F63,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F63,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F63=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F63,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F64<>\"\",COUNTIF($F$7:F64,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F64,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F64=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F64,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F65<>\"\",COUNTIF($F$7:F65,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F65,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F65=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F65,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F66<>\"\",COUNTIF($F$7:F66,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F66,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F66=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F66,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F67<>\"\",COUNTIF($F$7:F67,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F67,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F67=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F67,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F68<>\"\",COUNTIF($F$7:F68,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F68,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F68=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F68,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F69<>\"\",COUNTIF($F$7:F69,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F69,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F69=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F69,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F70<>\"\",COUNTIF($F$7:F70,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F70,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F70=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F70,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F71<>\"\",COUNTIF($F$7:F71,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F71=\"\",\"\",CONCATENATE(O71,\"V \",P71,\" \",Q71,\"uF\"))","v":""},{"$f":"\nIF(F71=\"\",\"\",CONCATENATE(\"Tol. \",R71,\"%\"))","v":""},"",{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F71,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F71=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F71,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F72<>\"\",COUNTIF($F$7:F72,\"*\")&\".\",\"\")","v":""},null,"","",{"$f":"\nIF(F72=\"\",\"\",CONCATENATE(\"L\"&S72,\"x W\",T72,\" x H\",U72))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F72,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F72=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F72,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F73<>\"\",COUNTIF($F$7:F73,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F73,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F73=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F73,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F74<>\"\",COUNTIF($F$7:F74,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F74,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F74=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F74,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F75<>\"\",COUNTIF($F$7:F75,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F75,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F75=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F75,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F76<>\"\",COUNTIF($F$7:F76,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F76,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F76=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F76,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F77<>\"\",COUNTIF($F$7:F77,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F77,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F77=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F77,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F78<>\"\",COUNTIF($F$7:F78,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F78,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F78=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F78,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F79<>\"\",COUNTIF($F$7:F79,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F79,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F79=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F79,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F80<>\"\",COUNTIF($F$7:F80,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F80,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F80=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F80,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F81<>\"\",COUNTIF($F$7:F81,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F81,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F81=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F81,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F82<>\"\",COUNTIF($F$7:F82,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F82,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F82=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F82,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F83<>\"\",COUNTIF($F$7:F83,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F83,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F83=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F83,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F84<>\"\",COUNTIF($F$7:F84,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F84,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F84=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F84,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F85<>\"\",COUNTIF($F$7:F85,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F85,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F85=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F85,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F86<>\"\",COUNTIF($F$7:F86,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F86,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F86=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F86,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F87<>\"\",COUNTIF($F$7:F87,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F87,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F87=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F87,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F88<>\"\",COUNTIF($F$7:F88,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F88,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F88=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F88,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F89<>\"\",COUNTIF($F$7:F89,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F89,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F89=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F89,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F90<>\"\",COUNTIF($F$7:F90,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F90,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F90=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F90,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F91<>\"\",COUNTIF($F$7:F91,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F91,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F91=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F91,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F92<>\"\",COUNTIF($F$7:F92,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F92,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F92=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F92,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F93<>\"\",COUNTIF($F$7:F93,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F93,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F93=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F93,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F94<>\"\",COUNTIF($F$7:F94,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F94,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F94=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F94,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F95<>\"\",COUNTIF($F$7:F95,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F95,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F95=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F95,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F96<>\"\",COUNTIF($F$7:F96,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F96,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F96=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F96,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F97<>\"\",COUNTIF($F$7:F97,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F97,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F97=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F97,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F98<>\"\",COUNTIF($F$7:F98,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F98,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F98=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F98,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F99<>\"\",COUNTIF($F$7:F99,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F99,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F99=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F99,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F100<>\"\",COUNTIF($F$7:F100,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F100,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F100=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F100,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F101<>\"\",COUNTIF($F$7:F101,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F101,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F101=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F101,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F102<>\"\",COUNTIF($F$7:F102,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F102,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F102=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F102,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F103<>\"\",COUNTIF($F$7:F103,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F103,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F103=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F103,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F104<>\"\",COUNTIF($F$7:F104,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F104,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F104=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F104,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F105<>\"\",COUNTIF($F$7:F105,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F105,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F105=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F105,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F106<>\"\",COUNTIF($F$7:F137,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F106,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F106=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F106,'Film Data'!G:G,0))))","v":""},{"$f":"IFERROR(HYPERLINK(INDEX(#REF!,MATCH(PPN[[#This Row],[Part Number]],#REF!,0)),\">More Info\"),\"\")","v":""}]
[null,null,null,null,{"$f":"\nIF(F107<>\"\",COUNTIF($F$7:F137,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F107=\"\",\"\",CONCATENATE(O107,\"V \",P107,\" \",Q107,\"uF\"))","v":""},{"$f":"\nIF(F107=\"\",\"\",CONCATENATE(\"Tol. \",R107,\"%\"))","v":""},{"$f":"\nIF(F107=\"\",\"\",CONCATENATE(\"L\"&S107,\"x W\",T107,\" x H\",U107))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F107,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F107=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F107,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F108<>\"\",COUNTIF($F$7:F137,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F108=\"\",\"\",CONCATENATE(O108,\"V \",P108,\" \",Q108,\"uF\"))","v":""},{"$f":"\nIF(F108=\"\",\"\",CONCATENATE(\"Tol. \",R108,\"%\"))","v":""},{"$f":"\nIF(F108=\"\",\"\",CONCATENATE(\"L\"&S108,\"x W\",T108,\" x H\",U108))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F108,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F108=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F108,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F109<>\"\",COUNTIF($F$7:F109,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F109=\"\",\"\",CONCATENATE(O109,\"V \",P109,\" \",Q109,\"uF\"))","v":""},{"$f":"\nIF(F109=\"\",\"\",CONCATENATE(\"Tol. \",R109,\"%\"))","v":""},{"$f":"\nIF(F109=\"\",\"\",CONCATENATE(\"L\"&S109,\"x W\",T109,\" x H\",U109))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F109,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F109=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F109,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F110<>\"\",COUNTIF($F$7:F110,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F110,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F110=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F110,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F111<>\"\",COUNTIF($F$7:F111,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F111,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F111=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F111,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F112<>\"\",COUNTIF($F$7:F112,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F112,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F112=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F112,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F113<>\"\",COUNTIF($F$7:F113,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F113,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F113=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F113,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F114<>\"\",COUNTIF($F$7:F114,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F114,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F114=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F114,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F115<>\"\",COUNTIF($F$7:F115,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F115,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F115=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F115,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F116<>\"\",COUNTIF($F$7:F116,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F116,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F116=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F116,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F117<>\"\",COUNTIF($F$7:F117,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F117,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F117=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F117,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F118<>\"\",COUNTIF($F$7:F118,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F118,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F118=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F118,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F119<>\"\",COUNTIF($F$7:F119,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F119,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F119=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F119,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F120<>\"\",COUNTIF($F$7:F120,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F120,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F120=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F120,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F121<>\"\",COUNTIF($F$7:F121,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F121,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F121=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F121,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F122<>\"\",COUNTIF($F$7:F122,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F122,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F122=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F122,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F123<>\"\",COUNTIF($F$7:F123,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F123,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F123=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F123,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F124<>\"\",COUNTIF($F$7:F124,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F124,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F124=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F124,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F125<>\"\",COUNTIF($F$7:F125,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F125,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F125=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F125,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F126<>\"\",COUNTIF($F$7:F126,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F126,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F126=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F126,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F127<>\"\",COUNTIF($F$7:F127,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F127,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F127=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F127,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F128<>\"\",COUNTIF($F$7:F128,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F128,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F128=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F128,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F129<>\"\",COUNTIF($F$7:F129,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F129,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F129=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F129,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F130<>\"\",COUNTIF($F$7:F130,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F130,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F130=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F130,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F131<>\"\",COUNTIF($F$7:F131,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F131,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F131=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F131,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F132<>\"\",COUNTIF($F$7:F132,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F132,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F132=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F132,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F133<>\"\",COUNTIF($F$7:F133,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F133,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F133=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F133,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F134<>\"\",COUNTIF($F$7:F134,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F134,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F134=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F134,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F135<>\"\",COUNTIF($F$7:F135,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F135,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F135=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F135,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F136<>\"\",COUNTIF($F$7:F137,\"*\")&\".\",\"\")","v":""},null,"","","",{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F136,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F136=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F136,'Film Data'!G:G,0))))","v":""}]
[null,null,null,null,{"$f":"\nIF(F137<>\"\",COUNTIF($F$7:F137,\"*\")&\".\",\"\")","v":""},null,{"$f":"\nIF(F137=\"\",\"\",CONCATENATE(O137,\"V \",P137,\" \",Q137,\"uF\"))","v":""},{"$f":"\nIF(F137=\"\",\"\",CONCATENATE(\"Tol. \",R137,\"%\"))","v":""},{"$f":"\nIF(F137=\"\",\"\",CONCATENATE(\"L\"&S137,\"x W\",T137,\" x H\",U137))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!Q:Q,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!D:D,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!F:F,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!E:E,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!H:H,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!I:I,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!J:J,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!K:K,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!L:L,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!M:M,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",INDEX('Film Data'!N:N,MATCH($F137,'Film Data'!G:G,0)))","v":""},{"$f":"\nIF($F137=\"\",\"\",HYPERLINK(INDEX('Film Data'!T:T,MATCH($F137,'Film Data'!G:G,0))))","v":""}]

{"sheet":"Film Data","index":3,"n_rows":7139,"n_cols":31,"rows_kept":2250,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":1000,"rows_last":250,"rows_between":1000,"halvings":1}}
[null,"Film Capacitors"]
[]
[]
[]
[]
[]
[null,null,null,null,null,"Note: EZPV is automotive grade except ***TA / TB / TC."]
[null,null,null,null,null,"↓"]
[null,"↓成型後データ(PBI出力)貼り付け",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMD, Crimped, Straight","yes, no"]
["Check","Status","Type","Dielectric Material","Automotive grade","Series","PartNumber","Rated \nVoltage (V)","Voltage type","Capacitance\n(uF)","Tolerance on capacitance\n(%)","Body length / dia\n(mm)","Body width\n(mm)","Max\nHeight\n(mm)","Lead Space P1\n(mm)","Shape of lead wire","Category Temperature Range \n(°C)","Packaging Type","MOQ\n(pcs)","URL","Length [Rough] (mm)","Width [Rough] (mm)","Height [Rough] (mm)","Terminal length\n(mm)","Numbers of leads","lead Ø\n(mm)","Lead Space P2\n(mm)","Terminal style","Cut version","Tangent\nof Loss \nAngle\n(at 1kHz / 20°C)","Remark"]
[null,"Std","box","PP","Yes","EZPV","EZPV80905MTU",800,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905MTU",{"$f":"IF(L11<=9.5,\"≤ \"&ROUNDUP(L11*1,0)/1,\"≤\"&ROUNDUP(L11*1,0)/1)","v":"≤31"},{"$f":"IF(M11<=9,\"≤ \"&ROUNDUP(M11*1,0)/1,\"≤\"&ROUNDUP(M11*1,0)/1)","v":"≤21"},{"$f":"IF(N11<=9.5,\"≤ \"&ROUNDUP(N11*2,0)/2,\"≤\"&ROUNDUP(N11*2,0)/2)","v":"≤41.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80905MTA",800,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905MTA",{"$f":"IF(L12<=9.5,\"≤ \"&ROUNDUP(L12*1,0)/1,\"≤\"&ROUNDUP(L12*1,0)/1)","v":"≤31"},{"$f":"IF(M12<=9,\"≤ \"&ROUNDUP(M12*1,0)/1,\"≤\"&ROUNDUP(M12*1,0)/1)","v":"≤21"},{"$f":"IF(N12<=9.5,\"≤ \"&ROUNDUP(N12*2,0)/2,\"≤\"&ROUNDUP(N12*2,0)/2)","v":"≤41.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80905LTU",800,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80905LTT",800,"DC",9,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80905LTB",800,"DC",9,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80905LTA",800,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80905LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80805LTT",800,"DC",8,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80805LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80805LTB",800,"DC",8,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80805LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80656MTS",800,"DC",65,"±10",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80656MTS","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80656MTC",800,"DC",65,"±10",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80656MTC","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80606MTS",800,"DC",60,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80606MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80606MTC",800,"DC",60,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80606MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80556MTS",800,"DC",55,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80556MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80556MTC",800,"DC",55,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80556MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80506MTT",800,"DC",50,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80506MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80506MTS",800,"DC",50,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80506MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80506MTC",800,"DC",50,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80506MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80506MTB",800,"DC",50,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80506MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80456MTT",800,"DC",45,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80456MTT","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80456MTS",800,"DC",45,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80456MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80456MTC",800,"DC",45,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80456MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80456MTB",800,"DC",45,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80456MTB","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80406MTT",800,"DC",40,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80406MTT","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80406MTS",800,"DC",40,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80406MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80406MTC",800,"DC",40,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80406MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80406MTB",800,"DC",40,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80406MTB","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80356MTT",800,"DC",35,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80356MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80356MTS",800,"DC",35,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80356MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80356MTC",800,"DC",35,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80356MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80356MTB",800,"DC",35,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80356MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80306MTT",800,"DC",30,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80306MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80306MTS",800,"DC",30,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80306MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80306MTC",800,"DC",30,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80306MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80306MTB",800,"DC",30,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80306MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80256MTT",800,"DC",25,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80256MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80256MTS",800,"DC",25,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80256MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80256MTC",800,"DC",25,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80256MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80256MTB",800,"DC",25,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80256MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80206MTT",800,"DC",20,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80206MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80206MTB",800,"DC",20,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80206MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80186MTU",800,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80186MTU","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80186MTA",800,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80186MTA","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80186LTU",800,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80186LTU","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80186LTA",800,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80186LTA","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80156MTT",800,"DC",15,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80156MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80156MTB",800,"DC",15,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80156MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80146MTU",800,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80146MTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80146MTA",800,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80146MTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80146LTU",800,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80146LTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80146LTA",800,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80146LTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80136MTU",800,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80136MTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80136MTA",800,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80136MTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80136LTU",800,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80136LTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80136LTA",800,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80136LTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80126MTU",800,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80126MTA",800,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80126LTU",800,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80126LTT",800,"DC",12,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126LTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80126LTB",800,"DC",12,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126LTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80126LTA",800,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80126LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80116MTU",800,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80116MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80116MTA",800,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80116MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80116LTU",800,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80116LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80116LTA",800,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80116LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80106MTU",800,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80106MTA",800,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106MTA",{"$f":"IF(L76<=9.5,\"≤ \"&ROUNDUP(L76*1,0)/1,\"≤\"&ROUNDUP(L76*1,0)/1)","v":"≤31"},{"$f":"IF(M76<=9,\"≤ \"&ROUNDUP(M76*1,0)/1,\"≤\"&ROUNDUP(M76*1,0)/1)","v":"≤21"},{"$f":"IF(N76<=9.5,\"≤ \"&ROUNDUP(N76*2,0)/2,\"≤\"&ROUNDUP(N76*2,0)/2)","v":"≤41.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80106LTU",800,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV80106LTT",800,"DC",10,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80106LTB",800,"DC",10,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV80106LTA",800,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV80106LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70905MTU",700,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70905MTA",700,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70905LTU",700,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70905LTT",700,"DC",9,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70905LTB",700,"DC",9,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70905LTA",700,"DC",9,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70905LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70805LTT",700,"DC",8,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70805LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70805LTB",700,"DC",8,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70805LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70656MTS",700,"DC",65,"±10",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70656MTS","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70656MTC",700,"DC",65,"±10",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70656MTC","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70606MTS",700,"DC",60,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70606MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70606MTC",700,"DC",60,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70606MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70556MTS",700,"DC",55,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70556MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70556MTC",700,"DC",55,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70556MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70506MTT",700,"DC",50,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70506MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70506MTS",700,"DC",50,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70506MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70506MTC",700,"DC",50,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70506MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70506MTB",700,"DC",50,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70506MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70456MTT",700,"DC",45,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70456MTT","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70456MTS",700,"DC",45,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70456MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70456MTC",700,"DC",45,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70456MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70456MTB",700,"DC",45,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70456MTB","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70406MTT",700,"DC",40,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70406MTT","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70406MTS",700,"DC",40,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70406MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70406MTC",700,"DC",40,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70406MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70406MTB",700,"DC",40,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70406MTB","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70356MTT",700,"DC",35,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70356MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70356MTS",700,"DC",35,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70356MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70356MTC",700,"DC",35,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70356MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70356MTB",700,"DC",35,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70356MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70306MTT",700,"DC",30,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70306MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70306MTS",700,"DC",30,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70306MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70306MTC",700,"DC",30,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70306MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70306MTB",700,"DC",30,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70306MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70256MTT",700,"DC",25,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70256MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70256MTS",700,"DC",25,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70256MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70256MTC",700,"DC",25,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70256MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70256MTB",700,"DC",25,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70256MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70206MTT",700,"DC",20,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70206MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70206MTB",700,"DC",20,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70206MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70186MTU",700,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70186MTU","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70186MTA",700,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70186MTA","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70186LTU",700,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70186LTU","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70186LTA",700,"DC",18,"±10",31,22,53.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70186LTA","≤31","≤22","≤53.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70156MTT",700,"DC",15,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70156MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70156MTB",700,"DC",15,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70156MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70146MTU",700,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70146MTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70146MTA",700,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70146MTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70146LTU",700,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70146LTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70146LTA",700,"DC",14,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70146LTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70136MTU",700,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70136MTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70136MTA",700,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70136MTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70136LTU",700,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70136LTU","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70136LTA",700,"DC",13,"±10",31,26,41,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70136LTA","≤31","≤26","≤41",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70126MTU",700,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70126MTA",700,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70126LTU",700,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70126LTT",700,"DC",12,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126LTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70126LTB",700,"DC",12,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126LTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70126LTA",700,"DC",12,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70126LTA",{"$f":"IF(L140<=9.5,\"≤ \"&ROUNDUP(L140*1,0)/1,\"≤\"&ROUNDUP(L140*1,0)/1)","v":"≤31"},{"$f":"IF(M140<=9,\"≤ \"&ROUNDUP(M140*1,0)/1,\"≤\"&ROUNDUP(M140*1,0)/1)","v":"≤21"},{"$f":"IF(N140<=9.5,\"≤ \"&ROUNDUP(N140*2,0)/2,\"≤\"&ROUNDUP(N140*2,0)/2)","v":"≤41.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70116MTU",700,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70116MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70116MTA",700,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70116MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70116LTU",700,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70116LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70116LTA",700,"DC",11,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70116LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70106MTU",700,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106MTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70106MTA",700,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106MTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70106LTU",700,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106LTU","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV70106LTT",700,"DC",10,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70106LTB",700,"DC",10,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV70106LTA",700,"DC",10,"±10",31,20.5,41.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV70106LTA","≤31","≤21","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60956MTS",600,"DC",95,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60956MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60956MTC",600,"DC",95,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60956MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60906MTS",600,"DC",90,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60906MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60906MTC",600,"DC",90,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60906MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60856MTT",600,"DC",85,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60856MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60856MTS",600,"DC",85,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60856MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60856MTC",600,"DC",85,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60856MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60856MTB",600,"DC",85,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60856MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60806MTT",600,"DC",80,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60806MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60806MTS",600,"DC",80,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60806MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60806MTC",600,"DC",80,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60806MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60806MTB",600,"DC",80,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60806MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60756MTT",600,"DC",75,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60756MTT","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60756MTS",600,"DC",75,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60756MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60756MTC",600,"DC",75,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60756MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60756MTB",600,"DC",75,"±10",42,38,57,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60756MTB","≤42","≤38","≤57",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60706MTT",600,"DC",70,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60706MTT","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60706MTS",600,"DC",70,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60706MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60706MTC",600,"DC",70,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60706MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60706MTB",600,"DC",70,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60706MTB","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60656MTT",600,"DC",65,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60656MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60656MTS",600,"DC",65,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60656MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60656MTC",600,"DC",65,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60656MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60656MTB",600,"DC",65,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60656MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60606MTT",600,"DC",60,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60606MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60606MTS",600,"DC",60,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60606MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60606MTC",600,"DC",60,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60606MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60606MTB",600,"DC",60,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60606MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60556MTT",600,"DC",55,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60556MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60556MTS",600,"DC",55,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60556MTS","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60556MTC",600,"DC",55,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60556MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60556MTB",600,"DC",55,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60556MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60506MTT",600,"DC",50,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60506MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60506MTS",600,"DC",50,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60506MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60506MTC",600,"DC",50,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60506MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60506MTB",600,"DC",50,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60506MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60456MTT",600,"DC",45,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60456MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60456MTS",600,"DC",45,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60456MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60456MTC",600,"DC",45,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60456MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60456MTB",600,"DC",45,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60456MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60406MTT",600,"DC",40,"±10",41.5,27.5,42,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60406MTT","≤42","≤28","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60406MTS",600,"DC",40,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60406MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60406MTC",600,"DC",40,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60406MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60406MTB",600,"DC",40,"±10",41.5,27.5,42,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60406MTB","≤42","≤28","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60356MTT",600,"DC",35,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60356MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60356MTB",600,"DC",35,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60356MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60306MTT",600,"DC",30,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60306MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60306MTB",600,"DC",30,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60306MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60256MTT",600,"DC",25,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60256MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60256MTB",600,"DC",25,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60256MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60226MTT",600,"DC",22,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60226MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60226MTB",600,"DC",22,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60226MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60206MTT",600,"DC",20,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60206MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60206MTB",600,"DC",20,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60206MTB",{"$f":"IF(L204<=9.5,\"≤ \"&ROUNDUP(L204*1,0)/1,\"≤\"&ROUNDUP(L204*1,0)/1)","v":"≤41"},{"$f":"IF(M204<=9,\"≤ \"&ROUNDUP(M204*1,0)/1,\"≤\"&ROUNDUP(M204*1,0)/1)","v":"≤22"},{"$f":"IF(N204<=9.5,\"≤ \"&ROUNDUP(N204*2,0)/2,\"≤\"&ROUNDUP(N204*2,0)/2)","v":"≤36"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60156LTT",600,"DC",15,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60156LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60156LTB",600,"DC",15,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60156LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60126LTT",600,"DC",12,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60126LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60126LTB",600,"DC",12,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60126LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60117MTS",600,"DC",110,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60117MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60117MTC",600,"DC",110,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60117MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60107MTS",600,"DC",100,"±10",57,40,51.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60107MTS","≤57","≤40","≤51.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60107MTC",600,"DC",100,"±10",57,40,51.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60107MTC","≤57","≤40","≤51.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV60106LTT",600,"DC",10,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60106LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV60106LTB",600,"DC",10,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV60106LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B905MTT",1100,"DC",9,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B905MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B905MTB",1100,"DC",9,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B905MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B805MTT",1100,"DC",8,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B805MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B805MTB",1100,"DC",8,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B805MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B705MTT",1100,"DC",7,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B705MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B705MTB",1100,"DC",7,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B705MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B605LTT",1100,"DC",6,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B605LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B605LTB",1100,"DC",6,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B605LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B505LTT",1100,"DC",5,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B505LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B505LTB",1100,"DC",5,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B505LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B475LTT",1100,"DC",4.7,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B475LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B475LTB",1100,"DC",4.7,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B475LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B406MTS",1100,"DC",40,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B406MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B406MTC",1100,"DC",40,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B406MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B405LTT",1100,"DC",4,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B405LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B405LTB",1100,"DC",4,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B405LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B356MTS",1100,"DC",35,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B356MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B356MTC",1100,"DC",35,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B356MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B306MTT",1100,"DC",30,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B306MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B306MTS",1100,"DC",30,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B306MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B306MTC",1100,"DC",30,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B306MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B306MTB",1100,"DC",30,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B306MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B305LTT",1100,"DC",3,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B305LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B305LTB",1100,"DC",3,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B305LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B256MTT",1100,"DC",25,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B256MTT","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B256MTS",1100,"DC",25,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B256MTS","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B256MTC",1100,"DC",25,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B256MTC","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B256MTB",1100,"DC",25,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B256MTB","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B206MTT",1100,"DC",20,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B206MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B206MTS",1100,"DC",20,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B206MTS","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B206MTC",1100,"DC",20,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B206MTC","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B206MTB",1100,"DC",20,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B206MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B186MTT",1100,"DC",18,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B186MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B186MTB",1100,"DC",18,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B186MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B156MTT",1100,"DC",15,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B156MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B156MTS",1100,"DC",15,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B156MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B156MTC",1100,"DC",15,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B156MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B156MTB",1100,"DC",15,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B156MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B126MTT",1100,"DC",12,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B126MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B126MTB",1100,"DC",12,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B126MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1B106MTT",1100,"DC",10,"±10",41.5,23.5,43.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B106MTT","≤42","≤24","≤43.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1B106MTB",1100,"DC",10,"±10",41.5,23.5,43.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1B106MTB","≤42","≤24","≤43.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A905MTT",1000,"DC",9,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A905MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A905MTB",1000,"DC",9,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A905MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A805MTT",1000,"DC",8,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A805MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A805MTB",1000,"DC",8,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A805MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A705MTT",1000,"DC",7,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A705MTT","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A705MTB",1000,"DC",7,"±10",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A705MTB","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A605LTT",1000,"DC",6,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A605LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A605LTB",1000,"DC",6,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A605LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A505LTT",1000,"DC",5,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A505LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A505LTB",1000,"DC",5,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A505LTB","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A475LTT",1000,"DC",4.7,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A475LTT","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A475LTB",1000,"DC",4.7,"±10",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A475LTB",{"$f":"IF(L268<=9.5,\"≤ \"&ROUNDUP(L268*1,0)/1,\"≤\"&ROUNDUP(L268*1,0)/1)","v":"≤41"},{"$f":"IF(M268<=9,\"≤ \"&ROUNDUP(M268*1,0)/1,\"≤\"&ROUNDUP(M268*1,0)/1)","v":"≤17"},{"$f":"IF(N268<=9.5,\"≤ \"&ROUNDUP(N268*2,0)/2,\"≤\"&ROUNDUP(N268*2,0)/2)","v":"≤34.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A406MTS",1000,"DC",40,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A406MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A406MTC",1000,"DC",40,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A406MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A405LTT",1000,"DC",4,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A405LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A405LTB",1000,"DC",4,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A405LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A356MTS",1000,"DC",35,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A356MTS","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A356MTC",1000,"DC",35,"±10",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A356MTC","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A306MTT",1000,"DC",30,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A306MTT","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A306MTS",1000,"DC",30,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A306MTS","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A306MTC",1000,"DC",30,"±10",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A306MTC","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A306MTB",1000,"DC",30,"±10",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A306MTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A305LTT",1000,"DC",3,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A305LTT","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A305LTB",1000,"DC",3,"±10",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A305LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A256MTT",1000,"DC",25,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A256MTT","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A256MTS",1000,"DC",25,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A256MTS","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A256MTC",1000,"DC",25,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A256MTC","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A256MTB",1000,"DC",25,"±10",42,38,52.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A256MTB","≤42","≤38","≤52.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A206MTT",1000,"DC",20,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A206MTT","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A206MTS",1000,"DC",20,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A206MTS","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A206MTC",1000,"DC",20,"±10",57.5,35.5,45.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A206MTC","≤58","≤36","≤45.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A206MTB",1000,"DC",20,"±10",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A206MTB","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A186MTT",1000,"DC",18,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A186MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A186MTB",1000,"DC",18,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A186MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A156MTT",1000,"DC",15,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A156MTT","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A156MTS",1000,"DC",15,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A156MTS","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A156MTC",1000,"DC",15,"±10",57,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A156MTC","≤57","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A156MTB",1000,"DC",15,"±10",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A156MTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A126MTT",1000,"DC",12,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A126MTT","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A126MTB",1000,"DC",12,"±10",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A126MTB","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","EZPV","EZPV1A106MTT",1000,"DC",10,"±10",41.5,23.5,43.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A106MTT","≤42","≤24","≤43.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPV","EZPV1A106MTB",1000,"DC",10,"±10",41.5,23.5,43.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPV1A106MTB","≤42","≤24","≤43.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60705MTD",600,"AC",7,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60705MTD","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60685MTD",600,"AC",6.8,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60685MTD","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60475MTE",600,"AC",4.7,"±10",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60475MTE","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60475MTD",600,"AC",4.7,"±10",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60475MTD","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60335MTD",600,"AC",3.3,"±10",41.5,27.5,42,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60335MTD","≤42","≤28","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60225LTD",600,"AC",2.2000000000000002,"±10",41.5,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60225LTD","≤42","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60155LTD",600,"AC",1.5,"±10",41.5,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60155LTD","≤42","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60126MTD",600,"AC",12,"±10",57.5,45,62,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60126MTD","≤58","≤45","≤62",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60106MTD",600,"AC",10,"±10",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60106MTD","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ60105LTD",600,"AC",1,"±10",41.5,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ60105LTD","≤42","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38955MTA",380,"AC",9.5,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38955MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38955LTA",380,"AC",9.5,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38955LTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38905MTA",380,"AC",9,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38905MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38905LTA",380,"AC",9,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38905LTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38855MTA",380,"AC",8.5,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38855MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38855LTA",380,"AC",8.5,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38855LTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38805MTA",380,"AC",8,"± 5",41.5,27.5,42,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38805MTA","≤42","≤28","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38805LTD",380,"AC",8,"± 5",41.5,27.5,42,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38805LTD","≤42","≤28","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38805LTC",380,"AC",8,"± 5",41.5,26.5,41.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38805LTC","≤42","≤27","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38755LTA",380,"AC",7.5,"± 5",41.5,26.5,41.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38755LTA","≤42","≤27","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38705LTA",380,"AC",7,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38705LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38605LTA",380,"AC",6,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38605LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38555LTA",380,"AC",5.5,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38555LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38505LTA",380,"AC",5,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38505LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38475LTA",380,"AC",4.7,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38475LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38455LTA",380,"AC",4.5,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38455LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38405LTA",380,"AC",4,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38405LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38355LTA",380,"AC",3.5,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38355LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38336MTA",380,"AC",33,"± 5",57.5,45,62,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38336MTA","≤58","≤45","≤62",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38335LTA",380,"AC",3.3,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38335LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38306MTA",380,"AC",30,"± 5",57.5,45,62,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38306MTA","≤58","≤45","≤62",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38305LTA",380,"AC",3,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38305LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38255LTB",380,"AC",2.5,"± 5",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38255LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38246MTC",380,"AC",24,"± 5",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38246MTC",{"$f":"IF(L332<=9.5,\"≤ \"&ROUNDUP(L332*1,0)/1,\"≤\"&ROUNDUP(L332*1,0)/1)","v":"≤58"},{"$f":"IF(M332<=9,\"≤ \"&ROUNDUP(M332*1,0)/1,\"≤\"&ROUNDUP(M332*1,0)/1)","v":"≤35"},{"$f":"IF(N332<=9.5,\"≤ \"&ROUNDUP(N332*2,0)/2,\"≤\"&ROUNDUP(N332*2,0)/2)","v":"≤64.5"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38226MTA",380,"AC",22,"± 5",57.5,35,56,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38226MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38225LTB",380,"AC",2.2000000000000002,"± 5",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38225LTB","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38206MTA",380,"AC",20,"± 5",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38206MTA","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38205LTA",380,"AC",2,"± 5",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38205LTA","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38186MTA",380,"AC",18,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38186MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38166MTA",380,"AC",16,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38166MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38156MTC",380,"AC",15,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38156MTC","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38156MTB",380,"AC",15,"± 5",42,38,57.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38156MTB","≤42","≤38","≤57.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38156LTB",380,"AC",15,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38156LTB","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38156LTA",380,"AC",15,"± 5",42,38,57.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38156LTA","≤42","≤38","≤57.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38155LTA",380,"AC",1.5,"± 5",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38155LTA","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38126MTA",380,"AC",12,"± 5",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38126MTA","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38126LTB",380,"AC",12,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38126LTB","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38126LTA",380,"AC",12,"± 5",41.5,30,56,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38126LTA","≤42","≤30","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38116LTA",380,"AC",11,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38116LTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38106MTA",380,"AC",10,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38106MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38106LTB",380,"AC",10,"± 5",57.5,25,40,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38106LTB","≤58","≤25","≤40",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38106LTA",380,"AC",10,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38106LTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ38105LTA",380,"AC",1,"± 5",41,15,29,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ38105LTA","≤41","≤15","≤29",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33905LTA",330,"AC",9,"± 5",41.5,26.5,41.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33905LTA","≤42","≤27","≤41.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33805LTA",330,"AC",8,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33805LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33705LTA",330,"AC",7,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33705LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33685LTA",330,"AC",6.8,"± 5",41,26,40.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33685LTA","≤41","≤26","≤40.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33605LTA",330,"AC",6,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33605LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33505LTA",330,"AC",5,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33505LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33475LTA",330,"AC",4.7,"± 5",41,22,36,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33475LTA","≤41","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33455LTA",330,"AC",4.5,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33455LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33405LTA",330,"AC",4,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33405LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33356MTA",330,"AC",35,"± 5",57.5,45,62,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33356MTA","≤58","≤45","≤62",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33355LTA",330,"AC",3.5,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33355LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33335LTA",330,"AC",3.3,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33335LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33306MTB",330,"AC",30,"± 5",57.5,45,62,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33306MTB","≤58","≤45","≤62",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33305LTA",330,"AC",3,"± 5",41,17,34.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33305LTA","≤41","≤17","≤34.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33286MTA",330,"AC",28,"± 5",57.5,35,64.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33286MTA","≤58","≤35","≤64.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33256MTB",330,"AC",25,"± 5",57.5,40,51.5,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33256MTB","≤58","≤40","≤51.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33226MTA",330,"AC",22,"± 5",57.5,35,50,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33226MTA","≤58","≤35","≤50",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33206MTB",330,"AC",20,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33206MTB","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33206MTA",330,"AC",20,"± 5",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33206MTA","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33206LTB",330,"AC",20,"± 5",41,43,58,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33206LTB","≤41","≤43","≤58",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33186MTA",330,"AC",18,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33186MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33156MTA",330,"AC",15,"± 5",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33156MTA","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33156LTB",330,"AC",15,"± 5",57.5,30,51,52.5,"Short cut lead wire type","-40 to 105 (85)","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33156LTB","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33156LTA",330,"AC",15,"± 5",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33156LTA","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33146MTA",330,"AC",14,"± 5",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33146MTA","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33146LTA",330,"AC",14,"± 5",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33146LTA","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33126MTA",330,"AC",12,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33126MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33126LTA",330,"AC",12,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33126LTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33106MTA",330,"AC",10,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33106MTA","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33106LTC",330,"AC",10,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33106LTC","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33106LTB",330,"AC",10,"± 5",41,30,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33106LTB","≤41","≤30","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ33106LTA",330,"AC",10,"± 5",42.5,35.5,50.5,37.5,"Short cut lead wire type","-40 to 105 (85)","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ33106LTA","≤43","≤36","≤50.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ25366LTA",250,"AC",36,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 85","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25366LTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ25226LTA",250,"AC",22,"±10",57.5,30,45,52.5,"Short cut lead wire type","-25 to 85","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25226LTA","≤58","≤30","≤45",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPQ","EZPQ25126LTA",250,"AC",12,"±10",48.5,22,36,45.6,"Short cut lead wire type","-25 to 85","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPQ25126LTA","≤49","≤22","≤36",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80606MTA",800,"DC",60,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80606MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80556MTA",800,"DC",55,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80556MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80506MTA",800,"DC",50,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80506MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80456MTA",800,"DC",45,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80456MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80406MTA",800,"DC",40,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80406MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80356MTA",800,"DC",35,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80356MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80306MTA",800,"DC",30,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80306MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80256MTA",800,"DC",25,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80256MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80206MTA",800,"DC",20,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80206MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80156MTA",800,"DC",15,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80156MTA",{"$f":"IF(L396<=9.5,\"≤ \"&ROUNDUP(L396*1,0)/1,\"≤\"&ROUNDUP(L396*1,0)/1)","v":"≤42"},{"$f":"IF(M396<=9,\"≤ \"&ROUNDUP(M396*1,0)/1,\"≤\"&ROUNDUP(M396*1,0)/1)","v":"≤20"},{"$f":"IF(N396<=9.5,\"≤ \"&ROUNDUP(N396*2,0)/2,\"≤\"&ROUNDUP(N396*2,0)/2)","v":"≤42"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE80106LTA",800,"DC",10,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE80106LTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE [Low profile]","EZPE63106LTB",630,"DC",10,"±15",41.5,24.5,19.5,37.5,"Short cut lead wire type","-25 to 70","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE63106LTB","≤42","≤25","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE [Low profile]","EZPE57126LTB",575,"DC",12,"±15",41.5,24.5,19.5,37.5,"Short cut lead wire type","-25 to 70","Other package",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE57126LTB","≤42","≤25","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE [Low profile]","EZPE52296MTB",525,"DC",29,"±15",37,48.5,23.5,34,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE52296MTB","≤37","≤49","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50956MTA",500,"DC",95,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50956MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50906MTA",500,"DC",90,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50906MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50856MTA",500,"DC",85,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50856MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50806MTA",500,"DC",80,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50806MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50756MTA",500,"DC",75,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50756MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50706MTA",500,"DC",70,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50706MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50656MTA",500,"DC",65,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50656MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50606MTA",500,"DC",60,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50606MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50556MTA",500,"DC",55,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50556MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50506MTA",500,"DC",50,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50506MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50456MTA",500,"DC",45,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50456MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50406MTA",500,"DC",40,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50406MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50356MTA",500,"DC",35,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50356MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50306MTA",500,"DC",30,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50306MTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50256LTA",500,"DC",25,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50256LTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50206LTA",500,"DC",20,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50206LTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50156LTA",500,"DC",15,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50156LTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50117MTA",500,"DC",110,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50117MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50107MTA",500,"DC",100,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50107MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE50106LTA",500,"DC",10,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE50106LTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE [Low profile]","EZPE45666MTB",450,"DC",66,"±15",32.5,90,24,27.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE45666MTB","≤33","≤90","≤24",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1D256MTA",1300,"DC",25,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1D256MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1D206MTA",1300,"DC",20,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1D206MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1D156MTA",1300,"DC",15,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1D156MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1D106MTA",1300,"DC",10,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1D106MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B406MTA",1100,"DC",40,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B406MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B356MTA",1100,"DC",35,"±10",57.5,35,56,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B356MTA","≤58","≤35","≤56",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B306MTA",1100,"DC",30,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B306MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B256MTA",1100,"DC",25,"±10",57.5,30,51,52.5,"Short cut lead wire type","-25 to 70","Other package",50,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B256MTA","≤58","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B206MTA",1100,"DC",20,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B206MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B156MTA",1100,"DC",15,"±10",41.5,30,51,37.5,"Short cut lead wire type","-25 to 70","Other package",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B156MTA","≤42","≤30","≤51",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","EZPE","EZPE1B106MTA",1100,"DC",10,"±10",41.5,20,42,37.5,"Short cut lead wire type","-25 to 70","Other package",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/EZPE1B106MTA","≤42","≤20","≤42",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWUC2J333JV",630,"DC",3.3000000000000002E-2,"± 5",7.1,6.3,5.0999999999999996,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWUC2J333JV","≤ 8","≤ 7","≤ 5.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWUC2J273JV",630,"DC",2.7E-2,"± 5",7.1,6.3,4.0999999999999996,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWUC2J273JV","≤ 8","≤ 7","≤ 4.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWUC2J223JV",630,"DC",2.1999999999999999E-2,"± 5",7.1,6.3,3.6,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWUC2J223JV","≤ 8","≤ 7","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2823V16",250,"DC",8.2000000000000003E-2,"± 5",6,5,3.2,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2823V16","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2823KC9",250,"DC",8.2000000000000003E-2,"±10",6,5,3.2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2823KC9","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2823JC9",250,"DC",8.2000000000000003E-2,"± 5",6,5,3.2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2823JC9","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2822V16",250,"DC",8.2000000000000007E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2822V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2822KC9",250,"DC",8.2000000000000007E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2822KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2822JC9",250,"DC",8.2000000000000007E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2822JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2683V16",250,"DC",6.8000000000000005E-2,"± 5",6,4.0999999999999996,3.2,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2683V16","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2683KC9",250,"DC",6.8000000000000005E-2,"±10",6,4.0999999999999996,3.2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2683KC9","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2683JC9",250,"DC",6.8000000000000005E-2,"± 5",6,4.0999999999999996,3.2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2683JC9","≤ 6","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2682V16",250,"DC",6.7999999999999996E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2682V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2682KC9",250,"DC",6.7999999999999996E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2682KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2682JC9",250,"DC",6.7999999999999996E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2682JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2563V16",250,"DC",5.6000000000000001E-2,"± 5",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2563V16","≤ 6","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2563KC9",250,"DC",5.6000000000000001E-2,"±10",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2563KC9","≤ 6","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2563JC9",250,"DC",5.6000000000000001E-2,"± 5",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2563JC9","≤ 6","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2562V16",250,"DC",5.5999999999999999E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2562V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2562KC9",250,"DC",5.5999999999999999E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2562KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2562JC9",250,"DC",5.5999999999999999E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2562JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2473V16",250,"DC",4.7E-2,"± 5",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2473V16","≤ 6","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2473KC9",250,"DC",4.7E-2,"±10",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2473KC9","≤ 6","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2473JC9",250,"DC",4.7E-2,"± 5",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2473JC9","≤ 6","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2472V16",250,"DC",4.7000000000000002E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2472V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2472KC9",250,"DC",4.7000000000000002E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2472KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2472JC9",250,"DC",4.7000000000000002E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2472JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2393V16",250,"DC",3.9E-2,"± 5",6,4.0999999999999996,2,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2393V16",{"$f":"IF(L460<=9.5,\"≤ \"&ROUNDUP(L460*1,0)/1,\"≤\"&ROUNDUP(L460*1,0)/1)","v":"≤ 6"},{"$f":"IF(M460<=9,\"≤ \"&ROUNDUP(M460*1,0)/1,\"≤\"&ROUNDUP(M460*1,0)/1)","v":"≤ 5"},{"$f":"IF(N460<=9.5,\"≤ \"&ROUNDUP(N460*2,0)/2,\"≤\"&ROUNDUP(N460*2,0)/2)","v":"≤ 2"},null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2393KC9",250,"DC",3.9E-2,"±10",6,4.0999999999999996,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2393KC9","≤ 6","≤ 5","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2393JC9",250,"DC",3.9E-2,"± 5",6,4.0999999999999996,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2393JC9","≤ 6","≤ 5","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2392V16",250,"DC",3.8999999999999998E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2392V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2392KC9",250,"DC",3.8999999999999998E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2392KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2392JC9",250,"DC",3.8999999999999998E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2392JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2333V16",250,"DC",3.3000000000000002E-2,"± 5",4.8,3.3,2.8,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2333V16","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2333KC9",250,"DC",3.3000000000000002E-2,"±10",4.8,3.3,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2333KC9","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2333JC9",250,"DC",3.3000000000000002E-2,"± 5",4.8,3.3,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2333JC9","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2332V16",250,"DC",3.3E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2332V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2332KC9",250,"DC",3.3E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2332KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2332JC9",250,"DC",3.3E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2332JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2273V16",250,"DC",2.7E-2,"± 5",4.8,3.3,2.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2273V16","≤ 5","≤ 4","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2273KC9",250,"DC",2.7E-2,"±10",4.8,3.3,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2273KC9","≤ 5","≤ 4","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2273JC9",250,"DC",2.7E-2,"± 5",4.8,3.3,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2273JC9","≤ 5","≤ 4","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2272V16",250,"DC",2.7000000000000001E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2272V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2272KC9",250,"DC",2.7000000000000001E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2272KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2272JC9",250,"DC",2.7000000000000001E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2272JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2223V16",250,"DC",2.1999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2223V16","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2223KC9",250,"DC",2.1999999999999999E-2,"±10",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2223KC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2223JC9",250,"DC",2.1999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2223JC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2222V16",250,"DC",2.2000000000000001E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2222V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2222KC9",250,"DC",2.2000000000000001E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2222KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2222JC9",250,"DC",2.2000000000000001E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2222JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2183V16",250,"DC",1.7999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2183V16","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2183KC9",250,"DC",1.7999999999999999E-2,"±10",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2183KC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2183JC9",250,"DC",1.7999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2183JC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2182V16",250,"DC",1.8E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2182V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2182KC9",250,"DC",1.8E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2182KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2182JC9",250,"DC",1.8E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2182JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2153V16",250,"DC",1.4999999999999999E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2153V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2153KC9",250,"DC",1.4999999999999999E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2153KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2153JC9",250,"DC",1.4999999999999999E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2153JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2152V16",250,"DC",1.5E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2152V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2152KC9",250,"DC",1.5E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2152KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2152JC9",250,"DC",1.5E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2152JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2124V16",250,"DC",0.12,"± 5",6,5,4.5,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2124V16","≤ 6","≤ 5","≤ 4.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2124KC9",250,"DC",0.12,"±10",6,5,4.5,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2124KC9","≤ 6","≤ 5","≤ 4.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2124JC9",250,"DC",0.12,"± 5",6,5,4.5,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2124JC9","≤ 6","≤ 5","≤ 4.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2123V16",250,"DC",1.2E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2123V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2123KC9",250,"DC",1.2E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2123KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2123JC9",250,"DC",1.2E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2123JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2122V16",250,"DC",1.1999999999999999E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2122V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2122KC9",250,"DC",1.1999999999999999E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2122KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2122JC9",250,"DC",1.1999999999999999E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2122JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2104V16",250,"DC",0.1,"± 5",6,5,3.8,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2104V16","≤ 6","≤ 5","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2104KC9",250,"DC",0.1,"±10",6,5,3.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2104KC9","≤ 6","≤ 5","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2104JC9",250,"DC",0.1,"± 5",6,5,3.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2104JC9","≤ 6","≤ 5","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2103V16",250,"DC",0.01,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2103V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2103KC9",250,"DC",0.01,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2103KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2103JC9",250,"DC",0.01,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2103JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(V16)","ECWU2102V16",250,"DC",1E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 85","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2102V16","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2102KC9",250,"DC",1E-3,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2102KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU2102JC9",250,"DC",1E-3,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU2102JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1824KCV",100,"DC",0.82,"±10",9.8000000000000007,6.3,4.3,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1824KCV","≤10","≤ 7","≤ 4.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1823KC9",100,"DC",8.2000000000000003E-2,"±10",4.8,3.3,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1823KC9","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1823JC9",100,"DC",8.2000000000000003E-2,"± 5",4.8,3.3,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1823JC9","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1822JX5",100,"DC",8.2000000000000007E-3,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1822JX5","≤ 4","≤ 3","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1684KCV",100,"DC",0.68,"±10",9.8000000000000007,6.3,3.6,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1684KCV","≤10","≤ 7","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1683KC9",100,"DC",6.8000000000000005E-2,"±10",4.8,3.3,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1683KC9","≤ 5","≤ 4","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1683JC9",100,"DC",6.8000000000000005E-2,"± 5",4.8,3.3,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1683JC9","≤ 5","≤ 4","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1682JX5",100,"DC",6.7999999999999996E-3,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1682JX5","≤ 4","≤ 3","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1564KCV",100,"DC",0.56000000000000005,"±10",9.8000000000000007,6.3,3,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1564KCV","≤10","≤ 7","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1563KC9",100,"DC",5.6000000000000001E-2,"±10",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1563KC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1563JC9",100,"DC",5.6000000000000001E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1563JC9",{"$f":"IF(L524<=9.5,\"≤ \"&ROUNDUP(L524*1,0)/1,\"≤\"&ROUNDUP(L524*1,0)/1)","v":"≤ 5"},{"$f":"IF(M524<=9,\"≤ \"&ROUNDUP(M524*1,0)/1,\"≤\"&ROUNDUP(M524*1,0)/1)","v":"≤ 4"},{"$f":"IF(N524<=9.5,\"≤ \"&ROUNDUP(N524*2,0)/2,\"≤\"&ROUNDUP(N524*2,0)/2)","v":"≤ 2"},null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1562JX5",100,"DC",5.5999999999999999E-3,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1562JX5","≤ 4","≤ 3","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1474KCV",100,"DC",0.47,"±10",7.7,5.5,4,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1474KCV","≤ 8","≤ 6","≤ 4",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1473KC9",100,"DC",4.7E-2,"±10",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1473KC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1473JC9",100,"DC",4.7E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1473JC9","≤ 5","≤ 4","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1472JX5",100,"DC",4.7000000000000002E-3,"± 5",3.2,1.6,1.5,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1472JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1394KCV",100,"DC",0.39,"±10",7.7,5.5,3.4,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1394KCV","≤ 8","≤ 6","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1393KC9",100,"DC",3.9E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1393KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1393JC9",100,"DC",3.9E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1393JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1392JX5",100,"DC",3.8999999999999998E-3,"± 5",3.2,1.6,1.5,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1392JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1334KC9",100,"DC",0.33,"±10",7.1,5,3.5,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1334KC9","≤ 8","≤ 5","≤ 3.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1333KC9",100,"DC",3.3000000000000002E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1333KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1333JC9",100,"DC",3.3000000000000002E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1333JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1332JX5",100,"DC",3.3E-3,"± 5",3.2,1.6,1.5,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1332JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1274KC9",100,"DC",0.27,"±10",7.1,5,2.9,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1274KC9","≤ 8","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1273KC9",100,"DC",2.7E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1273KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1273JC9",100,"DC",2.7E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1273JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1272JX5",100,"DC",2.7000000000000001E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1272JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1224KC9",100,"DC",0.22,"±10",7.1,5,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1224KC9","≤ 8","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1223KC9",100,"DC",2.1999999999999999E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1223KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1223JC9",100,"DC",2.1999999999999999E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1223JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1222JX5",100,"DC",2.2000000000000001E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1222JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1184KC9",100,"DC",0.18,"±10",7.1,5,2,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1184KC9","≤ 8","≤ 5","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1183KC9",100,"DC",1.7999999999999999E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1183KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1183JC9",100,"DC",1.7999999999999999E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1183JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1182JX5",100,"DC",1.8E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1182JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1154KC9",100,"DC",0.15,"±10",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1154KC9","≤ 6","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1154JC9",100,"DC",0.15,"± 5",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1154JC9","≤ 6","≤ 5","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1153KC9",100,"DC",1.4999999999999999E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1153KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1153JC9",100,"DC",1.4999999999999999E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1153JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1152JX5",100,"DC",1.5E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1152JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1124KC9",100,"DC",0.12,"±10",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1124KC9","≤ 6","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1124JC9",100,"DC",0.12,"± 5",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1124JC9","≤ 6","≤ 5","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1123KC9",100,"DC",1.2E-2,"±10",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1123KC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1123JC9",100,"DC",1.2E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1123JC9","≤ 5","≤ 4","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1122JX5",100,"DC",1.1999999999999999E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1122JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1105KCV",100,"DC",1,"±10",9.8000000000000007,6.3,5.0999999999999996,"'-","Non lead wire","-55 to 125 (85)","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1105KCV","≤10","≤ 7","≤ 5.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1104V33",100,"DC",0.1,"± 5",4.8,3.3,2.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1104V33","≤ 5","≤ 4","≤ 3",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1104KC9",100,"DC",0.1,"±10",6,4.0999999999999996,1.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1104KC9","≤ 6","≤ 5","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(C)","ECWU1104JC9",100,"DC",0.1,"± 5",6,4.0999999999999996,1.8,"'-","Non lead wire","-55 to 125 (85)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1104JC9","≤ 6","≤ 5","≤ 2",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1103JX5",100,"DC",0.01,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1103JX5","≤ 4","≤ 3","≤ 2.5",null,null,null,null,null,null,null,""]
[null,"Std","chip","PEN","No","ECWU(X)","ECWU1102JX5",100,"DC",1E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 105","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWU1102JX5","≤ 4","≤ 2","≤ 1.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F822JQ",3000,"DC",8.2000000000000007E-3,"± 5",25.8,7.5,22.3,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F822JQ","≤26","≤ 8","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F822JD",3000,"DC",8.2000000000000007E-3,"± 5",25.8,7.5,15.3,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F822JD","≤26","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F822J",3000,"DC",8.2000000000000007E-3,"± 5",25.8,7.5,15.3,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F822J","≤26","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F562JQ",3000,"DC",5.5999999999999999E-3,"± 5",25.8,7.3,19,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F562JQ","≤26","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F562JD",3000,"DC",5.5999999999999999E-3,"± 5",25.8,7.3,12,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F562JD","≤26","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F562J",3000,"DC",5.5999999999999999E-3,"± 5",25.8,7.3,12,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F562J","≤26","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F432JQ",3000,"DC",4.3E-3,"± 5",25.8,6.5,18.2,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F432JQ","≤26","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F432JD",3000,"DC",4.3E-3,"± 5",25.8,6.5,11.2,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F432JD","≤26","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F432J",3000,"DC",4.3E-3,"± 5",25.8,6.5,11.2,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F432J","≤26","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F392JQ",3000,"DC",3.8999999999999998E-3,"± 5",25.8,7.5,19.2,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F392JQ","≤26","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F392JD",3000,"DC",3.8999999999999998E-3,"± 5",25.8,7.5,12.2,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F392JD","≤26","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F392J",3000,"DC",3.8999999999999998E-3,"± 5",25.8,7.5,12.2,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F392J","≤26","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F362JQ",3000,"DC",3.5999999999999999E-3,"± 5",25.8,7.2,18.899999999999999,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F362JQ","≤26","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F362JD",3000,"DC",3.5999999999999999E-3,"± 5",25.8,7.2,11.9,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F362JD","≤26","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F362J",3000,"DC",3.5999999999999999E-3,"± 5",25.8,7.2,11.9,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F362J","≤26","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F242JQ",3000,"DC",2.3999999999999998E-3,"± 5",25.8,6.1,17.899999999999999,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F242JQ","≤26","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F242JD",3000,"DC",2.3999999999999998E-3,"± 5",25.8,6.1,10.9,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F242JD","≤26","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F242J",3000,"DC",2.3999999999999998E-3,"± 5",25.8,6.1,10.9,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F242J","≤26","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F103JQ",3000,"DC",0.01,"± 5",25.8,8.1999999999999993,23.1,23,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F103JQ","≤26","≤ 9","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F103JD",3000,"DC",0.01,"± 5",25.8,8.1999999999999993,16.100000000000001,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F103JD","≤26","≤ 9","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3F103J",3000,"DC",0.01,"± 5",25.8,8.1999999999999993,16.100000000000001,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3F103J","≤26","≤ 9","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3B803JA",1250,"DC",0.08,"± 5",20.7,12,19,17.5,"Short cut lead wire type","-40 to 85","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3B803JA","≤21","≤12","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3B124JA",1250,"DC",0.12,"± 5",20.7,14.9,21.9,17.5,"Short cut lead wire type","-40 to 85","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3B124JA",{"$f":"IF(L588<=9.5,\"≤ \"&ROUNDUP(L588*1,0)/1,\"≤\"&ROUNDUP(L588*1,0)/1)","v":"≤21"},{"$f":"IF(M588<=9,\"≤ \"&ROUNDUP(M588*1,0)/1,\"≤\"&ROUNDUP(M588*1,0)/1)","v":"≤15"},{"$f":"IF(N588<=9.5,\"≤ \"&ROUNDUP(N588*2,0)/2,\"≤\"&ROUNDUP(N588*2,0)/2)","v":"≤22"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3B114JA",1250,"DC",0.11,"± 5",20.7,14.2,21.3,17.5,"Short cut lead wire type","-40 to 85","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3B114JA","≤21","≤15","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWHC3B104JA",1250,"DC",0.1,"± 5",20.7,13.5,20.6,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHC3B104JA","≤21","≤14","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912JQ",1600,"DC",9.1000000000000004E-3,"± 5",17.8,7.1,18,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912JQ","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912JC",1600,"DC",9.1000000000000004E-3,"± 5",17.8,7.1,13,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912JC","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912JB",1600,"DC",9.1000000000000004E-3,"± 5",17.8,7.1,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912JB","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912J4",1600,"DC",9.1000000000000004E-3,"± 5",17.8,7.1,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912J4","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912J",1600,"DC",9.1000000000000004E-3,"± 5",17.8,7.1,13,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912J","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912HQ",1600,"DC",9.1000000000000004E-3,"± 3",17.8,7.1,18,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912HQ","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912HC",1600,"DC",9.1000000000000004E-3,"± 3",17.8,7.1,13,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912HC","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912HB",1600,"DC",9.1000000000000004E-3,"± 3",17.8,7.1,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912HB","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912H4",1600,"DC",9.1000000000000004E-3,"± 3",17.8,7.1,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912H4","≤18","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C912H",1600,"DC",9.1000000000000004E-3,"± 3",17.8,7.1,13,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C912H","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822JQ",1600,"DC",8.2000000000000007E-3,"± 5",17.8,6.8,17.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822JQ","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822JC",1600,"DC",8.2000000000000007E-3,"± 5",17.8,6.8,12.7,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822JC","≤18","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822JB",1600,"DC",8.2000000000000007E-3,"± 5",17.8,6.8,17.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822JB","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822J4",1600,"DC",8.2000000000000007E-3,"± 5",17.8,6.8,17.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822J4","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822J",1600,"DC",8.2000000000000007E-3,"± 5",17.8,6.8,12.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822J","≤18","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822HQ",1600,"DC",8.2000000000000007E-3,"± 3",17.8,6.8,17.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822HQ","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822HC",1600,"DC",8.2000000000000007E-3,"± 3",17.8,6.8,12.7,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822HC","≤18","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822HB",1600,"DC",8.2000000000000007E-3,"± 3",17.8,6.8,17.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822HB","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822H4",1600,"DC",8.2000000000000007E-3,"± 3",17.8,6.8,17.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822H4","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C822H",1600,"DC",8.2000000000000007E-3,"± 3",17.8,6.8,12.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C822H","≤18","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752JQ",1600,"DC",7.4999999999999997E-3,"± 5",17.8,6.5,17.399999999999999,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752JQ","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752JC",1600,"DC",7.4999999999999997E-3,"± 5",17.8,6.5,12.4,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752JC","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752JB",1600,"DC",7.4999999999999997E-3,"± 5",17.8,6.5,17.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752JB","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752J4",1600,"DC",7.4999999999999997E-3,"± 5",17.8,6.5,17.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752J4","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752J",1600,"DC",7.4999999999999997E-3,"± 5",17.8,6.5,12.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752J","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752HQ",1600,"DC",7.4999999999999997E-3,"± 3",17.8,6.5,17.399999999999999,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752HQ","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752HC",1600,"DC",7.4999999999999997E-3,"± 3",17.8,6.5,12.4,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752HC","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752HB",1600,"DC",7.4999999999999997E-3,"± 3",17.8,6.5,17.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752HB","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752H4",1600,"DC",7.4999999999999997E-3,"± 3",17.8,6.5,17.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752H4","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C752H",1600,"DC",7.4999999999999997E-3,"± 3",17.8,6.5,12.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C752H","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682JQ",1600,"DC",6.7999999999999996E-3,"± 5",17.8,6.1,17.100000000000001,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682JQ","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682JC",1600,"DC",6.7999999999999996E-3,"± 5",17.8,6.1,12.1,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682JC","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682JB",1600,"DC",6.7999999999999996E-3,"± 5",17.8,6.1,17.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682JB","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682J4",1600,"DC",6.7999999999999996E-3,"± 5",17.8,6.1,17.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682J4","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682J",1600,"DC",6.7999999999999996E-3,"± 5",17.8,6.1,12.1,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682J","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682HQ",1600,"DC",6.7999999999999996E-3,"± 3",17.8,6.1,17.100000000000001,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682HQ","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682HC",1600,"DC",6.7999999999999996E-3,"± 3",17.8,6.1,12.1,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682HC","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682HB",1600,"DC",6.7999999999999996E-3,"± 3",17.8,6.1,17.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682HB","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682H4",1600,"DC",6.7999999999999996E-3,"± 3",17.8,6.1,17.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682H4","≤18","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C682H",1600,"DC",6.7999999999999996E-3,"± 3",17.8,6.1,12.1,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C682H","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622JQ",1600,"DC",6.1999999999999998E-3,"± 5",17.8,7.1,14.8,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622JQ","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622JC",1600,"DC",6.1999999999999998E-3,"± 5",17.8,7.1,9.8000000000000007,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622JC","≤18","≤ 8","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622JB",1600,"DC",6.1999999999999998E-3,"± 5",17.8,7.1,14.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622JB","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622J4",1600,"DC",6.1999999999999998E-3,"± 5",17.8,7.1,14.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622J4","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622J",1600,"DC",6.1999999999999998E-3,"± 5",17.8,7.1,9.8000000000000007,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622J","≤18","≤ 8","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622HQ",1600,"DC",6.1999999999999998E-3,"± 3",17.8,7.1,14.8,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622HQ","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622HC",1600,"DC",6.1999999999999998E-3,"± 3",17.8,7.1,9.8000000000000007,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622HC","≤18","≤ 8","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622HB",1600,"DC",6.1999999999999998E-3,"± 3",17.8,7.1,14.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622HB","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622H4",1600,"DC",6.1999999999999998E-3,"± 3",17.8,7.1,14.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622H4","≤18","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C622H",1600,"DC",6.1999999999999998E-3,"± 3",17.8,7.1,9.8000000000000007,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C622H","≤18","≤ 8","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562JQ",1600,"DC",5.5999999999999999E-3,"± 5",17.8,6.8,14.6,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562JQ","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562JC",1600,"DC",5.5999999999999999E-3,"± 5",17.8,6.8,9.6,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562JC","≤18","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562JB",1600,"DC",5.5999999999999999E-3,"± 5",17.8,6.8,14.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562JB","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562J4",1600,"DC",5.5999999999999999E-3,"± 5",17.8,6.8,14.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562J4","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562J",1600,"DC",5.5999999999999999E-3,"± 5",17.8,6.8,9.6,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562J","≤18","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562HQ",1600,"DC",5.5999999999999999E-3,"± 3",17.8,6.8,14.6,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562HQ","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562HC",1600,"DC",5.5999999999999999E-3,"± 3",17.8,6.8,9.6,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562HC","≤18","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562HB",1600,"DC",5.5999999999999999E-3,"± 3",17.8,6.8,14.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562HB","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562H4",1600,"DC",5.5999999999999999E-3,"± 3",17.8,6.8,14.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562H4","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C562H",1600,"DC",5.5999999999999999E-3,"± 3",17.8,6.8,9.6,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C562H","≤18","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512JQ",1600,"DC",5.1000000000000004E-3,"± 5",17.8,6.6,14.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512JQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512JC",1600,"DC",5.1000000000000004E-3,"± 5",17.8,6.6,9.4,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512JC",{"$f":"IF(L652<=9.5,\"≤ \"&ROUNDUP(L652*1,0)/1,\"≤\"&ROUNDUP(L652*1,0)/1)","v":"≤18"},{"$f":"IF(M652<=9,\"≤ \"&ROUNDUP(M652*1,0)/1,\"≤\"&ROUNDUP(M652*1,0)/1)","v":"≤ 7"},{"$f":"IF(N652<=9.5,\"≤ \"&ROUNDUP(N652*2,0)/2,\"≤\"&ROUNDUP(N652*2,0)/2)","v":"≤ 9.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512JB",1600,"DC",5.1000000000000004E-3,"± 5",17.8,6.6,14.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512JB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512J4",1600,"DC",5.1000000000000004E-3,"± 5",17.8,6.6,14.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512J4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512J",1600,"DC",5.1000000000000004E-3,"± 5",17.8,6.6,9.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512J","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512HQ",1600,"DC",5.1000000000000004E-3,"± 3",17.8,6.6,14.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512HQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512HC",1600,"DC",5.1000000000000004E-3,"± 3",17.8,6.6,9.4,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512HC","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512HB",1600,"DC",5.1000000000000004E-3,"± 3",17.8,6.6,14.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512HB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512H4",1600,"DC",5.1000000000000004E-3,"± 3",17.8,6.6,14.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512H4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C512H",1600,"DC",5.1000000000000004E-3,"± 3",17.8,6.6,9.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C512H","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473JQ",1600,"DC",4.7E-2,"± 5",20.6,13.4,26.2,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473JQ","≤21","≤14","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473JC",1600,"DC",4.7E-2,"± 5",20.6,13.4,19.2,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473JC","≤21","≤14","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473JB",1600,"DC",4.7E-2,"± 5",20.6,13.4,24.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473JB","≤21","≤14","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473J4",1600,"DC",4.7E-2,"± 5",20.6,13.4,24.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473J4","≤21","≤14","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473J",1600,"DC",4.7E-2,"± 5",20.6,13.4,19.2,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473J","≤21","≤14","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473HQ",1600,"DC",4.7E-2,"± 3",20.6,13.4,26.2,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473HQ","≤21","≤14","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473HC",1600,"DC",4.7E-2,"± 3",20.6,13.4,19.2,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473HC","≤21","≤14","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473HB",1600,"DC",4.7E-2,"± 3",20.6,13.4,24.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473HB","≤21","≤14","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473H4",1600,"DC",4.7E-2,"± 3",20.6,13.4,24.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473H4","≤21","≤14","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C473H",1600,"DC",4.7E-2,"± 3",20.6,13.4,19.2,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C473H","≤21","≤14","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472JQ",1600,"DC",4.7000000000000002E-3,"± 5",17.8,6.4,14.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472JQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472JC",1600,"DC",4.7000000000000002E-3,"± 5",17.8,6.4,9.1,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472JC","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472JB",1600,"DC",4.7000000000000002E-3,"± 5",17.8,6.4,14.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472JB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472J4",1600,"DC",4.7000000000000002E-3,"± 5",17.8,6.4,14.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472J4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472J",1600,"DC",4.7000000000000002E-3,"± 5",17.8,6.4,9.1,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472J","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472HQ",1600,"DC",4.7000000000000002E-3,"± 3",17.8,6.4,14.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472HQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472HC",1600,"DC",4.7000000000000002E-3,"± 3",17.8,6.4,9.1,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472HC","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472HB",1600,"DC",4.7000000000000002E-3,"± 3",17.8,6.4,14.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472HB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472H4",1600,"DC",4.7000000000000002E-3,"± 3",17.8,6.4,14.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472H4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C472H",1600,"DC",4.7000000000000002E-3,"± 3",17.8,6.4,9.1,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C472H","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433JQ",1600,"DC",4.2999999999999997E-2,"± 5",20.6,12.8,25.6,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433JQ","≤21","≤13","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433JC",1600,"DC",4.2999999999999997E-2,"± 5",20.6,12.8,18.600000000000001,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433JC","≤21","≤13","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433JB",1600,"DC",4.2999999999999997E-2,"± 5",20.6,12.8,23.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433JB","≤21","≤13","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433J4",1600,"DC",4.2999999999999997E-2,"± 5",20.6,12.8,23.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433J4","≤21","≤13","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433J",1600,"DC",4.2999999999999997E-2,"± 5",20.6,12.8,18.600000000000001,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433J","≤21","≤13","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433HQ",1600,"DC",4.2999999999999997E-2,"± 3",20.6,12.8,25.6,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433HQ","≤21","≤13","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433HC",1600,"DC",4.2999999999999997E-2,"± 3",20.6,12.8,18.600000000000001,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433HC","≤21","≤13","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433HB",1600,"DC",4.2999999999999997E-2,"± 3",20.6,12.8,23.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433HB","≤21","≤13","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433H4",1600,"DC",4.2999999999999997E-2,"± 3",20.6,12.8,23.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433H4","≤21","≤13","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C433H",1600,"DC",4.2999999999999997E-2,"± 3",20.6,12.8,18.600000000000001,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C433H","≤21","≤13","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432JQ",1600,"DC",4.3E-3,"± 5",17.8,6.2,13.9,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432JQ","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432JB",1600,"DC",4.3E-3,"± 5",17.8,6.2,13.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432JB","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432J4",1600,"DC",4.3E-3,"± 5",17.8,6.2,13.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432J4","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432HQ",1600,"DC",4.3E-3,"± 3",17.8,6.2,13.9,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432HQ","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432HB",1600,"DC",4.3E-3,"± 3",17.8,6.2,13.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432HB","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C432H4",1600,"DC",4.3E-3,"± 3",17.8,6.2,13.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C432H4","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393JQ",1600,"DC",3.9E-2,"± 5",20.6,12.1,25,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393JQ","≤21","≤13","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393JC",1600,"DC",3.9E-2,"± 5",20.6,12.1,18,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393JC","≤21","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393JB",1600,"DC",3.9E-2,"± 5",20.6,12.1,23,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393JB","≤21","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393J4",1600,"DC",3.9E-2,"± 5",20.6,12.1,23,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393J4","≤21","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393J",1600,"DC",3.9E-2,"± 5",20.6,12.1,18,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393J","≤21","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393HQ",1600,"DC",3.9E-2,"± 3",20.6,12.1,25,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393HQ","≤21","≤13","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393HC",1600,"DC",3.9E-2,"± 3",20.6,12.1,18,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393HC","≤21","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393HB",1600,"DC",3.9E-2,"± 3",20.6,12.1,23,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393HB","≤21","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393H4",1600,"DC",3.9E-2,"± 3",20.6,12.1,23,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393H4","≤21","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C393H",1600,"DC",3.9E-2,"± 3",20.6,12.1,18,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C393H","≤21","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392JQ",1600,"DC",3.8999999999999998E-3,"± 5",17.8,6,13.8,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392JQ","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392JB",1600,"DC",3.8999999999999998E-3,"± 5",17.8,6,13.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392JB","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392J4",1600,"DC",3.8999999999999998E-3,"± 5",17.8,6,13.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392J4","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392HQ",1600,"DC",3.8999999999999998E-3,"± 3",17.8,6,13.8,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392HQ","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392HB",1600,"DC",3.8999999999999998E-3,"± 3",17.8,6,13.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392HB","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C392H4",1600,"DC",3.8999999999999998E-3,"± 3",17.8,6,13.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C392H4","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363JQ",1600,"DC",3.5999999999999997E-2,"± 5",20.6,11.7,24.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363JQ","≤21","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363JC",1600,"DC",3.5999999999999997E-2,"± 5",20.6,11.7,17.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363JC","≤21","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363JB",1600,"DC",3.5999999999999997E-2,"± 5",20.6,11.7,22.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363JB","≤21","≤12","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363J4",1600,"DC",3.5999999999999997E-2,"± 5",20.6,11.7,22.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363J4",{"$f":"IF(L716<=9.5,\"≤ \"&ROUNDUP(L716*1,0)/1,\"≤\"&ROUNDUP(L716*1,0)/1)","v":"≤21"},{"$f":"IF(M716<=9,\"≤ \"&ROUNDUP(M716*1,0)/1,\"≤\"&ROUNDUP(M716*1,0)/1)","v":"≤12"},{"$f":"IF(N716<=9.5,\"≤ \"&ROUNDUP(N716*2,0)/2,\"≤\"&ROUNDUP(N716*2,0)/2)","v":"≤22.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363J",1600,"DC",3.5999999999999997E-2,"± 5",20.6,11.7,17.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363J","≤21","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363HQ",1600,"DC",3.5999999999999997E-2,"± 3",20.6,11.7,24.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363HQ","≤21","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363HC",1600,"DC",3.5999999999999997E-2,"± 3",20.6,11.7,17.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363HC","≤21","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363HB",1600,"DC",3.5999999999999997E-2,"± 3",20.6,11.7,22.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363HB","≤21","≤12","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363H4",1600,"DC",3.5999999999999997E-2,"± 3",20.6,11.7,22.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363H4","≤21","≤12","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C363H",1600,"DC",3.5999999999999997E-2,"± 3",20.6,11.7,17.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C363H","≤21","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362JQ",1600,"DC",3.5999999999999999E-3,"± 5",17.8,5.7,13.5,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362JB",1600,"DC",3.5999999999999999E-3,"± 5",17.8,5.7,13.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362J4",1600,"DC",3.5999999999999999E-3,"± 5",17.8,5.7,13.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362HQ",1600,"DC",3.5999999999999999E-3,"± 3",17.8,5.7,13.5,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362HB",1600,"DC",3.5999999999999999E-3,"± 3",17.8,5.7,13.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C362H4",1600,"DC",3.5999999999999999E-3,"± 3",17.8,5.7,13.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C362H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333JQ",1600,"DC",3.3000000000000002E-2,"± 5",20.6,11.2,24,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333JQ","≤21","≤12","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333JC",1600,"DC",3.3000000000000002E-2,"± 5",20.6,11.2,17,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333JC","≤21","≤12","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333JB",1600,"DC",3.3000000000000002E-2,"± 5",20.6,11.2,22,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333JB","≤21","≤12","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333J4",1600,"DC",3.3000000000000002E-2,"± 5",20.6,11.2,22,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333J4","≤21","≤12","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333J",1600,"DC",3.3000000000000002E-2,"± 5",20.6,11.2,17,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333J","≤21","≤12","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333HQ",1600,"DC",3.3000000000000002E-2,"± 3",20.6,11.2,24,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333HQ","≤21","≤12","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333HC",1600,"DC",3.3000000000000002E-2,"± 3",20.6,11.2,17,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333HC","≤21","≤12","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333HB",1600,"DC",3.3000000000000002E-2,"± 3",20.6,11.2,22,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333HB","≤21","≤12","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333H4",1600,"DC",3.3000000000000002E-2,"± 3",20.6,11.2,22,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333H4","≤21","≤12","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C333H",1600,"DC",3.3000000000000002E-2,"± 3",20.6,11.2,17,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C333H","≤21","≤12","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332JQ",1600,"DC",3.3E-3,"± 5",17.8,5.6,13.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332JB",1600,"DC",3.3E-3,"± 5",17.8,5.6,13.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332J4",1600,"DC",3.3E-3,"± 5",17.8,5.6,13.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332HQ",1600,"DC",3.3E-3,"± 3",17.8,5.6,13.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332HB",1600,"DC",3.3E-3,"± 3",17.8,5.6,13.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C332H4",1600,"DC",3.3E-3,"± 3",17.8,5.6,13.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C332H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303JQ",1600,"DC",0.03,"± 5",20.6,10.7,23.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303JQ","≤21","≤11","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303JC",1600,"DC",0.03,"± 5",20.6,10.7,16.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303JC","≤21","≤11","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303JB",1600,"DC",0.03,"± 5",20.6,10.7,21.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303JB","≤21","≤11","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303J4",1600,"DC",0.03,"± 5",20.6,10.7,21.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303J4","≤21","≤11","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303J",1600,"DC",0.03,"± 5",20.6,10.7,16.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303J","≤21","≤11","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303HQ",1600,"DC",0.03,"± 3",20.6,10.7,23.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303HQ","≤21","≤11","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303HC",1600,"DC",0.03,"± 3",20.6,10.7,16.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303HC","≤21","≤11","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303HB",1600,"DC",0.03,"± 3",20.6,10.7,21.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303HB","≤21","≤11","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303H4",1600,"DC",0.03,"± 3",20.6,10.7,21.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303H4","≤21","≤11","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C303H",1600,"DC",0.03,"± 3",20.6,10.7,16.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C303H","≤21","≤11","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302JQ",1600,"DC",3.0000000000000001E-3,"± 5",17.8,5.5,13.2,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302JB",1600,"DC",3.0000000000000001E-3,"± 5",17.8,5.5,13.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302J4",1600,"DC",3.0000000000000001E-3,"± 5",17.8,5.5,13.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302HQ",1600,"DC",3.0000000000000001E-3,"± 3",17.8,5.5,13.2,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302HB",1600,"DC",3.0000000000000001E-3,"± 3",17.8,5.5,13.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C302H4",1600,"DC",3.0000000000000001E-3,"± 3",17.8,5.5,13.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C302H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273JQ",1600,"DC",2.7E-2,"± 5",20.6,10,22.9,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273JQ","≤21","≤10","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273JC",1600,"DC",2.7E-2,"± 5",20.6,10,15.9,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273JC","≤21","≤10","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273JB",1600,"DC",2.7E-2,"± 5",20.6,10,20.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273JB","≤21","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273J4",1600,"DC",2.7E-2,"± 5",20.6,10,20.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273J4","≤21","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273J",1600,"DC",2.7E-2,"± 5",20.6,10,15.9,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273J","≤21","≤10","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273HQ",1600,"DC",2.7E-2,"± 3",20.6,10,22.9,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273HQ","≤21","≤10","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273HC",1600,"DC",2.7E-2,"± 3",20.6,10,15.9,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273HC","≤21","≤10","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273HB",1600,"DC",2.7E-2,"± 3",20.6,10,20.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273HB","≤21","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273H4",1600,"DC",2.7E-2,"± 3",20.6,10,20.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273H4","≤21","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C273H",1600,"DC",2.7E-2,"± 3",20.6,10,15.9,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C273H","≤21","≤10","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272JQ",1600,"DC",2.7000000000000001E-3,"± 5",17.8,5.2,13,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272JQ","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272JB",1600,"DC",2.7000000000000001E-3,"± 5",17.8,5.2,13,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272JB","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272J4",1600,"DC",2.7000000000000001E-3,"± 5",17.8,5.2,13,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272J4","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272HQ",1600,"DC",2.7000000000000001E-3,"± 3",17.8,5.2,13,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272HQ","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272HB",1600,"DC",2.7000000000000001E-3,"± 3",17.8,5.2,13,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272HB","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C272H4",1600,"DC",2.7000000000000001E-3,"± 3",17.8,5.2,13,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C272H4","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243JQ",1600,"DC",2.4E-2,"± 5",20.6,9.6,22.4,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243JQ","≤21","≤10","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243JC",1600,"DC",2.4E-2,"± 5",20.6,9.6,15.4,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243JC","≤21","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243JB",1600,"DC",2.4E-2,"± 5",20.6,9.6,20.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243JB","≤21","≤10","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243J4",1600,"DC",2.4E-2,"± 5",20.6,9.6,20.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243J4",{"$f":"IF(L780<=9.5,\"≤ \"&ROUNDUP(L780*1,0)/1,\"≤\"&ROUNDUP(L780*1,0)/1)","v":"≤21"},{"$f":"IF(M780<=9,\"≤ \"&ROUNDUP(M780*1,0)/1,\"≤\"&ROUNDUP(M780*1,0)/1)","v":"≤10"},{"$f":"IF(N780<=9.5,\"≤ \"&ROUNDUP(N780*2,0)/2,\"≤\"&ROUNDUP(N780*2,0)/2)","v":"≤20.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243J",1600,"DC",2.4E-2,"± 5",20.6,9.6,15.4,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243J","≤21","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243HQ",1600,"DC",2.4E-2,"± 3",20.6,9.6,22.4,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243HQ","≤21","≤10","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243HC",1600,"DC",2.4E-2,"± 3",20.6,9.6,15.4,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243HC","≤21","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243HB",1600,"DC",2.4E-2,"± 3",20.6,9.6,20.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243HB","≤21","≤10","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243H4",1600,"DC",2.4E-2,"± 3",20.6,9.6,20.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243H4","≤21","≤10","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C243H",1600,"DC",2.4E-2,"± 3",20.6,9.6,15.4,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C243H","≤21","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242JQ",1600,"DC",2.3999999999999998E-3,"± 5",17.8,7,14.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242JQ","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242JB",1600,"DC",2.3999999999999998E-3,"± 5",17.8,7,14.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242JB","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242J4",1600,"DC",2.3999999999999998E-3,"± 5",17.8,7,14.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242J4","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242HQ",1600,"DC",2.3999999999999998E-3,"± 3",17.8,7,14.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242HQ","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242HB",1600,"DC",2.3999999999999998E-3,"± 3",17.8,7,14.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242HB","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C242H4",1600,"DC",2.3999999999999998E-3,"± 3",17.8,7,14.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C242H4","≤18","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223JQ",1600,"DC",2.1999999999999999E-2,"± 5",20.6,9.1,22,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223JQ","≤21","≤10","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223JC",1600,"DC",2.1999999999999999E-2,"± 5",20.6,9.1,15,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223JC","≤21","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223JB",1600,"DC",2.1999999999999999E-2,"± 5",20.6,9.1,20,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223JB","≤21","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223J4",1600,"DC",2.1999999999999999E-2,"± 5",20.6,9.1,20,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223J4","≤21","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223J",1600,"DC",2.1999999999999999E-2,"± 5",20.6,9.1,15,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223J","≤21","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223HQ",1600,"DC",2.1999999999999999E-2,"± 3",20.6,9.1,22,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223HQ","≤21","≤10","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223HC",1600,"DC",2.1999999999999999E-2,"± 3",20.6,9.1,15,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223HC","≤21","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223HB",1600,"DC",2.1999999999999999E-2,"± 3",20.6,9.1,20,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223HB","≤21","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223H4",1600,"DC",2.1999999999999999E-2,"± 3",20.6,9.1,20,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223H4","≤21","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C223H",1600,"DC",2.1999999999999999E-2,"± 3",20.6,9.1,15,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C223H","≤21","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222JQ",1600,"DC",2.2000000000000001E-3,"± 5",17.8,6.7,14.5,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222JQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222JB",1600,"DC",2.2000000000000001E-3,"± 5",17.8,6.7,14.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222JB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222J4",1600,"DC",2.2000000000000001E-3,"± 5",17.8,6.7,14.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222J4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222HQ",1600,"DC",2.2000000000000001E-3,"± 3",17.8,6.7,14.5,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222HQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222HB",1600,"DC",2.2000000000000001E-3,"± 3",17.8,6.7,14.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222HB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C222H4",1600,"DC",2.2000000000000001E-3,"± 3",17.8,6.7,14.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C222H4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203JQ",1600,"DC",0.02,"± 5",20.6,8.6999999999999993,21.6,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203JQ","≤21","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203JC",1600,"DC",0.02,"± 5",20.6,8.6999999999999993,14.6,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203JC","≤21","≤ 9","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203JB",1600,"DC",0.02,"± 5",20.6,8.6999999999999993,19.600000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203JB","≤21","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203J4",1600,"DC",0.02,"± 5",20.6,8.6999999999999993,19.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203J4","≤21","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203J",1600,"DC",0.02,"± 5",20.6,8.6999999999999993,14.6,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203J","≤21","≤ 9","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203HQ",1600,"DC",0.02,"± 3",20.6,8.6999999999999993,21.6,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203HQ","≤21","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203HC",1600,"DC",0.02,"± 3",20.6,8.6999999999999993,14.6,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203HC","≤21","≤ 9","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203HB",1600,"DC",0.02,"± 3",20.6,8.6999999999999993,19.600000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203HB","≤21","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203H4",1600,"DC",0.02,"± 3",20.6,8.6999999999999993,19.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203H4","≤21","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C203H",1600,"DC",0.02,"± 3",20.6,8.6999999999999993,14.6,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C203H","≤21","≤ 9","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202JQ",1600,"DC",2E-3,"± 5",17.8,6.6,14.3,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202JQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202JB",1600,"DC",2E-3,"± 5",17.8,6.6,14.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202JB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202J4",1600,"DC",2E-3,"± 5",17.8,6.6,14.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202J4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202HQ",1600,"DC",2E-3,"± 3",17.8,6.6,14.3,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202HQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202HB",1600,"DC",2E-3,"± 3",17.8,6.6,14.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202HB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C202H4",1600,"DC",2E-3,"± 3",17.8,6.6,14.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C202H4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183JQ",1600,"DC",1.7999999999999999E-2,"± 5",20.6,8.1999999999999993,21.1,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183JQ","≤21","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183JC",1600,"DC",1.7999999999999999E-2,"± 5",20.6,8.1999999999999993,14.1,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183JC","≤21","≤ 9","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183JB",1600,"DC",1.7999999999999999E-2,"± 5",20.6,8.1999999999999993,19.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183JB","≤21","≤ 9","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183J4",1600,"DC",1.7999999999999999E-2,"± 5",20.6,8.1999999999999993,19.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183J4","≤21","≤ 9","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183J",1600,"DC",1.7999999999999999E-2,"± 5",20.6,8.1999999999999993,14.1,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183J","≤21","≤ 9","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183HQ",1600,"DC",1.7999999999999999E-2,"± 3",20.6,8.1999999999999993,21.1,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183HQ","≤21","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183HC",1600,"DC",1.7999999999999999E-2,"± 3",20.6,8.1999999999999993,14.1,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183HC","≤21","≤ 9","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183HB",1600,"DC",1.7999999999999999E-2,"± 3",20.6,8.1999999999999993,19.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183HB","≤21","≤ 9","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183H4",1600,"DC",1.7999999999999999E-2,"± 3",20.6,8.1999999999999993,19.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183H4","≤21","≤ 9","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C183H",1600,"DC",1.7999999999999999E-2,"± 3",20.6,8.1999999999999993,14.1,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C183H","≤21","≤ 9","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182JQ",1600,"DC",1.8E-3,"± 5",17.8,6.4,14.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182JQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182JB",1600,"DC",1.8E-3,"± 5",17.8,6.4,14.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182JB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182J4",1600,"DC",1.8E-3,"± 5",17.8,6.4,14.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182J4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182HQ",1600,"DC",1.8E-3,"± 3",17.8,6.4,14.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182HQ","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182HB",1600,"DC",1.8E-3,"± 3",17.8,6.4,14.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182HB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C182H4",1600,"DC",1.8E-3,"± 3",17.8,6.4,14.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C182H4","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163JQ",1600,"DC",1.6E-2,"± 5",20.3,7.9,18.8,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163JQ","≤21","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163JC",1600,"DC",1.6E-2,"± 5",20.3,7.9,13.8,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163JC","≤21","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163JB",1600,"DC",1.6E-2,"± 5",20.3,7.9,18.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163JB","≤21","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163J4",1600,"DC",1.6E-2,"± 5",20.3,7.9,18.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163J4",{"$f":"IF(L844<=9.5,\"≤ \"&ROUNDUP(L844*1,0)/1,\"≤\"&ROUNDUP(L844*1,0)/1)","v":"≤21"},{"$f":"IF(M844<=9,\"≤ \"&ROUNDUP(M844*1,0)/1,\"≤\"&ROUNDUP(M844*1,0)/1)","v":"≤ 8"},{"$f":"IF(N844<=9.5,\"≤ \"&ROUNDUP(N844*2,0)/2,\"≤\"&ROUNDUP(N844*2,0)/2)","v":"≤19"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163J",1600,"DC",1.6E-2,"± 5",20.3,7.9,13.8,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163J","≤21","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163HQ",1600,"DC",1.6E-2,"± 3",20.3,7.9,18.8,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163HQ","≤21","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163HC",1600,"DC",1.6E-2,"± 3",20.3,7.9,13.8,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163HC","≤21","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163HB",1600,"DC",1.6E-2,"± 3",20.3,7.9,18.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163HB","≤21","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163H4",1600,"DC",1.6E-2,"± 3",20.3,7.9,18.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163H4","≤21","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C163H",1600,"DC",1.6E-2,"± 3",20.3,7.9,13.8,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C163H","≤21","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162JQ",1600,"DC",1.6000000000000001E-3,"± 5",17.8,6.1,13.9,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162JQ","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162JB",1600,"DC",1.6000000000000001E-3,"± 5",17.8,6.1,13.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162JB","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162J4",1600,"DC",1.6000000000000001E-3,"± 5",17.8,6.1,13.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162J4","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162HQ",1600,"DC",1.6000000000000001E-3,"± 3",17.8,6.1,13.9,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162HQ","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162HB",1600,"DC",1.6000000000000001E-3,"± 3",17.8,6.1,13.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162HB","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C162H4",1600,"DC",1.6000000000000001E-3,"± 3",17.8,6.1,13.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C162H4","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153JQ",1600,"DC",1.4999999999999999E-2,"± 5",20.3,7.6,18.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153JQ","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153JC",1600,"DC",1.4999999999999999E-2,"± 5",20.3,7.6,13.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153JC","≤21","≤ 8","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153JB",1600,"DC",1.4999999999999999E-2,"± 5",20.3,7.6,18.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153JB","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153J4",1600,"DC",1.4999999999999999E-2,"± 5",20.3,7.6,18.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153J4","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153J",1600,"DC",1.4999999999999999E-2,"± 5",20.3,7.6,13.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153J","≤21","≤ 8","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153HQ",1600,"DC",1.4999999999999999E-2,"± 3",20.3,7.6,18.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153HQ","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153HC",1600,"DC",1.4999999999999999E-2,"± 3",20.3,7.6,13.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153HC","≤21","≤ 8","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153HB",1600,"DC",1.4999999999999999E-2,"± 3",20.3,7.6,18.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153HB","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153H4",1600,"DC",1.4999999999999999E-2,"± 3",20.3,7.6,18.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153H4","≤21","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C153H",1600,"DC",1.4999999999999999E-2,"± 3",20.3,7.6,13.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C153H","≤21","≤ 8","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152JQ",1600,"DC",1.5E-3,"± 5",17.8,5.9,13.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152JQ","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152JB",1600,"DC",1.5E-3,"± 5",17.8,5.9,13.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152JB","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152J4",1600,"DC",1.5E-3,"± 5",17.8,5.9,13.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152J4","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152HQ",1600,"DC",1.5E-3,"± 3",17.8,5.9,13.7,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152HQ","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152HB",1600,"DC",1.5E-3,"± 3",17.8,5.9,13.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152HB","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C152H4",1600,"DC",1.5E-3,"± 3",17.8,5.9,13.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C152H4","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133JQ",1600,"DC",1.2999999999999999E-2,"± 5",20.3,7.1,18,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133JQ","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133JC",1600,"DC",1.2999999999999999E-2,"± 5",20.3,7.1,13,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133JC","≤21","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133JB",1600,"DC",1.2999999999999999E-2,"± 5",20.3,7.1,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133JB","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133J4",1600,"DC",1.2999999999999999E-2,"± 5",20.3,7.1,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133J4","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133J",1600,"DC",1.2999999999999999E-2,"± 5",20.3,7.1,13,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133J","≤21","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133HQ",1600,"DC",1.2999999999999999E-2,"± 3",20.3,7.1,18,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133HQ","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133HC",1600,"DC",1.2999999999999999E-2,"± 3",20.3,7.1,13,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133HC","≤21","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133HB",1600,"DC",1.2999999999999999E-2,"± 3",20.3,7.1,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133HB","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133H4",1600,"DC",1.2999999999999999E-2,"± 3",20.3,7.1,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133H4","≤21","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C133H",1600,"DC",1.2999999999999999E-2,"± 3",20.3,7.1,13,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C133H","≤21","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132JQ",1600,"DC",1.2999999999999999E-3,"± 5",17.8,5.7,13.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132JB",1600,"DC",1.2999999999999999E-3,"± 5",17.8,5.7,13.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132J4",1600,"DC",1.2999999999999999E-3,"± 5",17.8,5.7,13.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132HQ",1600,"DC",1.2999999999999999E-3,"± 3",17.8,5.7,13.4,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132HB",1600,"DC",1.2999999999999999E-3,"± 3",17.8,5.7,13.4,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C132H4",1600,"DC",1.2999999999999999E-3,"± 3",17.8,5.7,13.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C132H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123JQ",1600,"DC",1.2E-2,"± 5",20.3,6.8,17.8,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123JQ","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123JC",1600,"DC",1.2E-2,"± 5",20.3,6.8,12.8,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123JC","≤21","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123JB",1600,"DC",1.2E-2,"± 5",20.3,6.8,17.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123JB","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123J4",1600,"DC",1.2E-2,"± 5",20.3,6.8,17.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123J4","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123J",1600,"DC",1.2E-2,"± 5",20.3,6.8,12.8,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123J","≤21","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123HQ",1600,"DC",1.2E-2,"± 3",20.3,6.8,17.8,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123HQ","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123HC",1600,"DC",1.2E-2,"± 3",20.3,6.8,12.8,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123HC","≤21","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123HB",1600,"DC",1.2E-2,"± 3",20.3,6.8,17.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123HB","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123H4",1600,"DC",1.2E-2,"± 3",20.3,6.8,17.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123H4","≤21","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C123H",1600,"DC",1.2E-2,"± 3",20.3,6.8,12.8,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C123H","≤21","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122JQ",1600,"DC",1.1999999999999999E-3,"± 5",17.8,5.5,13.2,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122JB",1600,"DC",1.1999999999999999E-3,"± 5",17.8,5.5,13.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122J4",1600,"DC",1.1999999999999999E-3,"± 5",17.8,5.5,13.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122HQ",1600,"DC",1.1999999999999999E-3,"± 3",17.8,5.5,13.2,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122HB",1600,"DC",1.1999999999999999E-3,"± 3",17.8,5.5,13.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C122H4",1600,"DC",1.1999999999999999E-3,"± 3",17.8,5.5,13.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C122H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113JQ",1600,"DC",1.0999999999999999E-2,"± 5",20.3,6.6,17.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113JQ","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113JC",1600,"DC",1.0999999999999999E-2,"± 5",20.3,6.6,12.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113JC","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113JB",1600,"DC",1.0999999999999999E-2,"± 5",20.3,6.6,17.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113JB","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113J4",1600,"DC",1.0999999999999999E-2,"± 5",20.3,6.6,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113J4",{"$f":"IF(L908<=9.5,\"≤ \"&ROUNDUP(L908*1,0)/1,\"≤\"&ROUNDUP(L908*1,0)/1)","v":"≤21"},{"$f":"IF(M908<=9,\"≤ \"&ROUNDUP(M908*1,0)/1,\"≤\"&ROUNDUP(M908*1,0)/1)","v":"≤ 7"},{"$f":"IF(N908<=9.5,\"≤ \"&ROUNDUP(N908*2,0)/2,\"≤\"&ROUNDUP(N908*2,0)/2)","v":"≤17.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113J",1600,"DC",1.0999999999999999E-2,"± 5",20.3,6.6,12.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113J","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113HQ",1600,"DC",1.0999999999999999E-2,"± 3",20.3,6.6,17.5,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113HQ","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113HC",1600,"DC",1.0999999999999999E-2,"± 3",20.3,6.6,12.5,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113HC","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113HB",1600,"DC",1.0999999999999999E-2,"± 3",20.3,6.6,17.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113HB","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113H4",1600,"DC",1.0999999999999999E-2,"± 3",20.3,6.6,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113H4","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C113H",1600,"DC",1.0999999999999999E-2,"± 3",20.3,6.6,12.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C113H","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112JQ",1600,"DC",1.1000000000000001E-3,"± 5",17.8,5.4,13.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112JQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112JB",1600,"DC",1.1000000000000001E-3,"± 5",17.8,5.4,13.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112JB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112J4",1600,"DC",1.1000000000000001E-3,"± 5",17.8,5.4,13.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112J4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112HQ",1600,"DC",1.1000000000000001E-3,"± 3",17.8,5.4,13.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112HQ","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112HB",1600,"DC",1.1000000000000001E-3,"± 3",17.8,5.4,13.1,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112HB","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C112H4",1600,"DC",1.1000000000000001E-3,"± 3",17.8,5.4,13.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C112H4","≤18","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103JQ",1600,"DC",0.01,"± 5",20.3,6.4,17.3,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103JQ","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103JC",1600,"DC",0.01,"± 5",20.3,6.4,12.3,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103JC","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103JB",1600,"DC",0.01,"± 5",20.3,6.4,17.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103JB","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103J4",1600,"DC",0.01,"± 5",20.3,6.4,17.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103J4","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103J",1600,"DC",0.01,"± 5",20.3,6.4,12.3,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103J","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103HQ",1600,"DC",0.01,"± 3",20.3,6.4,17.3,17.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103HQ","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103HC",1600,"DC",0.01,"± 3",20.3,6.4,12.3,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103HC","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103HB",1600,"DC",0.01,"± 3",20.3,6.4,17.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103HB","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103H4",1600,"DC",0.01,"± 3",20.3,6.4,17.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103H4","≤21","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C103H",1600,"DC",0.01,"± 3",20.3,6.4,12.3,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C103H","≤21","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102JQ",1600,"DC",1E-3,"± 5",17.8,5.2,13,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102JQ","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102JB",1600,"DC",1E-3,"± 5",17.8,5.2,13,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102JB","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102J4",1600,"DC",1E-3,"± 5",17.8,5.2,13,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102J4","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102HQ",1600,"DC",1E-3,"± 3",17.8,5.2,13,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102HQ","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102HB",1600,"DC",1E-3,"± 3",17.8,5.2,13,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102HB","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWHA3C102H4",1600,"DC",1E-3,"± 3",17.8,5.2,13,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWHA3C102H4","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8473RHA",800,"DC",4.7E-2,"± 3",15.7,9.6999999999999993,19.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8473RHA","≤16","≤10","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8473HAQ",800,"DC",4.7E-2,"± 3",15.7,9.6999999999999993,21.1,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8473HAQ","≤16","≤10","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8473HAB",800,"DC",4.7E-2,"± 3",15.7,9.6999999999999993,19.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8473HAB","≤16","≤10","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8473HA",800,"DC",4.7E-2,"± 3",15.7,9.6999999999999993,14.1,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8473HA","≤16","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8393RHA",800,"DC",3.9E-2,"± 3",15.7,8.9,18.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8393RHA","≤16","≤ 9","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8393HAQ",800,"DC",3.9E-2,"± 3",15.7,8.9,20.3,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8393HAQ","≤16","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8393HAB",800,"DC",3.9E-2,"± 3",15.7,8.9,18.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8393HAB","≤16","≤ 9","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8393HA",800,"DC",3.9E-2,"± 3",15.7,8.9,13.3,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8393HA","≤16","≤ 9","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8333RHA",800,"DC",3.3000000000000002E-2,"± 3",15.7,8.4,17.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8333RHA","≤16","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8333HAQ",800,"DC",3.3000000000000002E-2,"± 3",15.7,8.4,19.8,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8333HAQ","≤16","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8333HAB",800,"DC",3.3000000000000002E-2,"± 3",15.7,8.4,17.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8333HAB","≤16","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8333HA",800,"DC",3.3000000000000002E-2,"± 3",15.7,8.4,12.8,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8333HA","≤16","≤ 9","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8273RHA",800,"DC",2.7E-2,"± 3",15.7,7.6,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8273RHA","≤16","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8273HAQ",800,"DC",2.7E-2,"± 3",15.7,7.6,19,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8273HAQ","≤16","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8273HAB",800,"DC",2.7E-2,"± 3",15.7,7.6,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8273HAB","≤16","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8273HA",800,"DC",2.7E-2,"± 3",15.7,7.6,12,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8273HA","≤16","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8223RHA",800,"DC",2.1999999999999999E-2,"± 3",15.7,7.1,16.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8223RHA","≤16","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8223HAQ",800,"DC",2.1999999999999999E-2,"± 3",15.7,7.1,18.5,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8223HAQ","≤16","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8223HAC",800,"DC",2.1999999999999999E-2,"± 3",15.7,7.1,11.5,12.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8223HAC","≤16","≤ 8","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8223HAB",800,"DC",2.1999999999999999E-2,"± 3",15.7,7.1,16.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8223HAB","≤16","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8223HA",800,"DC",2.1999999999999999E-2,"± 3",15.7,7.1,11.5,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8223HA","≤16","≤ 8","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8183RHA",800,"DC",1.7999999999999999E-2,"± 3",15.7,6.6,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8183RHA","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8183HAQ",800,"DC",1.7999999999999999E-2,"± 3",15.7,6.6,18,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8183HAQ","≤16","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8183HAC",800,"DC",1.7999999999999999E-2,"± 3",15.7,6.6,11,12.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8183HAC","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8183HAB",800,"DC",1.7999999999999999E-2,"± 3",15.7,6.6,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8183HAB","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8183HA",800,"DC",1.7999999999999999E-2,"± 3",15.7,6.6,11,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8183HA","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8153RHA",800,"DC",1.4999999999999999E-2,"± 3",15.4,6.2,15.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8153RHA","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8153HAQ",800,"DC",1.4999999999999999E-2,"± 3",15.4,6.2,15.6,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8153HAQ","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8153HAC",800,"DC",1.4999999999999999E-2,"± 3",15.4,6.2,10.6,12.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8153HAC","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8153HAB",800,"DC",1.4999999999999999E-2,"± 3",15.4,6.2,15.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8153HAB","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8153HA",800,"DC",1.4999999999999999E-2,"± 3",15.4,6.2,10.6,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8153HA","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8123RHA",800,"DC",1.2E-2,"± 3",15.4,5.8,15.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8123RHA","≤16","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8123HAQ",800,"DC",1.2E-2,"± 3",15.4,5.8,15.2,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8123HAQ","≤16","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8123HAC",800,"DC",1.2E-2,"± 3",15.4,5.8,10.199999999999999,12.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8123HAC","≤16","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8123HAB",800,"DC",1.2E-2,"± 3",15.4,5.8,15.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8123HAB","≤16","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8123HA",800,"DC",1.2E-2,"± 3",15.4,5.8,10.199999999999999,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8123HA",{"$f":"IF(L972<=9.5,\"≤ \"&ROUNDUP(L972*1,0)/1,\"≤\"&ROUNDUP(L972*1,0)/1)","v":"≤16"},{"$f":"IF(M972<=9,\"≤ \"&ROUNDUP(M972*1,0)/1,\"≤\"&ROUNDUP(M972*1,0)/1)","v":"≤ 6"},{"$f":"IF(N972<=9.5,\"≤ \"&ROUNDUP(N972*2,0)/2,\"≤\"&ROUNDUP(N972*2,0)/2)","v":"≤10.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8103RHA",800,"DC",0.01,"± 3",15.4,5.4,14.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8103RHA","≤16","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8103HAQ",800,"DC",0.01,"± 3",15.4,5.4,14.8,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8103HAQ","≤16","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8103HAC",800,"DC",0.01,"± 3",15.4,5.4,9.8000000000000007,12.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8103HAC","≤16","≤ 6","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8103HAB",800,"DC",0.01,"± 3",15.4,5.4,14.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8103HAB","≤16","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(A)","ECWH8103HA",800,"DC",0.01,"± 3",15.4,5.4,9.8000000000000007,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH8103HA","≤16","≤ 6","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6334HCC",630,"DC",0.33,"± 3",20.7,14.7,21.1,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6334HCC","≤21","≤15","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6334HC",630,"DC",0.33,"± 3",20.7,14.7,21.1,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6334HC","≤21","≤15","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6324HCC",630,"DC",0.32,"± 3",20.7,14.5,20.9,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6324HCC","≤21","≤15","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6324HC",630,"DC",0.32,"± 3",20.7,14.5,20.9,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6324HC","≤21","≤15","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6304HCC",630,"DC",0.3,"± 3",20.7,14.8,19.600000000000001,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6304HCC","≤21","≤15","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6304HC",630,"DC",0.3,"± 3",20.7,14.8,19.600000000000001,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6304HC","≤21","≤15","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6284HCC",630,"DC",0.28000000000000003,"± 3",20.7,14.3,19.100000000000001,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6284HCC","≤21","≤15","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6284HC",630,"DC",0.28000000000000003,"± 3",20.7,14.3,19.100000000000001,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6284HC","≤21","≤15","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6274HCC",630,"DC",0.27,"± 3",20.7,14,18.899999999999999,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6274HCC","≤21","≤14","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6274HC",630,"DC",0.27,"± 3",20.7,14,18.899999999999999,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6274HC","≤21","≤14","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6244HCC",630,"DC",0.24,"± 3",20.7,13.2,18.100000000000001,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6244HCC","≤21","≤14","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6244HC",630,"DC",0.24,"± 3",20.7,13.2,18.100000000000001,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6244HC","≤21","≤14","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6214RHC",630,"DC",0.21,"± 3",20.7,12.4,22.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6214RHC","≤21","≤13","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6214HCC",630,"DC",0.21,"± 3",20.7,12.4,17.2,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6214HCC","≤21","≤13","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6214HC",630,"DC",0.21,"± 3",20.7,12.4,17.2,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6214HC","≤21","≤13","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6184RHC",630,"DC",0.18,"± 3",20.7,11.5,21.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",250,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6184RHC","≤21","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6184HCC",630,"DC",0.18,"± 3",20.7,11.5,16.3,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6184HCC","≤21","≤12","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6184HC",630,"DC",0.18,"± 3",20.7,11.5,16.3,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6184HC","≤21","≤12","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6124RHC",630,"DC",0.12,"± 3",20.7,9.4,19.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6124RHC","≤21","≤10","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6124HCC",630,"DC",0.12,"± 3",20.7,9.4,14.3,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6124HCC","≤21","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6124HC",630,"DC",0.12,"± 3",20.7,9.4,14.3,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6124HC","≤21","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6114RHC",630,"DC",0.11,"± 3",20.7,9,18.899999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6114RHC","≤21","≤ 9","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6114HCC",630,"DC",0.11,"± 3",20.7,9,13.9,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6114HCC","≤21","≤ 9","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(C)","ECWH6114HC",630,"DC",0.11,"± 3",20.7,9,13.9,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH6114HC","≤21","≤ 9","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20912HV",2000,"DC",9.1000000000000004E-3,"± 3",23,10,19,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20912HV","≤23","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20822JVB",2000,"DC",8.2000000000000007E-3,"± 5",23,10,23,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20822JVB","≤23","≤10","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20752JV",2000,"DC",7.4999999999999997E-3,"± 5",23,9.5,18,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20752JV","≤23","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20622RJV",2000,"DC",6.1999999999999998E-3,"± 5",23,8,21.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20622RJV","≤23","≤ 8","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20622JV",2000,"DC",6.1999999999999998E-3,"± 5",23,8,16.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20622JV","≤23","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20562HVB",2000,"DC",5.5999999999999999E-3,"± 3",23,7.5,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20562HVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20512RHV",2000,"DC",5.1000000000000004E-3,"± 3",23,7.5,21,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20512RHV","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20472JVB",2000,"DC",4.7000000000000002E-3,"± 5",23,7,20.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20472JVB","≤23","≤ 7","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20432HV",2000,"DC",4.3E-3,"± 3",18,9.5,16,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20432HV","≤18","≤10","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20392RHV",2000,"DC",3.8999999999999998E-3,"± 3",18,9,21,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20392RHV","≤18","≤ 9","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20362JVB",2000,"DC",3.5999999999999999E-3,"± 5",18,9,20.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20362JVB","≤18","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20332HV",2000,"DC",3.3E-3,"± 3",18,8.5,15.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20332HV","≤18","≤ 9","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20302JVB",2000,"DC",3.0000000000000001E-3,"± 5",18,9.5,21,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20302JVB","≤18","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20272JV",2000,"DC",2.7000000000000001E-3,"± 5",18,9,16,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20272JV","≤18","≤ 9","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20242RJV",2000,"DC",2.3999999999999998E-3,"± 5",18,8.5,20.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20242RJV","≤18","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20222RHV",2000,"DC",2.2000000000000001E-3,"± 3",18,8.5,20,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20222RHV","≤18","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20202HVB",2000,"DC",2E-3,"± 3",18,8,20,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20202HVB","≤18","≤ 8","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20182JVB",2000,"DC",1.8E-3,"± 5",18,8,19.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20182JVB","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20162RHV",2000,"DC",1.6000000000000001E-3,"± 3",18,7.5,19.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20162RHV","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20153HVB",2000,"DC",1.4999999999999999E-2,"± 3",23,12,26.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20153HVB","≤23","≤12","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20153HV",2000,"DC",1.4999999999999999E-2,"± 3",23,12,21.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20153HV","≤23","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20133JVB",2000,"DC",1.2999999999999999E-2,"± 5",23,12,26,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20133JVB","≤23","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20133HV",2000,"DC",1.2999999999999999E-2,"± 3",23,12,21,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20133HV","≤23","≤12","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20123RJV",2000,"DC",1.2E-2,"± 5",23,11.5,25.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20123RJV","≤23","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20122JV",2000,"DC",1.1999999999999999E-3,"± 5",18,7,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20122JV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20113RJV",2000,"DC",1.0999999999999999E-2,"± 5",23,11,25,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20113RJV","≤23","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20112RJV",2000,"DC",1.1000000000000001E-3,"± 5",18,7,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20112RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20103JV",2000,"DC",0.01,"± 5",23,10.5,19.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20103JV","≤23","≤11","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH20103HVB",2000,"DC",0.01,"± 3",23,10.5,24.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH20103HVB","≤23","≤11","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16912RHV",1600,"DC",9.1000000000000004E-3,"± 3",23,8,21,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16912RHV","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16912HVB",1600,"DC",9.1000000000000004E-3,"± 3",23,8,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16912HVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16822HV",1600,"DC",8.2000000000000007E-3,"± 3",23,7.5,16,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16822HV","≤23","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16682JVB",1600,"DC",6.7999999999999996E-3,"± 5",23,7,20.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16682JVB","≤23","≤ 7","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16682HV",1600,"DC",6.7999999999999996E-3,"± 3",23,7,15.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16682HV","≤23","≤ 7","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16563JVB",1600,"DC",5.6000000000000001E-2,"± 5",28,16,29.5,17.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16563JVB","≤28","≤16","≤29.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16562HVB",1600,"DC",5.5999999999999999E-3,"± 3",23,6.5,20,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16562HVB","≤23","≤ 7","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16562HV",1600,"DC",5.5999999999999999E-3,"± 3",23,6.5,15,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16562HV","≤23","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16512HVB",1600,"DC",5.1000000000000004E-3,"± 3",23,6.5,20,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16512HVB","≤23","≤ 7","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16473JV",1600,"DC",4.7E-2,"± 5",28,15,23.5,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16473JV","≤28","≤15","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16472HVB",1600,"DC",4.7000000000000002E-3,"± 3",23,6.5,19.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16472HVB","≤23","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16432JV",1600,"DC",4.3E-3,"± 5",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16432JV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16392RJV",1600,"DC",3.8999999999999998E-3,"± 5",18,7,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16392RJV","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16392JV",1600,"DC",3.8999999999999998E-3,"± 5",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16392JV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16362JVB",1600,"DC",3.5999999999999999E-3,"± 5",18,7,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16362JVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16333JVB",1600,"DC",3.3000000000000002E-2,"± 5",28,11.5,25.5,17.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16333JVB","≤28","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16332RHV",1600,"DC",3.3E-3,"± 3",18,7.5,19.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16332RHV","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16332HVB",1600,"DC",3.3E-3,"± 3",18,7.5,19.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16332HVB","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16302RHV",1600,"DC",3.0000000000000001E-3,"± 3",18,7.5,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16302RHV","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16272RJV",1600,"DC",2.7000000000000001E-3,"± 5",18,7,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16272RJV","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16243JV",1600,"DC",2.4E-2,"± 5",28,10,18.5,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16243JV","≤28","≤10","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16242RJV",1600,"DC",2.3999999999999998E-3,"± 5",18,7,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16242RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16223HV",1600,"DC",2.1999999999999999E-2,"± 3",28,9.5,18,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16223HV","≤28","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16222RJV",1600,"DC",2.2000000000000001E-3,"± 5",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16222RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16203RHV",1600,"DC",0.02,"± 3",23,11,25,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16203RHV","≤23","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16202JV",1600,"DC",2E-3,"± 5",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16202JV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16183RJV",1600,"DC",1.7999999999999999E-2,"± 5",23,10.5,24.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16183RJV","≤23","≤11","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16182JV",1600,"DC",1.8E-3,"± 5",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16182JV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16163HVB",1600,"DC",1.6E-2,"± 3",23,10,23.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16163HVB","≤23","≤10","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16162RHV",1600,"DC",1.6000000000000001E-3,"± 3",18,7,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16162RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16153HVB",1600,"DC",1.4999999999999999E-2,"± 3",23,9.5,23,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16153HVB","≤23","≤10","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16153HV",1600,"DC",1.4999999999999999E-2,"± 3",23,9.5,18,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16153HV","≤23","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16133JVB",1600,"DC",1.2999999999999999E-2,"± 5",23,9,22.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16133JVB","≤23","≤ 9","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16133HV",1600,"DC",1.2999999999999999E-2,"± 3",23,9,17.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16133HV","≤23","≤ 9","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16132HV",1600,"DC",1.2999999999999999E-3,"± 3",18,6.5,13,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16132HV","≤18","≤ 7","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16122JVB",1600,"DC",1.1999999999999999E-3,"± 5",18,7,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16122JVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16113JV",1600,"DC",1.0999999999999999E-2,"± 5",23,8.5,17,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16113JV","≤23","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16112RJV",1600,"DC",1.1000000000000001E-3,"± 5",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16112RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16103JV",1600,"DC",0.01,"± 5",23,8,16.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16103JV","≤23","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH16103HVB",1600,"DC",0.01,"± 3",23,8,21.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH16103HVB","≤23","≤ 8","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12913JV",1250,"DC",9.0999999999999998E-2,"± 5",28,14.5,23,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12913JV","≤28","≤15","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12912HVB",1250,"DC",9.1000000000000004E-3,"± 3",18,7.5,19.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12912HVB","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12823HV",1250,"DC",8.2000000000000003E-2,"± 3",28,14,22.5,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12823HV","≤28","≤14","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12822HV",1250,"DC",8.2000000000000007E-3,"± 3",18,7.5,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12822HV","≤18","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12752JVB",1250,"DC",7.4999999999999997E-3,"± 5",18,7,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12752JVB","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12752HV",1250,"DC",7.4999999999999997E-3,"± 3",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12752HV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12682JVB",1250,"DC",6.7999999999999996E-3,"± 5",18,7,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12682JVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12682HV",1250,"DC",6.7999999999999996E-3,"± 3",18,7,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12682HV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12622HVB",1250,"DC",6.1999999999999998E-3,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12622HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12562RHV",1250,"DC",5.5999999999999999E-3,"± 3",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12562RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12562HVB",1250,"DC",5.5999999999999999E-3,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12562HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12513HVB",1250,"DC",5.0999999999999997E-2,"± 3",23,12,26,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12513HVB","≤23","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12473RHV",1250,"DC",4.7E-2,"± 3",23,11.5,25.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12473RHV","≤23","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12473HVB",1250,"DC",4.7E-2,"± 3",23,11.5,25.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12473HVB","≤23","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12472HV",1250,"DC",4.7000000000000002E-3,"± 3",18,6,13,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12472HV","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12433JVB",1250,"DC",4.2999999999999997E-2,"± 5",23,11,25,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12433JVB","≤23","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12432HV",1250,"DC",4.3E-3,"± 3",18,6,13,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12432HV","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12392RJV",1250,"DC",3.8999999999999998E-3,"± 5",18,6,17.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12392RJV","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12392JV",1250,"DC",3.8999999999999998E-3,"± 5",18,6,12.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12392JV","≤18","≤ 6","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12362RJV",1250,"DC",3.5999999999999999E-3,"± 5",18,6,17.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12362RJV","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12362JVB",1250,"DC",3.5999999999999999E-3,"± 5",18,6,17.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12362JVB","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12333JV",1250,"DC",3.3000000000000002E-2,"± 5",23,10,18.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12333JV","≤23","≤10","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12332HVB",1250,"DC",3.3E-3,"± 3",18,7.5,19.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12332HVB","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12303RHV",1250,"DC",0.03,"± 3",23,9.5,23,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12303RHV",{"$f":"IF(L1548<=9.5,\"≤ \"&ROUNDUP(L1548*1,0)/1,\"≤\"&ROUNDUP(L1548*1,0)/1)","v":"≤23"},{"$f":"IF(M1548<=9,\"≤ \"&ROUNDUP(M1548*1,0)/1,\"≤\"&ROUNDUP(M1548*1,0)/1)","v":"≤10"},{"$f":"IF(N1548<=9.5,\"≤ \"&ROUNDUP(N1548*2,0)/2,\"≤\"&ROUNDUP(N1548*2,0)/2)","v":"≤23"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12302HVB",1250,"DC",3.0000000000000001E-3,"± 3",18,7.5,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12302HVB","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12273HV",1250,"DC",2.7E-2,"± 3",23,9,17.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12273HV","≤23","≤ 9","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12272JVB",1250,"DC",2.7000000000000001E-3,"± 5",18,7,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12272JVB","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12243JV",1250,"DC",2.4E-2,"± 5",23,8.5,17,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12243JV","≤23","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12223RJV",1250,"DC",2.1999999999999999E-2,"± 5",23,8.5,21.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12223RJV","≤23","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12223HVB",1250,"DC",2.1999999999999999E-2,"± 3",23,8.5,21.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12223HVB","≤23","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12222JV",1250,"DC",2.2000000000000001E-3,"± 5",18,6.5,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12222JV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12203RJV",1250,"DC",0.02,"± 5",23,8,21.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12203RJV","≤23","≤ 8","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12202JV",1250,"DC",2E-3,"± 5",18,7,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12202JV","≤18","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12183HVB",1250,"DC",1.7999999999999999E-2,"± 3",23,7.5,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12183HVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12182RHV",1250,"DC",1.8E-3,"± 3",18,7,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12182RHV","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12163JVB",1250,"DC",1.6E-2,"± 5",23,7.5,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12163JVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12162HV",1250,"DC",1.6000000000000001E-3,"± 3",18,7,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12162HV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12153JVB",1250,"DC",1.4999999999999999E-2,"± 5",18,9.5,21,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12153JVB","≤18","≤10","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12152JVB",1250,"DC",1.5E-3,"± 5",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12152JVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12152HV",1250,"DC",1.5E-3,"± 3",18,6.5,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12152HV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12132RJV",1250,"DC",1.2999999999999999E-3,"± 5",18,6.5,18,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12132RJV","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12123JV",1250,"DC",1.2E-2,"± 5",18,8.5,15.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12123JV","≤18","≤ 9","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12122RJV",1250,"DC",1.1999999999999999E-3,"± 5",18,7,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12122RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12113RHV",1250,"DC",1.0999999999999999E-2,"± 3",18,8.5,20,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12113RHV","≤18","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12112HVB",1250,"DC",1.1000000000000001E-3,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12112HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12104JV",1250,"DC",0.1,"± 5",28,15.5,24,25,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12104JV","≤28","≤16","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12103HVB",1250,"DC",0.01,"± 3",18,8,20,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12103HVB","≤18","≤ 8","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH12102RHV",1250,"DC",1E-3,"± 3",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH12102RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10913RHV",1000,"DC",9.0999999999999998E-2,"± 3",23,11.5,25.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10913RHV","≤23","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10912HVB",1000,"DC",9.1000000000000004E-3,"± 3",18,6,18,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10912HVB","≤18","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10823RHV",1000,"DC",8.2000000000000003E-2,"± 3",23,11,25,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10823RHV","≤23","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10822JVB",1000,"DC",8.2000000000000007E-3,"± 5",18,6,17.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10822JVB","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10753HV",1000,"DC",7.4999999999999997E-2,"± 3",23,10.5,19.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10753HV","≤23","≤11","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10752JVB",1000,"DC",7.4999999999999997E-3,"± 5",18,6,17.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10752JVB","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10683JV",1000,"DC",6.8000000000000005E-2,"± 5",23,10,19,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10683JV","≤23","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10682RJV",1000,"DC",6.7999999999999996E-3,"± 5",18,7,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10682RJV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10623HVB",1000,"DC",6.2E-2,"± 3",23,9.5,23,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10623HVB","≤23","≤10","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10622JV",1000,"DC",6.1999999999999998E-3,"± 5",18,6.5,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10622JV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10563RJV",1000,"DC",5.6000000000000001E-2,"± 5",23,9.5,22.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10563RJV","≤23","≤10","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10562RHV",1000,"DC",5.5999999999999999E-3,"± 3",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10562RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10513HVB",1000,"DC",5.0999999999999997E-2,"± 3",23,9,22.5,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10513HVB","≤23","≤ 9","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10513HV",1000,"DC",5.0999999999999997E-2,"± 3",23,9,17.5,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10513HV","≤23","≤ 9","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10473JVB",1000,"DC",4.7E-2,"± 5",23,8.5,22,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10473JVB","≤23","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10473HV",1000,"DC",4.7E-2,"± 3",23,8.5,17,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10473HV","≤23","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10433RJV",1000,"DC",4.2999999999999997E-2,"± 5",23,8.5,21.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10433RJV","≤23","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10432RHV",1000,"DC",4.3E-3,"± 3",18,6,18,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10432RHV","≤18","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10432HV",1000,"DC",4.3E-3,"± 3",18,6,13,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10432HV","≤18","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10392RJV",1000,"DC",3.8999999999999998E-3,"± 5",18,6,17.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10392RJV","≤18","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10363JV",1000,"DC",3.5999999999999997E-2,"± 5",23,7.5,16,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10363JV","≤23","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10363HVB",1000,"DC",3.5999999999999997E-2,"± 3",23,7.5,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10363HVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10333RHV",1000,"DC",3.3000000000000002E-2,"± 3",23,7.5,21,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10333RHV","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10333HVB",1000,"DC",3.3000000000000002E-2,"± 3",23,7.5,21,15,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10333HVB","≤23","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10332HV",1000,"DC",3.3E-3,"± 3",18,7.5,14.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10332HV","≤18","≤ 8","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10302JVB",1000,"DC",3.0000000000000001E-3,"± 5",18,7.5,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10302JVB","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10302HV",1000,"DC",3.0000000000000001E-3,"± 3",18,7.5,14,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10302HV","≤18","≤ 8","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10273HV",1000,"DC",2.7E-2,"± 3",18,9,16,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10273HV","≤18","≤ 9","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10243JVB",1000,"DC",2.4E-2,"± 5",18,8.5,20.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10243JVB","≤18","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10243JV",1000,"DC",2.4E-2,"± 5",18,8.5,15.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10243JV","≤18","≤ 9","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10223RJV",1000,"DC",2.1999999999999999E-2,"± 5",18,8.5,20,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10223RJV","≤18","≤ 9","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10223JV",1000,"DC",2.1999999999999999E-2,"± 5",18,8.5,15,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10223JV","≤18","≤ 9","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10222HVB",1000,"DC",2.2000000000000001E-3,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10222HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10202RHV",1000,"DC",2E-3,"± 3",18,7,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10202RHV","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10183JVB",1000,"DC",1.7999999999999999E-2,"± 5",18,7.5,19.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10183JVB","≤18","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10182RHV",1000,"DC",1.8E-3,"± 3",18,7,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10182RHV","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10163RHV",1000,"DC",1.6E-2,"± 3",18,7.5,19,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10163RHV","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10163JVB",1000,"DC",1.6E-2,"± 5",18,7.5,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10163JVB","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10162HV",1000,"DC",1.6000000000000001E-3,"± 3",18,7,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10162HV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10153JVB",1000,"DC",1.4999999999999999E-2,"± 5",18,7,19,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10153JVB","≤18","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10152JV",1000,"DC",1.5E-3,"± 5",18,6.5,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10152JV",{"$f":"IF(L1932<=9.5,\"≤ \"&ROUNDUP(L1932*1,0)/1,\"≤\"&ROUNDUP(L1932*1,0)/1)","v":"≤18"},{"$f":"IF(M1932<=9,\"≤ \"&ROUNDUP(M1932*1,0)/1,\"≤\"&ROUNDUP(M1932*1,0)/1)","v":"≤ 7"},{"$f":"IF(N1932<=9.5,\"≤ \"&ROUNDUP(N1932*2,0)/2,\"≤\"&ROUNDUP(N1932*2,0)/2)","v":"≤13.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10132RJV",1000,"DC",1.2999999999999999E-3,"± 5",18,6.5,18,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10132RJV","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10123RHV",1000,"DC",1.2E-2,"± 3",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10123RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10123HVB",1000,"DC",1.2E-2,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10123HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10122HVB",1000,"DC",1.1999999999999999E-3,"± 3",18,7,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10122HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10113RHV",1000,"DC",1.0999999999999999E-2,"± 3",18,6.5,18.5,7.5,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10113RHV","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10112HVB",1000,"DC",1.1000000000000001E-3,"± 3",18,6.5,18.5,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10112HVB","≤18","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10104HV",1000,"DC",0.1,"± 3",23,12,21,20,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10104HV","≤23","≤12","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10103JVB",1000,"DC",0.01,"± 5",18,6.5,18,10,"Inner crimped lead wire type (Style B)","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10103JVB","≤18","≤ 7","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWH(V)","ECWH10102HV",1000,"DC",1E-3,"± 3",18,6.5,13.5,15,"Straight lead wire type","-25 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWH10102HV","≤18","≤ 7","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG80685JA",800,"DC",6.8,"± 5",31.5,17.5,32.5,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG80685JA","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG80605J",800,"DC",6,"± 5",31.5,16,29.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG80605J","≤32","≤16","≤29.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG80395JA",800,"DC",3.9,"± 5",31.5,13.5,28.5,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG80395JA","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG80355JA",800,"DC",3.5,"± 5",31.5,13.5,28.5,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG80355JA","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG80275J",800,"DC",2.7,"± 5",31.5,12,24.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG80275J","≤32","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG70475JA",700,"DC",4.7,"± 5",31.5,17.5,32.5,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG70475JA","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG70395K",700,"DC",3.9,"±10",31.5,17.5,32.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG70395K","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG70225JA",700,"DC",2.2000000000000002,"± 5",31.5,12,24.5,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",250,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG70225JA","≤32","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG70155K",700,"DC",1.5,"±10",31.5,10.5,21,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG70155K","≤32","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG70105KA",700,"DC",1,"±10",31.5,9.5,18,27.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",350,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG70105KA","≤32","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60805J",600,"DC",8,"± 5",31.5,13.5,28.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60805J","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60755JA",600,"DC",7.5,"± 5",31.5,13.5,28.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60755JA","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60505JA",600,"DC",5,"± 5",31.5,12,24.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",250,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60505JA","≤32","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60405J",600,"DC",4,"± 5",31.5,10.5,21,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60405J","≤32","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60355JA",600,"DC",3.5,"± 5",31.5,9.5,18,27.5,"Short cut lead wire type","-40 to 110","Tray packing",350,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60355JA","≤32","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG60225J",600,"DC",2.2000000000000002,"± 5",31.5,8,17,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",400,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG60225J","≤32","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J475KA",630,"DC",4.7,"±10",31.5,17.5,32.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J475KA","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J475J",630,"DC",4.7,"± 5",31.5,17.5,32.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J475J","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J305JA",630,"DC",3,"± 5",31.5,13.5,28.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J305JA","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J225Q1",630,"DC",2.2000000000000002,"±10",27,15.5,24,22.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J225Q1","≤27","≤16","≤24",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J155PA",630,"DC",1.5,"± 5",27,12,21,22.5,"Short cut lead wire type","-40 to 110","Tray packing",300,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J155PA","≤27","≤12","≤21",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J105QA",630,"DC",1,"±10",27,10.5,19,22.5,"Short cut lead wire type","-40 to 110","Tray packing",350,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J105QA","≤27","≤11","≤19",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG2J105P1",630,"DC",1,"± 5",27,10.5,19,22.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",400,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG2J105P1","≤27","≤11","≤19",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG1B405JA",1100,"DC",4,"± 5",31.5,17.5,32.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",100,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG1B405JA","≤32","≤18","≤32.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG1B225J",1100,"DC",2.2000000000000002,"± 5",31.5,13.5,28.5,27.5,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",150,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG1B225J","≤32","≤14","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","Yes","ECWFG","ECWFG1B155JA",1100,"DC",1.5,"± 5",31.5,12,24.5,27.5,"Short cut lead wire type","-40 to 110","Tray packing",250,"https://industrial.panasonic.com/ww/products/pt/automotive-film-cap/models/ECWFG1B155JA","≤32","≤12","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W684J",450,"DC",0.68,"± 5",17.5,7,12.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W684J","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W475PD",450,"DC",4.7,"± 5",31,15.5,25.5,27.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W475PD","≤31","≤16","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W474P1",450,"DC",0.47,"± 5",13,7,12.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W474P1","≤13","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W335PD",450,"DC",3.3,"± 5",31,13,23,27.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W335PD","≤31","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W335K",450,"DC",3.3,"±10",26,10,17,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W335K","≤26","≤10","≤17",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W334P5",450,"DC",0.33,"± 5",17.5,5,10.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W334P5","≤18","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W225KA",450,"DC",2.2000000000000002,"±10",17.5,10,15.5,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W225KA","≤18","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W225J",450,"DC",2.2000000000000002,"± 5",17.5,10,15.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W225J","≤18","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W224JA",450,"DC",0.22,"± 5",13,6,12,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W224JA","≤13","≤ 6","≤12",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W155Q8",450,"DC",1.5,"±10",31,9,19,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W155Q8","≤31","≤ 9","≤19",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W154PD",450,"DC",0.15,"± 5",17.5,5,10.5,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W154PD","≤18","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W105K",450,"DC",1,"±10",17.5,7,12.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W105K","≤18","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W104QD",450,"DC",0.1,"±10",17.5,5,10.5,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104QD","≤18","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2W104K",450,"DC",0.1,"±10",13,5,10.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2W104K","≤13","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J474P5",630,"DC",0.47,"± 5",26,8,15,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J474P5","≤26","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J474JA",630,"DC",0.47,"± 5",17.5,10,15.5,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J474JA","≤18","≤10","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J334K",630,"DC",0.33,"±10",17.5,8.5,14.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J334K","≤18","≤ 9","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J225QD",630,"DC",2.2000000000000002,"±10",31,13,23,27.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J225QD","≤31","≤13","≤23",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J224Q5",630,"DC",0.22,"±10",26,6,13,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J224Q5",{"$f":"IF(L2252<=9.5,\"≤ \"&ROUNDUP(L2252*1,0)/1,\"≤\"&ROUNDUP(L2252*1,0)/1)","v":"≤26"},{"$f":"IF(M2252<=9,\"≤ \"&ROUNDUP(M2252*1,0)/1,\"≤\"&ROUNDUP(M2252*1,0)/1)","v":"≤ 6"},{"$f":"IF(N2252<=9.5,\"≤ \"&ROUNDUP(N2252*2,0)/2,\"≤\"&ROUNDUP(N2252*2,0)/2)","v":"≤13"},null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J155QD",630,"DC",1.5,"±10",31,11,21,27.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J155QD","≤31","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J155P5",630,"DC",1.5,"± 5",31,11,21,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J155P5","≤31","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J154PD",630,"DC",0.15,"± 5",26,6,13,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J154PD","≤26","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J105Q5",630,"DC",1,"±10",31,9,19,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J105Q5","≤31","≤ 9","≤19",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J105K",630,"DC",1,"±10",26,10,17,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J105K","≤26","≤10","≤17",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J104KA",630,"DC",0.1,"±10",17.5,5,10.5,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J104KA","≤18","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","box","PP","No","ECWFE","ECWFE2J104J",630,"DC",0.1,"± 5",17.5,5,10.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFE2J104J","≤18","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W824JC",450,"DC",0.82,"± 5",17.5,7.2,10.4,15,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W824JC","≤18","≤ 8","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W684Q1",450,"DC",0.68,"±10",12.6,7.7,12.4,10,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W684Q1","≤13","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W684PB",450,"DC",0.68,"± 5",12.6,7.7,17.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W684PB","≤13","≤ 8","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W684K4",450,"DC",0.68,"±10",17.5,6.7,14.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W684K4",{"$f":"IF(L2316<=9.5,\"≤ \"&ROUNDUP(L2316*1,0)/1,\"≤\"&ROUNDUP(L2316*1,0)/1)","v":"≤18"},{"$f":"IF(M2316<=9,\"≤ \"&ROUNDUP(M2316*1,0)/1,\"≤\"&ROUNDUP(M2316*1,0)/1)","v":"≤ 7"},{"$f":"IF(N2316<=9.5,\"≤ \"&ROUNDUP(N2316*2,0)/2,\"≤\"&ROUNDUP(N2316*2,0)/2)","v":"≤15"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W564KB",450,"DC",0.56000000000000005,"±10",17.5,6.2,14.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W564KB","≤18","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W564K",450,"DC",0.56000000000000005,"±10",17.5,6.2,9.4,15,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W564K","≤18","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W475KC",450,"DC",4.7,"±10",25.3,11.7,16.399999999999999,22.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W475KC","≤26","≤12","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W475JQ",450,"DC",4.7,"± 5",25.3,11.7,21.4,22.5,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W475JQ","≤26","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W474Q4",450,"DC",0.47,"±10",12.6,6.5,16.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W474Q4","≤13","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W474KQ",450,"DC",0.47,"±10",17.5,5.8,16,15,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W474KQ","≤18","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W474K4",450,"DC",0.47,"±10",17.5,5.8,14,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W474K4","≤18","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W395KQ",450,"DC",3.9,"±10",25.3,10.7,20.399999999999999,22.5,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W395KQ","≤26","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W394KB",450,"DC",0.39,"±10",12.6,6,15.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W394KB","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W394JQ",450,"DC",0.39,"± 5",12.6,6,15.7,10,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W394JQ","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W335KQ",450,"DC",3.3,"±10",25.3,9.8000000000000007,19.600000000000001,22.5,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W335KQ","≤26","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W335JC",450,"DC",3.3,"± 5",25.3,9.8000000000000007,14.6,22.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W335JC","≤26","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W334JQ",450,"DC",0.33,"± 5",12.6,5.6,15.4,10,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W334JQ","≤13","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W275JC",450,"DC",2.7,"± 5",25.3,9,13.7,22.5,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W275JC","≤26","≤ 9","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W274KQ",450,"DC",0.27,"±10",12.6,5.3,15,10,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W274KQ","≤13","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W274J3",450,"DC",0.27,"± 5",12.6,5.3,15,5,"Inner crimped lead wire type (Style B)","-40 to 110","12.7P crimped lead taping (ammo packing)",1300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W274J3","≤13","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W225J4",450,"DC",2.2000000000000002,"± 5",17.5,11.1,19.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W225J4","≤18","≤12","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W225J",450,"DC",2.2000000000000002,"± 5",17.5,11.1,14.3,15,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W225J","≤18","≤12","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W185KQ",450,"DC",1.8,"±10",17.5,10.1,20.3,15,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W185KQ","≤18","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W185JC",450,"DC",1.8,"± 5",17.5,10.1,13.3,15,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W185JC","≤18","≤11","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W185J",450,"DC",1.8,"± 5",17.5,10.1,13.3,15,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W185J","≤18","≤11","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W155KQ",450,"DC",1.5,"±10",17.5,9.3000000000000007,19.5,15,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W155KQ","≤18","≤10","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W155K4",450,"DC",1.5,"±10",17.5,9.3000000000000007,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W155K4","≤18","≤10","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W154KQ",450,"DC",0.15,"±10",12.6,4.5999999999999996,14.1,10,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W154KQ","≤13","≤ 5","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W125KC",450,"DC",1.2,"±10",17.5,8.5,11.6,15,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W125KC","≤18","≤ 9","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W125KB",450,"DC",1.2,"±10",17.5,8.5,16.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W125KB","≤18","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W124KB",450,"DC",0.12,"±10",12.6,4.5999999999999996,14,7.5,"Inner crimped lead wire type (Style B)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W124KB","≤13","≤ 5","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W124JQ",450,"DC",0.12,"± 5",12.6,4.5999999999999996,14,10,"Crimped lead wire type (Style D)","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W124JQ","≤13","≤ 5","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W105Q3",450,"DC",1,"±10",12.6,9.1999999999999993,18.899999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 110","12.7P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W105Q3","≤13","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W105P1",450,"DC",1,"± 5",12.6,9.1999999999999993,13.9,10,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W105P1","≤13","≤10","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W105JC",450,"DC",1,"± 5",17.5,7.8,11,15,"Short cut lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W105JC","≤18","≤ 8","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2W105J",450,"DC",1,"± 5",17.5,7.8,11,15,"Straight lead wire type","-40 to 110","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2W105J","≤18","≤ 8","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J824KQ",630,"DC",0.82,"±10",17.8,10.199999999999999,22.1,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J824KQ","≤18","≤11","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J824KC",630,"DC",0.82,"±10",17.8,10.199999999999999,15.1,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J824KC","≤18","≤11","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J823KQ",630,"DC",8.2000000000000003E-2,"±10",12.6,5.4,13.7,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J823KQ","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J823JQ",630,"DC",8.2000000000000003E-2,"± 5",12.6,5.4,13.7,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J823JQ","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J684K",630,"DC",0.68,"±10",17.8,9.3000000000000007,14.2,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J684K","≤18","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J684J",630,"DC",0.68,"± 5",17.8,9.3000000000000007,14.2,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J684J","≤18","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J564K4",630,"DC",0.56000000000000005,"±10",17.8,8.4,13.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J564K4","≤18","≤ 9","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J564JC",630,"DC",0.56000000000000005,"± 5",17.8,8.4,13.3,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J564JC","≤18","≤ 9","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J563J4",630,"DC",5.6000000000000001E-2,"± 5",12.6,4.7,8.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J563J4","≤13","≤ 5","≤ 8.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J475KQ",630,"DC",4.7,"±10",25.3,18.3,30.9,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J475KQ","≤26","≤19","≤31",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J474KC",630,"DC",0.47,"±10",17.8,7.8,12.7,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J474KC","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J474K",630,"DC",0.47,"±10",17.8,7.8,12.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J474K","≤18","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J473KB",630,"DC",4.7E-2,"±10",12.6,4.4000000000000004,12.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J473KB","≤13","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J395JQ",630,"DC",3.9,"± 5",25.3,16.600000000000001,29.1,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J395JQ","≤26","≤17","≤29.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J394KB",630,"DC",0.39,"±10",17.8,7.1,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J394KB","≤18","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J394JQ",630,"DC",0.39,"± 5",17.8,7.1,19,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J394JQ","≤18","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J335KQ",630,"DC",3.3,"±10",25.3,15.3,27.7,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J335KQ","≤26","≤16","≤28",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J335KC",630,"DC",3.3,"±10",25.3,15.3,20.7,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J335KC","≤26","≤16","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J334KB",630,"DC",0.33,"±10",17.8,6.6,16.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J334KB","≤18","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J334J",630,"DC",0.33,"± 5",17.8,6.6,11.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J334J","≤18","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J333JQ",630,"DC",3.3000000000000002E-2,"± 5",12.6,7.5,15.5,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J333JQ","≤13","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J275J",630,"DC",2.7,"± 5",25.3,13.8,19.2,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J275J",{"$f":"IF(L2636<=9.5,\"≤ \"&ROUNDUP(L2636*1,0)/1,\"≤\"&ROUNDUP(L2636*1,0)/1)","v":"≤26"},{"$f":"IF(M2636<=9,\"≤ \"&ROUNDUP(M2636*1,0)/1,\"≤\"&ROUNDUP(M2636*1,0)/1)","v":"≤14"},{"$f":"IF(N2636<=9.5,\"≤ \"&ROUNDUP(N2636*2,0)/2,\"≤\"&ROUNDUP(N2636*2,0)/2)","v":"≤19.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J274JC",630,"DC",0.27,"± 5",17.8,6,11,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J274JC","≤18","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J274J",630,"DC",0.27,"± 5",17.8,6,11,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J274J","≤18","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J225K",630,"DC",2.2000000000000002,"±10",25.3,12.4,17.7,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J225K","≤26","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J225JQ",630,"DC",2.2000000000000002,"± 5",25.3,12.4,24.7,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J225JQ","≤26","≤13","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J224J4",630,"DC",0.22,"± 5",12.6,8.1,11.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J224J4","≤13","≤ 9","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J185KB",630,"DC",1.8,"±10",25.3,11.2,21.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J185KB","≤26","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J185JC",630,"DC",1.8,"± 5",25.3,11.2,16.5,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J185JC","≤26","≤12","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J183KQ",630,"DC",1.7999999999999999E-2,"±10",12.6,5.9,14,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J183KQ","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J155K",630,"DC",1.5,"±10",25.3,10.3,15.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J155K","≤26","≤11","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J155JB",630,"DC",1.5,"± 5",25.3,10.3,20.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J155JB","≤26","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J154JQ",630,"DC",0.15,"± 5",12.6,6.8,15.2,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J154JQ","≤13","≤ 7","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J153KB",630,"DC",1.4999999999999999E-2,"±10",12.6,5.6,13.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J153KB","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J125JB",630,"DC",1.2,"± 5",25.3,9.1999999999999993,19.3,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J125JB","≤26","≤10","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J124J4",630,"DC",0.12,"± 5",12.6,6.2,9.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J124J4","≤13","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J123JQ",630,"DC",1.2E-2,"± 5",12.6,5.2,13.2,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J123JQ","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J105PB",630,"DC",1,"± 5",17.8,11.2,21.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J105PB","≤18","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J105JQ",630,"DC",1,"± 5",25.3,8.4,20.5,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J105JQ","≤26","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J105J",630,"DC",1,"± 5",25.3,8.4,13.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J105J","≤26","≤ 9","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWFD","ECWFD2J103KQ",630,"DC",0.01,"±10",12.6,4.9000000000000004,13,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFD2J103KQ","≤13","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J824J",630,"DC",0.82,"± 5",26,10.1,15.3,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J824J","≤26","≤11","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J684J4",630,"DC",0.68,"± 5",18.2,12,22.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J684J4","≤19","≤12","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J474JQ",630,"DC",0.47,"± 5",18.2,10,20.100000000000001,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J474JQ","≤19","≤10","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J474J4",630,"DC",0.47,"± 5",18.2,10,20.100000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J474J4","≤19","≤10","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J334JB",630,"DC",0.33,"± 5",18.2,8.5,18.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J334JB","≤19","≤ 9","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J274J",630,"DC",0.27,"± 5",18.2,7.8,12.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J274J","≤19","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J225JB",630,"DC",2.2000000000000002,"± 5",26,16.3,26.4,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J225JB","≤26","≤17","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J185JQ",630,"DC",1.8,"± 5",26,14.8,24.8,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J185JQ","≤26","≤15","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J185J",630,"DC",1.8,"± 5",26,14.8,19.8,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J185J","≤26","≤15","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J155JB",630,"DC",1.5,"± 5",26,13.5,23.6,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J155JB","≤26","≤14","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J125JQ",630,"DC",1.2,"± 5",26,12.1,22.2,22.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J125JQ","≤26","≤13","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J125J",630,"DC",1.2,"± 5",26,12.1,17.2,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J125J","≤26","≤13","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWFA2J105JC",630,"DC",1,"± 5",26,11.1,16.2,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWFA2J105JC","≤26","≤12","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6914JL",630,"DC",0.91,"± 5",28,14.6,21.2,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6914JL","≤28","≤15","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6913RJL",630,"DC",9.0999999999999998E-2,"± 5",15.5,8.3000000000000007,17.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6913RJL","≤16","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6824JL",630,"DC",0.82,"± 5",28,13.9,20.5,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6824JL","≤28","≤14","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6823RJL",630,"DC",8.2000000000000003E-2,"± 5",15.5,8,17.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6823RJL","≤16","≤ 8","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6754HL",630,"DC",0.75,"± 3",28,13.3,19.899999999999999,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6754HL","≤28","≤14","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6753JL",630,"DC",7.4999999999999997E-2,"± 5",15.5,7.7,12.1,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6753JL","≤16","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6684HLB",630,"DC",0.68,"± 3",28,12.7,24.3,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6684HLB","≤28","≤13","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6683HL",630,"DC",6.8000000000000005E-2,"± 3",15.5,7.4,11.8,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6683HL","≤16","≤ 8","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6623HLB",630,"DC",6.2E-2,"± 3",15.5,7.1,16.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6623HLB","≤16","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6564JL",630,"DC",0.56000000000000005,"± 5",28,11.6,17.8,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6564JL","≤28","≤12","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6563HLB",630,"DC",5.6000000000000001E-2,"± 3",15.5,6.8,16.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6563HLB","≤16","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6514JL",630,"DC",0.51,"± 5",28,11.1,17.3,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6514JL","≤28","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6474JLB",630,"DC",0.47,"± 5",20.5,13.5,25.1,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6474JLB","≤21","≤14","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6473JL",630,"DC",4.7E-2,"± 5",15.5,6.4,10.8,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6473JL","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6434JL",630,"DC",0.43,"± 5",20.5,13,19.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6434JL","≤21","≤13","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6433RJL",630,"DC",4.2999999999999997E-2,"± 5",13,7.9,15.7,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6433RJL","≤13","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6394JL",630,"DC",0.39,"± 5",20.5,12.4,19,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6394JL","≤21","≤13","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6393RJL",630,"DC",3.9E-2,"± 5",13,7.6,15.4,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6393RJL","≤13","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6364RHL",630,"DC",0.36,"± 3",20.5,11.9,23.5,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6364RHL","≤21","≤12","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6364HLB",630,"DC",0.36,"± 3",20.5,11.9,23.5,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6364HLB","≤21","≤12","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6363HL",630,"DC",3.5999999999999997E-2,"± 3",13,7.3,10.199999999999999,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6363HL","≤13","≤ 8","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6333JLB",630,"DC",3.3000000000000002E-2,"± 5",13,7.1,15,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6333JLB","≤13","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6333HL",630,"DC",3.3000000000000002E-2,"± 3",13,7.1,10,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6333HL","≤13","≤ 8","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6303RHL",630,"DC",0.03,"± 3",13,6.9,14.7,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6303RHL","≤13","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6274JLB",630,"DC",0.27,"± 5",20.5,10.4,21.7,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6274JLB","≤21","≤11","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6274HL",630,"DC",0.27,"± 3",20.5,10.4,16.7,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6274HL","≤21","≤11","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6244RJL",630,"DC",0.24,"± 5",18,11.2,20.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6244RJL","≤18","≤12","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6244JL",630,"DC",0.24,"± 5",18,11.2,15.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6244JL","≤18","≤12","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6243HLB",630,"DC",2.4E-2,"± 3",12.5,6.4,14.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6243HLB","≤13","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6223RHL",630,"DC",2.1999999999999999E-2,"± 3",12.5,6.2,14,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6223RHL","≤13","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6223HLB",630,"DC",2.1999999999999999E-2,"± 3",12.5,6.2,14,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6223HLB","≤13","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6204HL",630,"DC",0.2,"± 3",18,10.3,14.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6204HL","≤18","≤11","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6203HLB",630,"DC",0.02,"± 3",12.5,6.5,14.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6203HLB","≤13","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6184JLB",630,"DC",0.18,"± 5",18,9.8000000000000007,19.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6184JLB",{"$f":"IF(L3020<=9.5,\"≤ \"&ROUNDUP(L3020*1,0)/1,\"≤\"&ROUNDUP(L3020*1,0)/1)","v":"≤18"},{"$f":"IF(M3020<=9,\"≤ \"&ROUNDUP(M3020*1,0)/1,\"≤\"&ROUNDUP(M3020*1,0)/1)","v":"≤10"},{"$f":"IF(N3020<=9.5,\"≤ \"&ROUNDUP(N3020*2,0)/2,\"≤\"&ROUNDUP(N3020*2,0)/2)","v":"≤19.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6183HL",630,"DC",1.7999999999999999E-2,"± 3",12.5,6.2,9.1,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6183HL","≤13","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6164JLB",630,"DC",0.16,"± 5",18,9.3000000000000007,18.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6164JLB","≤18","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6163JL",630,"DC",1.6E-2,"± 5",12.5,6,8.9,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6163JL","≤13","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6153RJL",630,"DC",1.4999999999999999E-2,"± 5",12.5,5.9,13.7,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6153RJL","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6153JL",630,"DC",1.4999999999999999E-2,"± 5",12.5,5.9,8.6999999999999993,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6153JL","≤13","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6134RJL",630,"DC",0.13,"± 5",18,8.5,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6134RJL","≤18","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6133JL",630,"DC",1.2999999999999999E-2,"± 5",12.5,5.6,8.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6133JL","≤13","≤ 6","≤ 8.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6133HLB",630,"DC",1.2999999999999999E-2,"± 3",12.5,5.6,13.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6133HLB","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6124JLB",630,"DC",0.12,"± 5",18,8.3000000000000007,17.7,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6124JLB","≤18","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6124HL",630,"DC",0.12,"± 3",18,8.3000000000000007,12.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6124HL","≤18","≤ 9","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6115JLB",630,"DC",1.1000000000000001,"± 5",28,16.3,28,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6115JLB","≤28","≤17","≤28",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6114HL",630,"DC",0.11,"± 3",18,8,12.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6114HL","≤18","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6113JLB",630,"DC",1.0999999999999999E-2,"± 5",12.5,5.4,13.2,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6113JLB","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6105HL",630,"DC",1,"± 3",28,15.5,22.3,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6105HL","≤28","≤16","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6103JLB",630,"DC",0.01,"± 5",12.5,5.2,13,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6103JLB","≤13","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF6103JL",630,"DC",0.01,"± 5",12.5,5.2,8,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF6103JL","≤13","≤ 6","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4913RJL",400,"DC",9.0999999999999998E-2,"± 5",13,7.8,15.7,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4913RJL","≤13","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4913JLB",400,"DC",9.0999999999999998E-2,"± 5",13,7.8,15.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4913JLB","≤13","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4824JL",400,"DC",0.82,"± 5",23,11.8,18.5,20,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4824JL","≤23","≤12","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4754RJL",400,"DC",0.75,"± 5",20.5,12.3,24.1,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4754RJL","≤21","≤13","≤24.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4753RHL",400,"DC",7.4999999999999997E-2,"± 3",13,7.3,15.1,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4753RHL","≤13","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4753HLB",400,"DC",7.4999999999999997E-2,"± 3",13,7.3,15.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4753HLB","≤13","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4683RHL",400,"DC",6.8000000000000005E-2,"± 3",13,7,14.9,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4683RHL","≤13","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4683JLB",400,"DC",6.8000000000000005E-2,"± 5",13,7,14.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4683JLB","≤13","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4624HL",400,"DC",0.62,"± 3",20.5,11.3,17.899999999999999,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4624HL","≤21","≤12","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4623JL",400,"DC",6.2E-2,"± 5",13,6.8,9.6,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4623JL","≤13","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4564JLB",400,"DC",0.56000000000000005,"± 5",20.5,10.7,22.3,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4564JLB","≤21","≤11","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4563HL",400,"DC",5.6000000000000001E-2,"± 3",12.5,6.6,9.4,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4563HL","≤13","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4513RJL",400,"DC",5.0999999999999997E-2,"± 5",12.5,6.4,14.2,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4513RJL","≤13","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4513JL",400,"DC",5.0999999999999997E-2,"± 5",12.5,6.4,9.1999999999999993,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4513JL","≤13","≤ 7","≤ 9.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4473RJL",400,"DC",4.7E-2,"± 5",12.5,6.2,14,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4473RJL","≤13","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4473RHL",400,"DC",4.7E-2,"± 3",12.5,6.2,14,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4473RHL","≤13","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4434HLB",400,"DC",0.43,"± 3",18,10.7,20.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4434HLB","≤18","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4433HL",400,"DC",4.2999999999999997E-2,"± 3",12.5,6,8.8000000000000007,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4433HL","≤13","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4394RHL",400,"DC",0.39,"± 3",18,10.3,20.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4394RHL","≤18","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4393HLB",400,"DC",3.9E-2,"± 3",12.5,5.8,13.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4393HLB","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4364HL",400,"DC",0.36,"± 3",18,9.9,14.7,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4364HL","≤18","≤10","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4363JLB",400,"DC",3.5999999999999997E-2,"± 5",12.5,5.7,13.4,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4363JLB","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4334HL",400,"DC",0.33,"± 3",18,9.6,14.3,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4334HL","≤18","≤10","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4333RJL",400,"DC",3.3000000000000002E-2,"± 5",12.5,6.7,14.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4333RJL","≤13","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4304JL",400,"DC",0.3,"± 5",18,9.1999999999999993,13.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4304JL","≤18","≤10","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4303HLB",400,"DC",0.03,"± 3",12.5,6.4,14.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4303HLB","≤13","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4274RHL",400,"DC",0.27,"± 3",18,8.8000000000000007,18.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4274RHL","≤18","≤ 9","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4273JL",400,"DC",2.7E-2,"± 5",12.5,6.2,9,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4273JL","≤13","≤ 7","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4244RJL",400,"DC",0.24,"± 5",18,8.3000000000000007,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4244RJL","≤18","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4244JL",400,"DC",0.24,"± 5",18,8.3000000000000007,13,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4244JL","≤18","≤ 9","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4225JLB",400,"DC",2.2000000000000002,"± 5",28,16.8,29,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4225JLB","≤28","≤17","≤29",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4225JL",400,"DC",2.2000000000000002,"± 5",28,16.8,24,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4225JL","≤28","≤17","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4223RJL",400,"DC",2.1999999999999999E-2,"± 5",12.5,5.8,13.6,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4223RJL","≤13","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4205JL",400,"DC",2,"± 5",28,16,23.1,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4205JL","≤28","≤16","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4204RJL",400,"DC",0.2,"± 5",15.5,8.6,18.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4204RJL","≤16","≤ 9","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4185HL",400,"DC",1.8,"± 3",28,15.2,22.2,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4185HL","≤28","≤16","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4184JL",400,"DC",0.18,"± 5",15.5,8.1999999999999993,12.8,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4184JL","≤16","≤ 9","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4165HLB",400,"DC",1.6,"± 3",28,14.2,26.2,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4165HLB",{"$f":"IF(L3340<=9.5,\"≤ \"&ROUNDUP(L3340*1,0)/1,\"≤\"&ROUNDUP(L3340*1,0)/1)","v":"≤28"},{"$f":"IF(M3340<=9,\"≤ \"&ROUNDUP(M3340*1,0)/1,\"≤\"&ROUNDUP(M3340*1,0)/1)","v":"≤15"},{"$f":"IF(N3340<=9.5,\"≤ \"&ROUNDUP(N3340*2,0)/2,\"≤\"&ROUNDUP(N3340*2,0)/2)","v":"≤26.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4164HL",400,"DC",0.16,"± 3",15.5,7.8,12.4,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4164HL","≤16","≤ 8","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4155HLB",400,"DC",1.5,"± 3",28,13.7,25.7,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4155HLB","≤28","≤14","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4135JL",400,"DC",1.3,"± 5",28,12.8,19.600000000000001,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4135JL","≤28","≤13","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4134HLB",400,"DC",0.13,"± 3",15.5,7.2,16.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4134HLB","≤16","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4125JL",400,"DC",1.2,"± 5",28,12.3,19.100000000000001,25,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4125JL","≤28","≤13","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4115JLB",400,"DC",1.1000000000000001,"± 5",23,13.6,25.5,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4115JLB","≤23","≤14","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4114JL",400,"DC",0.11,"± 5",15.5,6.8,11.3,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4114JL","≤16","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4114HLB",400,"DC",0.11,"± 3",15.5,6.8,16.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4114HLB","≤16","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4104RJL",400,"DC",0.1,"± 5",15.5,6.5,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4104RJL","≤16","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(L)","ECWF4104JL",400,"DC",0.1,"± 5",15.5,6.5,11,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF4104JL","≤16","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W824JAB",450,"DC",0.82,"± 5",18.100000000000001,8.1999999999999993,17.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W824JAB","≤19","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W684JAQ",450,"DC",0.68,"± 5",18.100000000000001,7.5,19.100000000000001,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W684JAQ","≤19","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W564RKA",450,"DC",0.56000000000000005,"±10",18.100000000000001,7,16.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W564RKA","≤19","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W475KAB",450,"DC",4.7,"±10",26.3,13.8,24.6,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W475KAB","≤27","≤14","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W474KAQ",450,"DC",0.47,"±10",13,8.6999999999999993,17.899999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W474KAQ","≤13","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W474JAB",450,"DC",0.47,"± 5",13,8.6999999999999993,17.899999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W474JAB","≤13","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W394RJA",450,"DC",0.39,"± 5",13,8.1,17.2,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W394RJA","≤13","≤ 9","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W394KAQ",450,"DC",0.39,"±10",13,8.1,17.2,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W394KAQ","≤13","≤ 9","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W335JA",450,"DC",3.3,"± 5",26.3,11.7,17.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W335JA","≤27","≤12","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W275KAQ",450,"DC",2.7,"±10",26.3,10.6,23.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W275KAQ","≤27","≤11","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W275JAQ",450,"DC",2.7,"± 5",26.3,10.6,23.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W275JAQ","≤27","≤11","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W274JAQ",450,"DC",0.27,"± 5",13,7,16.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W274JAQ","≤13","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W225JA",450,"DC",2.2000000000000002,"± 5",18.8,12.8,17.899999999999999,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W225JA","≤19","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W224KAQ",450,"DC",0.22,"±10",13,6.5,15.6,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W224KAQ","≤13","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W185KAB",450,"DC",1.8,"±10",18.8,11.6,21.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W185KAB","≤19","≤12","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W184RKA",450,"DC",0.18,"±10",13,6.1,15.2,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W184RKA","≤13","≤ 7","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W155RKA",450,"DC",1.5,"±10",18.8,10.7,20.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W155RKA","≤19","≤11","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W155JA",450,"DC",1.5,"± 5",18.8,10.7,15.8,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W155JA","≤19","≤11","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W154KAQ",450,"DC",0.15,"±10",13,5.7,14.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W154KAQ","≤13","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W125KAB",450,"DC",1.2,"±10",18.8,9.6999999999999993,19.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W125KAB","≤19","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W124JAQ",450,"DC",0.12,"± 5",13,5.4,14.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W124JAQ","≤13","≤ 6","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W105RJA",450,"DC",1,"± 5",18.100000000000001,9.3000000000000007,17.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W105RJA","≤19","≤10","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W105JA",450,"DC",1,"± 5",18.100000000000001,9.3000000000000007,12.6,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W105JA","≤19","≤10","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2W104KAQ",450,"DC",0.1,"±10",13,5.0999999999999996,14.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2W104KAQ","≤13","≤ 6","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2824JAB",250,"DC",0.82,"± 5",18.100000000000001,8,17.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2824JAB","≤19","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2685HA",250,"DC",6.8,"± 3",23.8,17.8,23.5,20,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2685HA","≤24","≤18","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2684JAQ",250,"DC",0.68,"± 5",18.100000000000001,7.4,19,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2684JAQ","≤19","≤ 8","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2565HAQ",250,"DC",5.6,"± 3",23.8,16.2,28.9,20,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2565HAQ","≤24","≤17","≤29",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2475JAQ",250,"DC",4.7,"± 5",23.8,14.8,27.6,20,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2475JAQ","≤24","≤15","≤28",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2475HAQ",250,"DC",4.7,"± 3",23.8,14.8,27.6,20,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2475HAQ","≤24","≤15","≤28",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2474HAQ",250,"DC",0.47,"± 3",13,8.4,17.600000000000001,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2474HAQ","≤13","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2395JAQ",250,"DC",3.9,"± 5",23.8,13.5,26.3,20,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2395JAQ","≤24","≤14","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2394RHA",250,"DC",0.39,"± 3",13,7.8,16.899999999999999,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2394RHA","≤13","≤ 8","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2335JA",250,"DC",3.3,"± 5",23.8,12.5,18.3,20,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2335JA","≤24","≤13","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2335HAB",250,"DC",3.3,"± 3",23.8,12.5,23.3,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2335HAB","≤24","≤13","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2334HAB",250,"DC",0.33,"± 3",13,7.3,16.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2334HAB","≤13","≤ 8","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2274RJA",250,"DC",0.27,"± 5",13,6.8,15.9,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2274RJA","≤13","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2274JAB",250,"DC",0.27,"± 5",13,6.8,15.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2274JAB","≤13","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2225JA",250,"DC",2.2000000000000002,"± 5",18.8,12.6,17.600000000000001,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2225JA","≤19","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2225HA",250,"DC",2.2000000000000002,"± 3",18.8,12.6,17.600000000000001,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2225HA","≤19","≤13","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2185RJA",250,"DC",1.8,"± 5",18.8,11.4,21.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2185RJA","≤19","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2184RHA",250,"DC",0.18,"± 3",13,5.9,15.1,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2184RHA","≤13","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2184HAB",250,"DC",0.18,"± 3",13,5.9,15.1,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2184HAB","≤13","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2155JA",250,"DC",1.5,"± 5",18.8,10.5,15.6,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2155JA","≤19","≤11","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2154HAB",250,"DC",0.15,"± 3",13,5.6,14.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2154HAB","≤13","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2125RJA",250,"DC",1.2,"± 5",18.8,9.5,19.600000000000001,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2125RJA","≤19","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2124RHA",250,"DC",0.12,"± 3",13,5.3,14.4,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2124RHA","≤13","≤ 6","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2124HAQ",250,"DC",0.12,"± 3",13,5.3,14.4,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2124HAQ","≤13","≤ 6","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PP","No","ECWF(A)","ECWF2105HAQ",250,"DC",1,"± 3",18.100000000000001,8.5,20.3,15,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECWF2105HAQ","≤19","≤ 9","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6824KTB",630,"DC",0.82,"±10",31.5,11.3,25.5,22.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6824KTB",{"$f":"IF(L3696<=9.5,\"≤ \"&ROUNDUP(L3696*1,0)/1,\"≤\"&ROUNDUP(L3696*1,0)/1)","v":"≤32"},{"$f":"IF(M3696<=9,\"≤ \"&ROUNDUP(M3696*1,0)/1,\"≤\"&ROUNDUP(M3696*1,0)/1)","v":"≤12"},{"$f":"IF(N3696<=9.5,\"≤ \"&ROUNDUP(N3696*2,0)/2,\"≤\"&ROUNDUP(N3696*2,0)/2)","v":"≤25.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6824KFB",630,"DC",0.82,"±10",31,11.3,25.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6824KFB","≤31","≤12","≤25.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6824JF",630,"DC",0.82,"± 5",31,11.3,20.5,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6824JF","≤31","≤12","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6823KFB",630,"DC",8.2000000000000003E-2,"±10",18.5,6.5,17,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6823KFB","≤19","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6823KF3",630,"DC",8.2000000000000003E-2,"±10",18.5,6.5,17,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6823KF3","≤19","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6822RKF",630,"DC",5.5999999999999999E-3,"±10",12,4.5,15,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6822RKF","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6822KFB",630,"DC",8.2000000000000007E-3,"±10",12,4.5,15,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6822KFB","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6684KTB",630,"DC",0.68,"±10",26.5,11.5,26,15,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6684KTB","≤27","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6684JF",630,"DC",0.68,"± 5",26,11.5,21,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6684JF","≤26","≤12","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6683RJT",630,"DC",6.8000000000000005E-2,"± 5",19,5.8,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6683RJT","≤19","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6683KF3",630,"DC",6.8000000000000005E-2,"±10",18.5,5.8,16,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6683KF3","≤19","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6683JF",630,"DC",6.8000000000000005E-2,"± 5",18.5,5.8,11,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6683JF","≤19","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6682RKF",630,"DC",4.7000000000000002E-3,"±10",12,4.5,15,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6682RKF","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6682JF",630,"DC",6.7999999999999996E-3,"± 5",12,4.9000000000000004,10,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6682JF","≤12","≤ 5","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6564KFW",630,"DC",0.56000000000000005,"±10",26,10,25,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6564KFW","≤26","≤10","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6564JF",630,"DC",0.56000000000000005,"± 5",26,10,20,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6564JF","≤26","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6563KFB",630,"DC",5.6000000000000001E-2,"±10",18.5,5.4,15.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6563KFB","≤19","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6563JFB",630,"DC",5.6000000000000001E-2,"± 5",18.5,5.4,15.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6563JFB","≤19","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6562RKF",630,"DC",3.8999999999999998E-3,"±10",10,4.5,15,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6562RKF","≤10","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6562JF",630,"DC",5.5999999999999999E-3,"± 5",12,4.5,10,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6562JF","≤12","≤ 5","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6474KFB",630,"DC",0.47,"±10",26,9.3000000000000007,23.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6474KFB","≤26","≤10","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6474JFB",630,"DC",0.47,"± 5",26,9.3000000000000007,23.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6474JFB","≤26","≤10","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6473RKF",630,"DC",4.7E-2,"±10",12,6.5,18.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6473RKF","≤12","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6473KFB",630,"DC",4.7E-2,"±10",12,6.5,18.5,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6473KFB","≤12","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6473JF9",630,"DC",4.7E-2,"± 5",12,6.5,18.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6473JF9","≤12","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6394KF",630,"DC",0.39,"±10",26,8.5,17.899999999999999,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6394KF","≤26","≤ 9","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6394JFW",630,"DC",0.39,"± 5",26,8.5,22.9,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6394JFW","≤26","≤ 9","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6393KT",630,"DC",3.9E-2,"±10",12.5,6,13.4,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6393KT","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6393KFW",630,"DC",3.9E-2,"±10",12,6,18.399999999999999,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6393KFW","≤12","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6393JT",630,"DC",3.9E-2,"± 5",12.5,6,13.4,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6393JT","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6334KFW",630,"DC",0.33,"±10",26,7.8,22,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6334KFW","≤26","≤ 8","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6334JTB",630,"DC",0.33,"± 5",26.5,7.8,22,15,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6334JTB","≤27","≤ 8","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6333KTB",630,"DC",3.3000000000000002E-2,"±10",12.5,6,16.899999999999999,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6333KTB","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6333KF",630,"DC",3.3000000000000002E-2,"±10",12,6,11.9,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6333KF","≤12","≤ 6","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6333JT",630,"DC",3.3000000000000002E-2,"± 5",12.5,6,11.9,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6333JT","≤13","≤ 6","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6274KFB",630,"DC",0.27,"±10",26,7,21.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6274KFB","≤26","≤ 7","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6274KF",630,"DC",0.27,"±10",26,7,16.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6274KF","≤26","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6273RJF",630,"DC",2.7E-2,"± 5",12,5.5,15.9,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6273RJF","≤12","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6273KT",630,"DC",2.7E-2,"±10",12.5,5.5,10.9,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6273KT","≤13","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6273JTB",630,"DC",2.7E-2,"± 5",12.5,5.5,15.9,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6273JTB","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6225KT",630,"DC",2.2000000000000002,"±10",31.5,19.5,29,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6225KT","≤32","≤20","≤29",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6225JFB",630,"DC",2.2000000000000002,"± 5",31,19.5,34,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6225JFB","≤31","≤20","≤34",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6224RKF",630,"DC",0.22,"±10",18.5,9,21.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6224RKF","≤19","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6224KF",630,"DC",0.22,"±10",18.5,9,16.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6224KF","≤19","≤ 9","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6224JTB",630,"DC",0.22,"± 5",19,9,21.5,10,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6224JTB","≤19","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6223RJT",630,"DC",2.1999999999999999E-2,"± 5",12.5,5.3,15.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6223RJT","≤13","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6223KF9",630,"DC",2.1999999999999999E-2,"±10",12,5.3,15.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6223KF9","≤12","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6223JT",630,"DC",2.1999999999999999E-2,"± 5",12.5,5.3,10.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6223JT","≤13","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6185KTB",630,"DC",1.8,"±10",31.5,16.8,32,22.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6185KTB","≤32","≤17","≤32",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6185JFW",630,"DC",1.8,"± 5",31,16.8,32,22.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6185JFW","≤31","≤17","≤32",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6184RKT",630,"DC",0.18,"±10",19,8,21,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6184RKT","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6184KFW",630,"DC",0.18,"±10",18.5,8,21,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6184KFW","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6184KF",630,"DC",0.18,"±10",18.5,8,16,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6184KF","≤19","≤ 8","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6183RKF",630,"DC",1.7999999999999999E-2,"±10",12,4.9000000000000004,15,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6183RKF","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6183KFB",630,"DC",1.7999999999999999E-2,"±10",12,4.9000000000000004,15,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6183KFB","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6183KF",630,"DC",1.7999999999999999E-2,"±10",12,4.9000000000000004,10,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6183KF","≤12","≤ 5","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6183JF9",630,"DC",1.7999999999999999E-2,"± 5",12,4.9000000000000004,15,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6183JF9","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6155JT",630,"DC",1.5,"± 5",31.5,15.3,24.7,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6155JT","≤32","≤16","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6155JF",630,"DC",1.5,"± 5",31,15.3,24.7,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6155JF","≤31","≤16","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6154KT",630,"DC",0.15,"±10",19,7.5,15.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6154KT","≤19","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6154KF3",630,"DC",0.15,"±10",18.5,7.5,20.399999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6154KF3","≤19","≤ 8","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6153RKT",630,"DC",1.4999999999999999E-2,"±10",12.5,5,13.2,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6153RKT","≤13","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6153KFW",630,"DC",1.4999999999999999E-2,"±10",12,5,13.2,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6153KFW","≤12","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6153KF3",630,"DC",1.4999999999999999E-2,"±10",12,5,13.2,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6153KF3","≤12","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6153JF9",630,"DC",1.4999999999999999E-2,"± 5",12,5,13.2,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6153JF9","≤12","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6125KT",630,"DC",1.2,"±10",31.5,13.5,23,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6125KT","≤32","≤14","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6125JFB",630,"DC",1.2,"± 5",31,13.5,28,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6125JFB","≤31","≤14","≤28",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6124KT3",630,"DC",0.12,"±10",19,6.3,19.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6124KT3","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6124KFB",630,"DC",0.12,"±10",18.5,6.3,19.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6124KFB","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6124JF",630,"DC",0.12,"± 5",18.5,6.3,14.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6124JF","≤19","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6123KT",630,"DC",1.2E-2,"±10",12.5,4.5,7.8,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6123KT","≤13","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6123KF9",630,"DC",1.2E-2,"±10",12,4.5,12.8,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6123KF9","≤12","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6123JFB",630,"DC",1.2E-2,"± 5",12,4.5,12.8,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6123JFB","≤12","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6105JTB",630,"DC",1,"± 5",31.5,12.5,26.9,22.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6105JTB","≤32","≤13","≤27",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6105JF",630,"DC",1,"± 5",31,12.5,21.9,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6105JF","≤31","≤13","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6104KTB",630,"DC",0.1,"±10",19,6.3,19,10,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6104KTB","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6104KFW",630,"DC",0.1,"±10",18.5,6.3,19,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6104KFW","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6104JF3",630,"DC",0.1,"± 5",18.5,6.3,19,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6104JF3","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE6103KT3",630,"DC",0.01,"±10",12.5,4.5,12.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6103KT3","≤13","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6103KFB",630,"DC",0.01,"±10",12,4.5,12.5,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6103KFB","≤12","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE6103JFW",630,"DC",0.01,"± 5",12,4.5,12.5,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE6103JFW","≤12","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4824KF",400,"DC",0.82,"±10",26,7.9,17.3,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4824KF","≤26","≤ 8","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4824JFW",400,"DC",0.82,"± 5",26,7.9,22.3,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4824JFW","≤26","≤ 8","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4823RJF",400,"DC",8.2000000000000003E-2,"± 5",12,5.8,16,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4823RJF","≤12","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4823KT",400,"DC",8.2000000000000003E-2,"±10",12.5,5.8,11,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4823KT","≤13","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4823JT3",400,"DC",8.2000000000000003E-2,"± 5",12.5,5.8,16,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4823JT3","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4684KFW",400,"DC",0.68,"±10",26,7,21.5,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4684KFW","≤26","≤ 7","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4684JTB",400,"DC",0.68,"± 5",26.5,7,21.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4684JTB","≤27","≤ 7","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4683RJT",400,"DC",6.8000000000000005E-2,"± 5",12.5,5.4,15.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4683RJT","≤13","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4683KF",400,"DC",6.8000000000000005E-2,"±10",12,5.4,10.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4683KF","≤12","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4683JT",400,"DC",6.8000000000000005E-2,"± 5",12.5,5.4,10.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4683JT","≤13","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4564KT",400,"DC",0.56000000000000005,"±10",26.5,6.5,16,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4564KT","≤27","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4564KF",400,"DC",0.56000000000000005,"±10",26,6.5,16,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4564KF","≤26","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4563RKT",400,"DC",5.6000000000000001E-2,"±10",12.5,5,15,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4563RKT","≤13","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4563KF9",400,"DC",5.6000000000000001E-2,"±10",12,5,15,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4563KF9","≤12","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4563JTB",400,"DC",5.6000000000000001E-2,"± 5",12.5,5,15,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4563JTB","≤13","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4563JF",400,"DC",5.6000000000000001E-2,"± 5",12,5,10,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4563JF","≤12","≤ 5","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4474KFB",400,"DC",0.47,"±10",18.5,7.8,22,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4474KFB","≤19","≤ 8","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4474JTB",400,"DC",0.47,"± 5",19,7.8,22,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4474JTB","≤19","≤ 8","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4473RKT",400,"DC",4.7E-2,"±10",12.5,5,13.3,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4473RKT","≤13","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4473RJF",400,"DC",4.7E-2,"± 5",12,5,13.3,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4473RJF","≤12","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4473JT3",400,"DC",4.7E-2,"± 5",12.5,5,13.3,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4473JT3","≤13","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4473JF3",400,"DC",4.7E-2,"± 5",12,5,13.3,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4473JF3","≤12","≤ 5","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4394RKF",400,"DC",0.39,"±10",18.5,7.5,20.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4394RKF",{"$f":"IF(L4299<=9.5,\"≤ \"&ROUNDUP(L4299*1,0)/1,\"≤\"&ROUNDUP(L4299*1,0)/1)","v":"≤19"},{"$f":"IF(M4299<=9,\"≤ \"&ROUNDUP(M4299*1,0)/1,\"≤\"&ROUNDUP(M4299*1,0)/1)","v":"≤ 8"},{"$f":"IF(N4299<=9.5,\"≤ \"&ROUNDUP(N4299*2,0)/2,\"≤\"&ROUNDUP(N4299*2,0)/2)","v":"≤20.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4394KFB",400,"DC",0.39,"±10",18.5,7.5,20.399999999999999,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4394KFB","≤19","≤ 8","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4394JF",400,"DC",0.39,"± 5",18.5,7.5,15.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4394JF","≤19","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4393RKT",400,"DC",3.9E-2,"±10",12.5,4.9000000000000004,13,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",900,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4393RKT","≤13","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4393KF9",400,"DC",3.9E-2,"±10",12,4.9000000000000004,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4393KF9","≤12","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4393JTB",400,"DC",3.9E-2,"± 5",12.5,4.9000000000000004,13,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4393JTB","≤13","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4393JF",400,"DC",3.9E-2,"± 5",12,4.9000000000000004,8,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4393JF","≤12","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4334KT",400,"DC",0.33,"±10",19,7,14.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4334KT","≤19","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4334KF",400,"DC",0.33,"±10",18.5,7,14.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4334KF","≤19","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4334JF",400,"DC",0.33,"± 5",18.5,7,14.9,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4334JF","≤19","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4333KFB",400,"DC",3.3000000000000002E-2,"±10",10.3,6,14,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4333KFB","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4333KF9",400,"DC",3.3000000000000002E-2,"±10",10.3,6,14,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4333KF9",{"$f":"IF(L4363<=9.5,\"≤ \"&ROUNDUP(L4363*1,0)/1,\"≤\"&ROUNDUP(L4363*1,0)/1)","v":"≤11"},{"$f":"IF(M4363<=9,\"≤ \"&ROUNDUP(M4363*1,0)/1,\"≤\"&ROUNDUP(M4363*1,0)/1)","v":"≤ 6"},{"$f":"IF(N4363<=9.5,\"≤ \"&ROUNDUP(N4363*2,0)/2,\"≤\"&ROUNDUP(N4363*2,0)/2)","v":"≤14"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4333JF3",400,"DC",3.3000000000000002E-2,"± 5",10.3,6,14,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4333JF3","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4274RKF",400,"DC",0.27,"±10",18.5,6.5,19.3,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4274RKF","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4274KFB",400,"DC",0.27,"±10",18.5,6.5,19.3,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4274KFB","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4274JF",400,"DC",0.27,"± 5",18.5,6.5,14.3,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4274JF","≤19","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4273RJT",400,"DC",2.7E-2,"± 5",10.8,5.5,13,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4273RJT","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4273KFB",400,"DC",2.7E-2,"±10",10.3,5.5,13,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4273KFB","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4273JF9",400,"DC",2.7E-2,"± 5",10.3,5.5,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4273JF9","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4273JF3",400,"DC",2.7E-2,"± 5",10.3,5.5,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4273JF3","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4225JFW",400,"DC",2.2000000000000002,"± 5",31,11,27,22.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4225JFW","≤31","≤11","≤27",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4224RKT",400,"DC",0.22,"±10",19,5.9,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4224RKT","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4224KFW",400,"DC",0.22,"±10",18.5,5.9,18,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4224KFW","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4224JF3",400,"DC",0.22,"± 5",18.5,5.9,18,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4224JF3","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4223KT3",400,"DC",2.1999999999999999E-2,"±10",10.8,4.8,12.9,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4223KT3","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4223KF3",400,"DC",2.1999999999999999E-2,"±10",10.3,4.8,12.9,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4223KF3","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4223JFB",400,"DC",2.1999999999999999E-2,"± 5",10.3,4.8,12.9,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4223JFB","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4223JF9",400,"DC",2.1999999999999999E-2,"± 5",10.3,4.8,12.9,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4223JF9","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4185JT",400,"DC",1.8,"± 5",31.5,11,20.5,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4185JT","≤32","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4185JF",400,"DC",1.8,"± 5",31,11,20.5,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4185JF","≤31","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4184KT",400,"DC",0.18,"±10",19,5.4,12.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4184KT","≤19","≤ 6","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4184JFB",400,"DC",0.18,"± 5",18.5,5.4,17.5,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4184JFB","≤19","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4183KTB",400,"DC",1.7999999999999999E-2,"±10",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4183KTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4183KFW",400,"DC",1.7999999999999999E-2,"±10",10.3,4.4000000000000004,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4183KFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4183JT3",400,"DC",1.7999999999999999E-2,"± 5",10.8,4.4000000000000004,12.5,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4183JT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4183JFB",400,"DC",1.7999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4183JFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4155JTB",400,"DC",1.5,"± 5",31.5,9.5,24,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4155JTB","≤32","≤10","≤24",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4154RJT",400,"DC",0.15,"± 5",19,5,17.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4154RJT","≤19","≤ 5","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4154KT3",400,"DC",0.15,"±10",19,5,17.399999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4154KT3","≤19","≤ 5","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4154JFW",400,"DC",0.15,"± 5",18.5,5,17.399999999999999,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4154JFW","≤19","≤ 5","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4153RJF",400,"DC",1.4999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4153RJF","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4153KT",400,"DC",1.4999999999999999E-2,"±10",10.8,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4153KT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4153JFW",400,"DC",1.4999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4153JFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4153JF9",400,"DC",1.4999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4153JF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4125KF",400,"DC",1.2,"±10",26,9.5,18.899999999999999,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4125KF","≤26","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4124RKF",400,"DC",0.12,"±10",18.5,5,15,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4124RKF","≤19","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4124KTB",400,"DC",0.12,"±10",19,5,15,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4124KTB","≤19","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4124JT",400,"DC",0.12,"± 5",19,5,10,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4124JT","≤19","≤ 5","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4123RJT",400,"DC",1.2E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4123RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4123KT3",400,"DC",1.2E-2,"±10",10.8,4.4000000000000004,12.5,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4123KT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4123JT",400,"DC",1.2E-2,"± 5",10.8,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4123JT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4123JFW",400,"DC",1.2E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4123JFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4105JTB",400,"DC",1,"± 5",26.5,8.5,23,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4105JTB","≤27","≤ 9","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4104RKT",400,"DC",0.1,"±10",12.5,6.3,17,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4104RKT","≤13","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4104RJF",400,"DC",0.1,"± 5",12,6.3,17,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4104RJF","≤12","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4104JTB",400,"DC",0.1,"± 5",12.5,6.3,17,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4104JTB","≤13","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4104JF",400,"DC",0.1,"± 5",12,6.3,12,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4104JF","≤12","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4103RJT",400,"DC",0.01,"± 5",10.8,4.3,12.4,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4103RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE4103KF9",400,"DC",0.01,"±10",10.3,4.3,12.4,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4103KF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE4103JTB",400,"DC",0.01,"± 5",10.8,4.3,12.4,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE4103JTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A823RJF",250,"AC",8.2000000000000003E-2,"± 5",18.5,6.3,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A823RJF","≤19","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A823KF",250,"AC",8.2000000000000003E-2,"±10",18.5,6.3,12,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A823KF","≤19","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A823JT",250,"AC",8.2000000000000003E-2,"± 5",19,6.3,12,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A823JT","≤19","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A683KFW",250,"AC",6.8000000000000005E-2,"±10",18.5,5.8,16,10,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A683KFW","≤19","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A683JFB",250,"AC",6.8000000000000005E-2,"± 5",18.5,5.8,16,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A683JFB","≤19","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A563RJF",250,"AC",5.6000000000000001E-2,"± 5",18.5,5.4,15.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A563RJF",{"$f":"IF(L4683<=9.5,\"≤ \"&ROUNDUP(L4683*1,0)/1,\"≤\"&ROUNDUP(L4683*1,0)/1)","v":"≤19"},{"$f":"IF(M4683<=9,\"≤ \"&ROUNDUP(M4683*1,0)/1,\"≤\"&ROUNDUP(M4683*1,0)/1)","v":"≤ 6"},{"$f":"IF(N4683<=9.5,\"≤ \"&ROUNDUP(N4683*2,0)/2,\"≤\"&ROUNDUP(N4683*2,0)/2)","v":"≤15.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A563JTB",250,"AC",5.6000000000000001E-2,"± 5",19,5.4,15.5,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A563JTB","≤19","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A563JFW",250,"AC",5.6000000000000001E-2,"± 5",18.5,5.4,15.5,10,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A563JFW","≤19","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A474JT",250,"AC",0.47,"± 5",26.5,9.3000000000000007,18.5,22.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A474JT","≤27","≤10","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A473KT6",250,"AC",4.7E-2,"±10",13,6.5,19.399999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A473KT6","≤13","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A473KFB",250,"AC",4.7E-2,"±10",12.5,6.5,19.399999999999999,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A473KFB","≤13","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A473JFB",250,"AC",4.7E-2,"± 5",12.5,6.5,19.399999999999999,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A473JFB","≤13","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A394JFW",250,"AC",0.39,"± 5",26,8.5,22.9,15,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A394JFW","≤26","≤ 9","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A393RKF",250,"AC",3.9E-2,"±10",12.5,6,18.399999999999999,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A393RKF","≤13","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A393KF",250,"AC",3.9E-2,"±10",12.5,6,13.4,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A393KF","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A393JT",250,"AC",3.9E-2,"± 5",13,6,13.4,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A393JT","≤13","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A334JTB",250,"AC",0.33,"± 5",26.5,7.8,22,15,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A334JTB","≤27","≤ 8","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A333KTB",250,"AC",3.3000000000000002E-2,"±10",13,6,16.899999999999999,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A333KTB","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A333KFW",250,"AC",3.3000000000000002E-2,"±10",12.5,6,16.899999999999999,10,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A333KFW","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A333JT6",250,"AC",3.3000000000000002E-2,"± 5",13,6,16.899999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A333JT6","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A274KF",250,"AC",0.27,"±10",26,7,16.5,22.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A274KF","≤26","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A274JFW",250,"AC",0.27,"± 5",26,7,21.5,15,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A274JFW","≤26","≤ 7","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A273KT",250,"AC",2.7E-2,"±10",13,5.5,10.9,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A273KT","≤13","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A273KF6",250,"AC",2.7E-2,"±10",12.5,5.5,15.9,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A273KF6","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A224RKF",250,"AC",0.22,"±10",18.5,9,21.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A224RKF","≤19","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A224KF",250,"AC",0.22,"±10",18.5,9,16.899999999999999,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A224KF","≤19","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A224JT",250,"AC",0.22,"± 5",19,9,16.899999999999999,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A224JT","≤19","≤ 9","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A223KT6",250,"AC",2.1999999999999999E-2,"±10",13,6,16.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A223KT6","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A223JT6",250,"AC",2.1999999999999999E-2,"± 5",13,6,16.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A223JT6","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A223JF6",250,"AC",2.1999999999999999E-2,"± 5",12.5,6,16.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A223JF6","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A184KFW",250,"AC",0.18,"±10",18.5,8,21,10,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A184KFW","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A184JTB",250,"AC",0.18,"± 5",19,8,21,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A184JTB","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A183RJF",250,"AC",1.7999999999999999E-2,"± 5",12.5,6,16.899999999999999,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A183RJF","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A183JT6",250,"AC",1.7999999999999999E-2,"± 5",13,6,16.899999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A183JT6","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A183JFB",250,"AC",1.7999999999999999E-2,"± 5",12.5,6,16.899999999999999,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A183JFB","≤13","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A154KT",250,"AC",0.15,"±10",19,7.5,15.4,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A154KT","≤19","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A154JF",250,"AC",0.15,"± 5",18.5,7.5,15.4,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A154JF","≤19","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A153RJF",250,"AC",1.4999999999999999E-2,"± 5",12.5,5.5,14.9,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A153RJF","≤13","≤ 6","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A153KF",250,"AC",1.4999999999999999E-2,"±10",12.5,6.3,9.9,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A153KF","≤13","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A153JT",250,"AC",1.4999999999999999E-2,"± 5",13,6.3,9.9,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A153JT","≤13","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE2A124KTB",250,"AC",0.12,"±10",19,6.8,19.5,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A124KTB","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A124JFW",250,"AC",0.12,"± 5",18.5,6.8,19.5,10,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A124JFW","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A123RKF",250,"AC",1.2E-2,"±10",12.5,6,16.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A123RKF","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A123KF6",250,"AC",1.2E-2,"±10",12.5,6,16.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A123KF6","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A104RKF",250,"AC",0.1,"±10",18.5,6.3,19,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A104RKF","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A104RJF",250,"AC",0.1,"± 5",18.5,6.3,19,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A104RJF","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A104KF",250,"AC",0.1,"±10",18.5,6.3,14,15,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A104KF","≤19","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A104JFB",250,"AC",0.1,"± 5",18.5,6.3,19,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A104JFB","≤19","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A103KFW",250,"AC",0.01,"±10",12.5,5.5,15.8,10,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A103KFW","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE2A103JF6",250,"AC",0.01,"± 5",12.5,5.5,15.8,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2A103JF6","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2825KT",250,"DC",8.1999999999999993,"±10",31.5,14.3,23.5,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2825KT","≤32","≤15","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2825JFB",250,"DC",8.1999999999999993,"± 5",31,14.3,28.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2825JFB","≤31","≤15","≤28.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2824KT3",250,"DC",0.82,"±10",19,6.5,19.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2824KT3","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2824KT",250,"DC",0.82,"±10",19,6.5,14.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2824KT","≤19","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2824JT3",250,"DC",0.82,"± 5",19,6.5,19.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2824JT3","≤19","≤ 7","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2824JBB",250,"DC",0.82,"± 5",15.3,6.3,18.3,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2824JBB","≤16","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2823RKT",250,"DC",8.2000000000000003E-2,"±10",10.8,4.9000000000000004,13,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2823RKT","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2823KF9",250,"DC",8.2000000000000003E-2,"±10",10.3,4.9000000000000004,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2823KF9","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2823KBB",250,"DC",8.2000000000000003E-2,"±10",7.9,5.4,13.6,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2823KBB","≤ 8","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2823JFW",250,"DC",8.2000000000000003E-2,"± 5",10.3,4.9000000000000004,13,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2823JFW","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2685KTB",250,"DC",6.8,"±10",31.5,13,27.4,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2685KTB","≤32","≤13","≤27.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2685KT",250,"DC",6.8,"±10",31.5,13,22.4,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2685KT","≤32","≤13","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2684RKT",250,"DC",0.68,"±10",19,6,18.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2684RKT","≤19","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2684RJT",250,"DC",0.68,"± 5",19,6,18.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2684RJT","≤19","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2684KF3",250,"DC",0.68,"±10",18.5,6,18.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2684KF3","≤19","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2684JT",250,"DC",0.68,"± 5",19,6,13.5,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2684JT","≤19","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2684JB",250,"DC",0.68,"± 5",12.3,7.3,12.7,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2684JB","≤13","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2683RJT",250,"DC",6.8000000000000005E-2,"± 5",10.8,4.5,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2683RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2683KF",250,"DC",6.8000000000000005E-2,"±10",10.3,4.5,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2683KF","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2683KBB",250,"DC",6.8000000000000005E-2,"±10",7.9,5.0999999999999996,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2683KBB","≤ 8","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2683JF9",250,"DC",6.8000000000000005E-2,"± 5",10.3,4.5,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2683JF9",{"$f":"IF(L5067<=9.5,\"≤ \"&ROUNDUP(L5067*1,0)/1,\"≤\"&ROUNDUP(L5067*1,0)/1)","v":"≤11"},{"$f":"IF(M5067<=9,\"≤ \"&ROUNDUP(M5067*1,0)/1,\"≤\"&ROUNDUP(M5067*1,0)/1)","v":"≤ 5"},{"$f":"IF(N5067<=9.5,\"≤ \"&ROUNDUP(N5067*2,0)/2,\"≤\"&ROUNDUP(N5067*2,0)/2)","v":"≤12.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2683JBB",250,"DC",6.8000000000000005E-2,"± 5",7.9,5.0999999999999996,13,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2683JBB","≤ 8","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2565KFB",250,"DC",5.6,"±10",31,11.8,26,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2565KFB","≤31","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2565JFB",250,"DC",5.6,"± 5",31,11.8,26,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2565JFB","≤31","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2564KT",250,"DC",0.56000000000000005,"±10",19,5.5,13,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2564KT","≤19","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2564KF3",250,"DC",0.56000000000000005,"±10",18.5,5.5,18,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2564KF3","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2564JFB",250,"DC",0.56000000000000005,"± 5",18.5,5.5,18,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2564JFB","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2564JF3",250,"DC",0.56000000000000005,"± 5",18.5,5.5,18,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2564JF3","≤19","≤ 6","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2563KTB",250,"DC",5.6000000000000001E-2,"±10",10.8,4.8,12.9,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2563KTB","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2563KFW",250,"DC",5.6000000000000001E-2,"±10",10.3,4.8,12.9,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2563KFW","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2563KB2",250,"DC",5.6000000000000001E-2,"±10",7.9,4.7,7.7,5,"Straight lead wire type","-40 to 105 (85)","12.7P straight lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2563KB2","≤ 8","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2563JF",250,"DC",5.6000000000000001E-2,"± 5",10.3,4.8,7.9,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2563JF","≤11","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2475RJB",250,"DC",4.7,"± 5",20.8,11.9,26,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2475RJB","≤21","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2475KFW",250,"DC",4.7,"±10",26,12,26.5,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2475KFW","≤26","≤12","≤26.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2475JF",250,"DC",4.7,"± 5",26,12,21.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2475JF","≤26","≤12","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2475JBB",250,"DC",4.7,"± 5",20.8,11.9,26,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2475JBB","≤21","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2474KT3",250,"DC",0.47,"±10",19,5.3,17.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2474KT3","≤19","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2474KB3",250,"DC",0.47,"±10",12.3,6.2,16.399999999999999,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2474KB3","≤13","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2474JT3",250,"DC",0.47,"± 5",19,5.3,17.5,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2474JT3","≤19","≤ 6","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2473RKT",250,"DC",4.7E-2,"±10",10.8,4.5,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2473RKT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2473KFW",250,"DC",4.7E-2,"±10",10.3,4.5,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2473KFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2473KF3",250,"DC",4.7E-2,"±10",10.3,4.5,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2473KF3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2473JT",250,"DC",4.7E-2,"± 5",10.8,4.5,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2473JT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2473JFW",250,"DC",4.7E-2,"± 5",10.3,4.5,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2473JFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2395RKB",250,"DC",3.9,"±10",20.8,10.8,24.8,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2395RKB","≤21","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2395KBB",250,"DC",3.9,"±10",20.8,10.8,24.8,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2395KBB","≤21","≤11","≤25",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2395JT",250,"DC",3.9,"± 5",26.5,11,20.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2395JT","≤27","≤11","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2394RJT",250,"DC",0.39,"± 5",19,4.9000000000000004,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2394RJT","≤19","≤ 5","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2394KFB",250,"DC",0.39,"±10",18.5,4.9000000000000004,17,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2394KFB","≤19","≤ 5","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2394KBB",250,"DC",0.39,"±10",12.3,5.7,15.9,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2394KBB","≤13","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2394JT",250,"DC",0.39,"± 5",19,4.9000000000000004,12,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2394JT","≤19","≤ 5","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2394JF",250,"DC",0.39,"± 5",18.5,4.9000000000000004,12,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2394JF","≤19","≤ 5","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2393KT3",250,"DC",3.9E-2,"±10",10.8,4.5,12.5,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2393KT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2393KB3",250,"DC",3.9E-2,"±10",7.9,4.5,12.4,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2393KB3","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2393JTB",250,"DC",3.9E-2,"± 5",10.8,4.5,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2393JTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2393JB3",250,"DC",3.9E-2,"± 5",7.9,4.5,12.4,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2393JB3","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2335KFW",250,"DC",3.3,"±10",26,10.3,23,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2335KFW","≤26","≤11","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2335KBB",250,"DC",3.3,"±10",20.8,10.5,22.9,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2335KBB","≤21","≤11","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2335JBB",250,"DC",3.3,"± 5",20.8,10.5,22.9,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2335JBB","≤21","≤11","≤23",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2334RJB",250,"DC",0.33,"± 5",10.3,6.4,16.3,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2334RJB","≤11","≤ 7","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2334KFW",250,"DC",0.33,"±10",12,6.5,17,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2334KFW","≤12","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2334KB",250,"DC",0.33,"±10",10.3,6.4,11.3,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2334KB","≤11","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2334JT",250,"DC",0.33,"± 5",12.5,6.5,12,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2334JT","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2333RKT",250,"DC",3.3000000000000002E-2,"±10",10.8,4.5,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2333RKT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2333KFW",250,"DC",3.3000000000000002E-2,"±10",10.3,4.5,12.5,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2333KFW","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2333KF3",250,"DC",3.3000000000000002E-2,"±10",10.3,4.5,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2333KF3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2333JT3",250,"DC",3.3000000000000002E-2,"± 5",10.8,4.5,12.5,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2333JT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2333JFB",250,"DC",3.3000000000000002E-2,"± 5",10.3,4.5,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2333JFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2275RKB",250,"DC",2.7,"±10",20.8,9.3000000000000007,21.7,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2275RKB","≤21","≤10","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2275KBB",250,"DC",2.7,"±10",20.8,9.3000000000000007,21.7,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2275KBB","≤21","≤10","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2275JT",250,"DC",2.7,"± 5",26.5,9.4,17,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2275JT","≤27","≤10","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2274RKF",250,"DC",0.27,"±10",12,6,16.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2274RKF","≤12","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2274KFB",250,"DC",0.27,"±10",12,6,16.5,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2274KFB","≤12","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2274KF",250,"DC",0.27,"±10",12,6,11.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2274KF","≤12","≤ 6","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2274JFW",250,"DC",0.27,"± 5",12,6,16.5,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2274JFW","≤12","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2274JF3",250,"DC",0.27,"± 5",12,6,16.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2274JF3","≤12","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2273KTB",250,"DC",2.7E-2,"±10",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2273KTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2273KFB",250,"DC",2.7E-2,"±10",10.3,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2273KFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2273KB3",250,"DC",2.7E-2,"±10",7.9,4.3,12.2,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2273KB3","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2273JFB",250,"DC",2.7E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2273JFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2225RJB",250,"DC",2.2000000000000002,"± 5",20.8,8.4,20.6,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2225RJB","≤21","≤ 9","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2225KFW",250,"DC",2.2000000000000002,"±10",26,8.5,21.3,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2225KFW","≤26","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2225JFW",250,"DC",2.2000000000000002,"± 5",26,8.5,21.3,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2225JFW","≤26","≤ 9","≤21.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2225JBB",250,"DC",2.2000000000000002,"± 5",20.8,8.4,20.6,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2225JBB","≤21","≤ 9","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2224RJB",250,"DC",0.22,"± 5",10.3,5.4,15.1,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2224RJB","≤11","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2224KBB",250,"DC",0.22,"±10",10.3,5.4,15.1,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2224KBB",{"$f":"IF(L5451<=9.5,\"≤ \"&ROUNDUP(L5451*1,0)/1,\"≤\"&ROUNDUP(L5451*1,0)/1)","v":"≤11"},{"$f":"IF(M5451<=9,\"≤ \"&ROUNDUP(M5451*1,0)/1,\"≤\"&ROUNDUP(M5451*1,0)/1)","v":"≤ 6"},{"$f":"IF(N5451<=9.5,\"≤ \"&ROUNDUP(N5451*2,0)/2,\"≤\"&ROUNDUP(N5451*2,0)/2)","v":"≤15.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2224JT",250,"DC",0.22,"± 5",12.5,5.5,10.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2224JT","≤13","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2224JF9",250,"DC",0.22,"± 5",12,5.5,15.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2224JF9","≤12","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2223RJT",250,"DC",2.1999999999999999E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2223RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2223KT3",250,"DC",2.1999999999999999E-2,"±10",10.8,4.4000000000000004,12.5,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2223KT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2223KBB",250,"DC",2.1999999999999999E-2,"±10",7.9,4.3,12.2,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2223KBB","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2223KB",250,"DC",2.1999999999999999E-2,"±10",7.9,4.3,7.2,5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2223KB","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2223JF3",250,"DC",2.1999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2223JF3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2185KT",250,"DC",1.8,"±10",26.5,7.5,15.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2185KT","≤27","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2185KF",250,"DC",1.8,"±10",26,7.5,15.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2185KF","≤26","≤ 8","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2185JBB",250,"DC",1.8,"± 5",20.8,7.6,19.600000000000001,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2185JBB","≤21","≤ 8","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2184RJB",250,"DC",0.18,"± 5",10.3,5,14.7,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2184RJB","≤11","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2184KT",250,"DC",0.18,"±10",12.5,5,10.3,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2184KT","≤13","≤ 5","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2184KB3",250,"DC",0.18,"±10",10.3,5,14.7,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2184KB3","≤11","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2184JT3",250,"DC",0.18,"± 5",12.5,5,15.3,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",800,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2184JT3","≤13","≤ 5","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2184JBB",250,"DC",0.18,"± 5",10.3,5,14.7,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2184JBB","≤11","≤ 5","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2183KT",250,"DC",1.7999999999999999E-2,"±10",10.8,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2183KT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2183KF9",250,"DC",1.7999999999999999E-2,"±10",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2183KF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2183JTB",250,"DC",1.7999999999999999E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2183JTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2183JF9",250,"DC",1.7999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2183JF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2183JB3",250,"DC",1.7999999999999999E-2,"± 5",7.9,4.3,12.2,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2183JB3","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2155KTB",250,"DC",1.5,"±10",19,9,21.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2155KTB","≤19","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2155KFW",250,"DC",1.5,"±10",18.5,9,21.8,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2155KFW","≤19","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2155JTB",250,"DC",1.5,"± 5",19,9,21.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2155JTB","≤19","≤ 9","≤22",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2155JB",250,"DC",1.5,"± 5",15.3,8.6,15.7,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2155JB","≤16","≤ 9","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2154RJT",250,"DC",0.15,"± 5",10.8,6,15.8,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2154RJT","≤11","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2154KF9",250,"DC",0.15,"±10",10.3,6,15.8,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2154KF9","≤11","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2154JT",250,"DC",0.15,"± 5",10.8,6,10.8,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2154JT","≤11","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2154JFW",250,"DC",0.15,"± 5",10.3,6,15.8,7.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2154JFW","≤11","≤ 6","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2154JB",250,"DC",0.15,"± 5",7.9,6.3,11.2,5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2154JB","≤ 8","≤ 7","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2153RJT",250,"DC",1.4999999999999999E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2153RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2153KF9",250,"DC",1.4999999999999999E-2,"±10",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2153KF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2153JT",250,"DC",1.4999999999999999E-2,"± 5",10.8,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2153JT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2153JF9",250,"DC",1.4999999999999999E-2,"± 5",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2153JF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2125RKT",250,"DC",1.2,"±10",19,8,20.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2125RKT","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2125KFW",250,"DC",1.2,"±10",18.5,8,20.9,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2125KFW","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2125KFB",250,"DC",1.2,"±10",18.5,8,20.9,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2125KFB","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2125JFW",250,"DC",1.2,"± 5",18.5,8,20.9,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2125JFW","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2125JF3",250,"DC",1.2,"± 5",18.5,8,20.9,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2125JF3","≤19","≤ 8","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2124RJT",250,"DC",0.12,"± 5",10.8,6,14,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2124RJT","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2124KF",250,"DC",0.12,"±10",10.3,6,9,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2124KF","≤11","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2124JT",250,"DC",0.12,"± 5",10.8,6,9,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2124JT","≤11","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2124JF9",250,"DC",0.12,"± 5",10.3,6,14,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2124JF9","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2123RJT",250,"DC",1.2E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2123RJT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2123RJF",250,"DC",1.2E-2,"± 5",10.3,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2123RJF","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2123KBB",250,"DC",1.2E-2,"±10",7.9,4.2,12.1,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2123KBB","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2123JTB",250,"DC",1.2E-2,"± 5",10.8,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2123JTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2123JF9",250,"DC",1.2E-2,"± 5",10.3,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2123JF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2106KFW",250,"DC",10,"±10",31,15.9,30.8,22.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2106KFW","≤31","≤16","≤31",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2106JF",250,"DC",10,"± 5",31,15.9,25.8,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2106JF","≤31","≤16","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2105RKB",250,"DC",1,"±10",15.3,7,19,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2105RKB","≤16","≤ 7","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2105KF3",250,"DC",1,"±10",18.5,7.4,20,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2105KF3","≤19","≤ 8","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2105KF",250,"DC",1,"±10",18.5,7.4,15,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2105KF","≤19","≤ 8","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2105JF3",250,"DC",1,"± 5",18.5,7.4,20,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2105JF3","≤19","≤ 8","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2104RJT",250,"DC",0.1,"± 5",10.8,5.8,13.4,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2104RJT","≤11","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2104KTB",250,"DC",0.1,"±10",10.8,5.8,13.4,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2104KTB",{"$f":"IF(L5771<=9.5,\"≤ \"&ROUNDUP(L5771*1,0)/1,\"≤\"&ROUNDUP(L5771*1,0)/1)","v":"≤11"},{"$f":"IF(M5771<=9,\"≤ \"&ROUNDUP(M5771*1,0)/1,\"≤\"&ROUNDUP(M5771*1,0)/1)","v":"≤ 6"},{"$f":"IF(N5771<=9.5,\"≤ \"&ROUNDUP(N5771*2,0)/2,\"≤\"&ROUNDUP(N5771*2,0)/2)","v":"≤13.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2104KB3",250,"DC",0.1,"±10",7.9,5.9,14,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2104KB3","≤ 8","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2104JFB",250,"DC",0.1,"± 5",10.3,5.8,13.4,7.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2104JFB","≤11","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2104JF",250,"DC",0.1,"± 5",10.3,5.8,8.4,7.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2104JF","≤11","≤ 6","≤ 8.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2103KTB",250,"DC",0.01,"±10",10.8,4.3,12.4,7.5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2103KTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[DC]","ECQE2103KT3",250,"DC",0.01,"±10",10.8,4.3,12.4,5,"Crimped lead wire type (Style Y)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2103KT3","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2103KB2",250,"DC",0.01,"±10",7.9,4.2,7.1,5,"Straight lead wire type","-40 to 105 (85)","12.7P straight lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2103KB2","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE2103JF9",250,"DC",0.01,"± 5",10.3,4.3,12.4,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Reel packing (radial leaded)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2103JF9","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[DC]","ECQE2103JBB",250,"DC",0.01,"± 5",7.9,4.2,12.1,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE2103JBB","≤ 8","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A824KB3",125,"AC",0.82,"±10",15.3,6.3,18.3,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A824KB3","≤16","≤ 7","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A823RKF",125,"AC",8.2000000000000003E-2,"±10",10.5,6.5,14.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823RKF","≤11","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A823RJF",125,"AC",8.2000000000000003E-2,"± 5",10.5,6.5,14.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823RJF","≤11","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A823KF",125,"AC",8.2000000000000003E-2,"±10",10.5,6.5,9.8000000000000007,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823KF","≤11","≤ 7","≤10",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A823KBZ",125,"AC",8.2000000000000003E-2,"±10",10.3,4.5999999999999996,7.6,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823KBZ","≤11","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A823JFW",125,"AC",8.2000000000000003E-2,"± 5",10.5,6.5,14.8,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823JFW","≤11","≤ 7","≤15",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A823JB",125,"AC",8.2000000000000003E-2,"± 5",10.3,4.5999999999999996,7.6,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A823JB","≤11","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A684MB",125,"AC",0.68,"±20",12.3,7.3,12.7,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A684MB","≤13","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A683RKT",125,"AC",6.8000000000000005E-2,"±10",11,6.3,14.4,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1200,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A683RKT","≤11","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A683KTB",125,"AC",6.8000000000000005E-2,"±10",11,6.3,14.4,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A683KTB","≤11","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A683KFB",125,"AC",6.8000000000000005E-2,"±10",10.5,6.3,14.4,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A683KFB","≤11","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A683JT6",125,"AC",6.8000000000000005E-2,"± 5",11,6.3,14.4,5,"Crimped lead wire type (Style D)","-40 to 85","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A683JT6","≤11","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A683JFW",125,"AC",6.8000000000000005E-2,"± 5",10.5,6.3,14.4,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A683JFW","≤11","≤ 7","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A564KBZ",125,"AC",0.56000000000000005,"±10",12.3,6.7,11.9,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A564KBZ","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A564JB",125,"AC",0.56000000000000005,"± 5",12.3,6.7,11.9,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A564JB","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A563RJT",125,"AC",5.6000000000000001E-2,"± 5",11,5.9,13.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A563RJT","≤11","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A563KF",125,"AC",5.6000000000000001E-2,"±10",10.5,5.9,8.5,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A563KF","≤11","≤ 6","≤ 8.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A563JFZ",125,"AC",5.6000000000000001E-2,"± 5",10.5,5.9,8.5,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A563JFZ","≤11","≤ 6","≤ 8.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A563JFW",125,"AC",5.6000000000000001E-2,"± 5",10.5,5.9,13.5,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A563JFW","≤11","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A475KBB",125,"AC",4.7,"±10",25.8,11.8,25.8,15,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A475KBB","≤26","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A475JBB",125,"AC",4.7,"± 5",25.8,11.8,25.8,15,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A475JBB","≤26","≤12","≤26",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A474KT3",125,"AC",0.47,"±10",19,7.5,20.3,5,"Crimped lead wire type (Style D)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A474KT3","≤19","≤ 8","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A474KBZ",125,"AC",0.47,"±10",12.3,7,12.2,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A474KBZ","≤13","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A474KB",125,"AC",0.47,"±10",12.3,7,12.2,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A474KB","≤13","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A474JBZ",125,"AC",0.47,"± 5",12.3,7,12.2,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A474JBZ","≤13","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A473RJF",125,"AC",4.7E-2,"± 5",10.5,5.5,13,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A473RJF","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A473KT",125,"AC",4.7E-2,"±10",11,5.5,8,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A473KT","≤11","≤ 6","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A473KB",125,"AC",4.7E-2,"±10",7.9,4.8,7.7,5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A473KB","≤ 8","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A473JTB",125,"AC",4.7E-2,"± 5",11,5.5,13,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A473JTB","≤11","≤ 6","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A473JB2",125,"AC",4.7E-2,"± 5",7.9,4.8,7.7,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A473JB2","≤ 8","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A395JB",125,"AC",3.9,"± 5",25.8,10.6,19.7,22.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A395JB","≤26","≤11","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A394RKB",125,"AC",0.39,"±10",12.3,6.4,16.600000000000001,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A394RKB","≤13","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A394KFZ",125,"AC",0.39,"±10",18.5,7.4,13,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A394KFZ","≤19","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A394JTB",125,"AC",0.39,"± 5",19,7.4,18,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A394JTB","≤19","≤ 8","≤18",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A394JFZ",125,"AC",0.39,"± 5",18.5,7.4,13,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A394JFZ","≤19","≤ 8","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A394JB3",125,"AC",0.39,"± 5",12.3,6.4,16.600000000000001,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A394JB3","≤13","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A393RJF",125,"AC",3.9E-2,"± 5",10.5,4.5,12.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A393RJF","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A393KFB",125,"AC",3.9E-2,"±10",10.5,4.5,12.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A393KFB","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A393JT6",125,"AC",3.9E-2,"± 5",11,4.5,12.8,5,"Crimped lead wire type (Style D)","-40 to 85","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A393JT6","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A393JFW",125,"AC",3.9E-2,"± 5",10.5,4.5,12.8,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A393JFW","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A335KBZ",125,"AC",3.3,"±10",25.8,9.6,18.7,22.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A335KBZ","≤26","≤10","≤19",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A334RJT",125,"AC",0.33,"± 5",19,6.9,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A334RJT","≤19","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A334MB",125,"AC",0.33,"±20",12.3,5.9,11.2,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A334MB","≤13","≤ 6","≤11.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A334KF3",125,"AC",0.33,"±10",18.5,6.9,17.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A334KF3","≤19","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A334KBB",125,"AC",0.33,"±10",12.3,5.9,16.2,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A334KBB","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A334JFW",125,"AC",0.33,"± 5",18.5,6.9,17.5,10,"Double crimped lead wire type (Style T)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A334JFW","≤19","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A333RKT",125,"AC",3.3000000000000002E-2,"±10",11,4.5,12.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A333RKT","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A333RJF",125,"AC",3.3000000000000002E-2,"± 5",10.5,4.5,12.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A333RJF","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A333KF6",125,"AC",3.3000000000000002E-2,"±10",10.5,4.5,12.8,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A333KF6","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A333JFW",125,"AC",3.3000000000000002E-2,"± 5",10.5,4.5,12.8,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A333JFW","≤11","≤ 5","≤13",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A333JF",125,"AC",3.3000000000000002E-2,"± 5",10.5,4.5,7.8,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A333JF","≤11","≤ 5","≤ 8",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A275KBB",125,"AC",2.7,"±10",20.8,10.9,23.2,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A275KBB","≤21","≤11","≤23.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A275JBZ",125,"AC",2.7,"± 5",20.8,10.9,18.2,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A275JBZ","≤21","≤11","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A274RJT",125,"AC",0.27,"± 5",19,6.3,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A274RJT","≤19","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A274KF3",125,"AC",0.27,"±10",18.5,6.3,17,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",600,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A274KF3","≤19","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A274KBZ",125,"AC",0.27,"±10",12.3,5.4,10.7,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A274KBZ","≤13","≤ 6","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A274JFZ",125,"AC",0.27,"± 5",18.5,6.3,12,15,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A274JFZ",{"$f":"IF(L6155<=9.5,\"≤ \"&ROUNDUP(L6155*1,0)/1,\"≤\"&ROUNDUP(L6155*1,0)/1)","v":"≤19"},{"$f":"IF(M6155<=9,\"≤ \"&ROUNDUP(M6155*1,0)/1,\"≤\"&ROUNDUP(M6155*1,0)/1)","v":"≤ 7"},{"$f":"IF(N6155<=9.5,\"≤ \"&ROUNDUP(N6155*2,0)/2,\"≤\"&ROUNDUP(N6155*2,0)/2)","v":"≤12"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A273RKT",125,"AC",2.7E-2,"±10",11,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A273RKT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A273RJF",125,"AC",2.7E-2,"± 5",10.5,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A273RJF","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A273KF6",125,"AC",2.7E-2,"±10",10.5,4.4000000000000004,12.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A273KF6","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A273KB2",125,"AC",2.7E-2,"±10",7.9,4.3,7.2,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A273KB2","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A273JFB",125,"AC",2.7E-2,"± 5",10.5,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A273JFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A225KBB",125,"AC",2.2000000000000002,"±10",20.8,9.6999999999999993,22.1,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A225KBB","≤21","≤10","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A225JBB",125,"AC",2.2000000000000002,"± 5",20.8,9.6999999999999993,22.1,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A225JBB","≤21","≤10","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A224RKB",125,"AC",0.22,"±10",10.3,6.1,16,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224RKB","≤11","≤ 7","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A224KFB",125,"AC",0.22,"±10",12.5,7.5,18.399999999999999,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224KFB","≤13","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A224KF3",125,"AC",0.22,"±10",12.5,7.5,18.399999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224KF3","≤13","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A224JT6",125,"AC",0.22,"± 5",13,7.5,18.399999999999999,5,"Crimped lead wire type (Style D)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224JT6","≤13","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A224JFW",125,"AC",0.22,"± 5",12.5,7.5,18.399999999999999,10,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224JFW","≤13","≤ 8","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A224JB2",125,"AC",0.22,"± 5",10.3,6.1,11,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A224JB2","≤11","≤ 7","≤11",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A223KFZ",125,"AC",2.1999999999999999E-2,"±10",10.5,4.4000000000000004,7.5,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A223KFZ","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A223KF6",125,"AC",2.1999999999999999E-2,"±10",10.5,4.4000000000000004,12.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A223KF6","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A223JT6",125,"AC",2.1999999999999999E-2,"± 5",11,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 85","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A223JT6","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A223JB",125,"AC",2.1999999999999999E-2,"± 5",7.9,4.3,7.2,5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A223JB","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A185RKB",125,"AC",1.8,"±10",20.8,8.6999999999999993,20.9,7.5,"Inner crimped lead wire type (Style B)","-40 to 85","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A185RKB","≤21","≤ 9","≤21",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A185JB",125,"AC",1.8,"± 5",20.8,8.6999999999999993,15.9,17.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A185JB","≤21","≤ 9","≤16",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A184RKB",125,"AC",0.18,"±10",10.3,5.6,15.3,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A184RKB","≤11","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A184KFZ",125,"AC",0.18,"±10",12.5,7,12.5,10,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A184KFZ","≤13","≤ 7","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A184KB",125,"AC",0.18,"±10",10.3,5.6,10.3,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A184KB","≤11","≤ 6","≤10.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A184JF3",125,"AC",0.18,"± 5",12.5,7,17.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A184JF3","≤13","≤ 7","≤17.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A184JBB",125,"AC",0.18,"± 5",10.3,5.6,15.3,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A184JBB","≤11","≤ 6","≤15.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A183KT6",125,"AC",1.7999999999999999E-2,"±10",11,4.4000000000000004,12.5,5,"Crimped lead wire type (Style D)","-40 to 85","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A183KT6","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A183KT",125,"AC",1.7999999999999999E-2,"±10",11,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A183KT","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A183JTB",125,"AC",1.7999999999999999E-2,"± 5",11,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A183JTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A183JFZ",125,"AC",1.7999999999999999E-2,"± 5",10.5,4.4000000000000004,7.5,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A183JFZ","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A183JB",125,"AC",1.7999999999999999E-2,"± 5",7.9,4.3,7.2,5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A183JB","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A155JB3",125,"AC",1.5,"± 5",20.8,8,20.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 85","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A155JB3","≤21","≤ 8","≤20.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A154RJB",125,"AC",0.15,"± 5",10.3,5.7,13.9,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154RJB","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A154KT",125,"AC",0.15,"±10",13,6.5,12,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154KT","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A154KB2",125,"AC",0.15,"±10",10.3,5.7,8.9,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154KB2","≤11","≤ 6","≤ 9",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A154JT",125,"AC",0.15,"± 5",13,6.5,12,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154JT","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A154JF",125,"AC",0.15,"± 5",12.5,6.5,12,10,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154JF","≤13","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A154JB6",125,"AC",0.15,"± 5",10.3,5.7,13.9,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A154JB6","≤11","≤ 6","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A153KTB",125,"AC",1.4999999999999999E-2,"±10",11,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A153KTB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A153KB2",125,"AC",1.4999999999999999E-2,"±10",7.9,4.2,7.1,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A153KB2","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A153JFB",125,"AC",1.4999999999999999E-2,"± 5",10.5,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A153JFB","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A153JBZ",125,"AC",1.4999999999999999E-2,"± 5",7.9,4.2,7.1,5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A153JBZ","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A125JBZ",125,"AC",1.2,"± 5",20.8,7.1,14.1,17.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A125JBZ","≤21","≤ 8","≤14.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A125JBB",125,"AC",1.2,"± 5",20.8,7.1,19.100000000000001,10,"Inner crimped lead wire type (Style B)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A125JBB","≤21","≤ 8","≤19.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A124RJF",125,"AC",0.12,"± 5",12.5,5.9,16.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A124RJF","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A124KF6",125,"AC",0.12,"±10",12.5,5.9,16.5,5,"Inner crimped lead wire type (Style B)","-40 to 85","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A124KF6","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A124KBB",125,"AC",0.12,"±10",10.3,5.3,13.4,7.5,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A124KBB","≤11","≤ 6","≤13.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A124JFB",125,"AC",0.12,"± 5",12.5,5.9,16.5,10,"Crimped lead wire type (Style D)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A124JFB","≤13","≤ 6","≤16.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A123RKT",125,"AC",1.2E-2,"±10",11,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123RKT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A123RJF",125,"AC",1.2E-2,"± 5",10.5,4.4000000000000004,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123RJF","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A123KBZ",125,"AC",1.2E-2,"±10",7.9,4.2,7.1,5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123KBZ","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A123KB2",125,"AC",1.2E-2,"±10",7.9,4.2,7.1,5,"Straight lead wire type","-40 to 85","12.7P straight lead taping (ammo packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123KB2","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A123JF",125,"AC",1.2E-2,"± 5",10.5,4.4000000000000004,7.5,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123JF","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A123JB",125,"AC",1.2E-2,"± 5",7.9,4.2,7.1,5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A123JB","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A105KB",125,"AC",1,"±10",15.3,7,14,12.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A105KB","≤16","≤ 7","≤14",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A104RJF",125,"AC",0.1,"± 5",10.5,6.5,16.8,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A104RJF",{"$f":"IF(L6475<=9.5,\"≤ \"&ROUNDUP(L6475*1,0)/1,\"≤\"&ROUNDUP(L6475*1,0)/1)","v":"≤11"},{"$f":"IF(M6475<=9,\"≤ \"&ROUNDUP(M6475*1,0)/1,\"≤\"&ROUNDUP(M6475*1,0)/1)","v":"≤ 7"},{"$f":"IF(N6475<=9.5,\"≤ \"&ROUNDUP(N6475*2,0)/2,\"≤\"&ROUNDUP(N6475*2,0)/2)","v":"≤17"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A104KFW",125,"AC",0.1,"±10",10.5,6.5,16.8,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A104KFW","≤11","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A104KF",125,"AC",0.1,"±10",10.5,6.5,11.8,7.5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A104KF","≤11","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A104JFZ",125,"AC",0.1,"± 5",10.5,6.5,11.8,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A104JFZ","≤11","≤ 7","≤12",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A104JFW",125,"AC",0.1,"± 5",10.5,6.5,16.8,7.5,"Double crimped lead wire type (Style N)","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A104JFW","≤11","≤ 7","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(T)[AC]","ECQE1A103RKT",125,"AC",0.01,"±10",11,4.5,12.5,7.5,"Crimped lead wire type (Style D)","-40 to 85","15.0P crimped lead taping (ammo packing)",1700,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A103RKT","≤11","≤ 5","≤12.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A103KFZ",125,"AC",0.01,"±10",10.5,4.5,7.5,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A103KFZ","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A103KBZ",125,"AC",0.01,"±10",7.9,4.2,7.1,5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A103KBZ","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[AC]","ECQE1A103JFZ",125,"AC",0.01,"± 5",10.5,4.5,7.5,7.5,"Short cut lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A103JFZ","≤11","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(B)[AC]","ECQE1A103JB",125,"AC",0.01,"± 5",7.9,4.2,7.1,5,"Straight lead wire type","-40 to 85","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1A103JB","≤ 8","≤ 5","≤ 7.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1825KF",100,"DC",8.1999999999999993,"±10",26,10,20,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1825KF","≤26","≤10","≤20",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1824KF",100,"DC",0.82,"±10",12,6,13.5,10,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1824KF",{"$f":"IF(L6539<=9.5,\"≤ \"&ROUNDUP(L6539*1,0)/1,\"≤\"&ROUNDUP(L6539*1,0)/1)","v":"≤12"},{"$f":"IF(M6539<=9,\"≤ \"&ROUNDUP(M6539*1,0)/1,\"≤\"&ROUNDUP(M6539*1,0)/1)","v":"≤ 6"},{"$f":"IF(N6539<=9.5,\"≤ \"&ROUNDUP(N6539*2,0)/2,\"≤\"&ROUNDUP(N6539*2,0)/2)","v":"≤13.5"},null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1824JF3",100,"DC",0.82,"± 5",12,6,18.5,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","15.0P crimped lead taping (ammo packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1824JF3","≤12","≤ 6","≤18.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1684KFB",100,"DC",0.68,"±10",12,6,16.899999999999999,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1684KFB","≤12","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1684JF3",100,"DC",0.68,"± 5",12,6,16.899999999999999,5,"Crimped lead wire type (Style D)","-40 to 105 (85)","12.7P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1684JF3","≤12","≤ 6","≤17",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1565KFB",100,"DC",5.6,"±10",26,8.3000000000000007,22.5,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1565KFB","≤26","≤ 9","≤22.5",null,null,null,null,null,null,null,""]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1564KFB",100,"DC",0.56000000000000005,"±10",12,5.5,15.9,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1564KFB","≤12","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1475KFW",100,"DC",4.7,"±10",26,7.5,22,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1475KFW","≤26","≤ 8","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1475JFW",100,"DC",4.7,"± 5",26,7.5,22,15,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1475JFW","≤26","≤ 8","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1395JFB",100,"DC",3.9,"± 5",26,7,21.4,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1395JFB","≤26","≤ 7","≤21.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1335RJF",100,"DC",3.3,"± 5",18.5,8.5,21.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1335RJF","≤19","≤ 9","≤21.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12823KFW",1250,"DC",8.2000000000000003E-2,"±10",31,9,23.5,22.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12823KFW","≤31","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12822RJF",1250,"DC",8.2000000000000007E-3,"± 5",21,5,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12822RJF","≤21","≤ 5","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12822KF",1250,"DC",8.2000000000000007E-3,"±10",21,5,12,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12822KF","≤21","≤ 5","≤12"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1275KFB",100,"DC",2.7,"±10",18.5,8,20.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1275KFB","≤19","≤ 8","≤21"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1275JFB",100,"DC",2.7,"± 5",18.5,8,20.8,10,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1275JFB","≤19","≤ 8","≤21"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12683JFB",1250,"DC",6.8000000000000005E-2,"± 5",31,8,22.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12683JFB","≤31","≤ 8","≤22.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12682JFW",1250,"DC",6.7999999999999996E-3,"± 5",15.5,7.5,20,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12682JFW","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12563KFW",1250,"DC",5.6000000000000001E-2,"±10",31,7.5,22,22.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12563KFW","≤31","≤ 8","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12562KFB",1250,"DC",5.5999999999999999E-3,"±10",15.5,7.5,18,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12562KFB","≤16","≤ 8","≤18"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12473KF",1250,"DC",4.7E-2,"±10",26,8,17,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12473KF","≤26","≤ 8","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12473JF",1250,"DC",4.7E-2,"± 5",26,8,17,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12473JF","≤26","≤ 8","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12472JFB",1250,"DC",4.7000000000000002E-3,"± 5",15.5,7,17.5,10,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12472JFB","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12392RJF",1250,"DC",3.8999999999999998E-3,"± 5",15.5,6.5,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12392RJF","≤16","≤ 7","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12392JFW",1250,"DC",3.8999999999999998E-3,"± 5",15.5,6.5,17,10,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12392JFW","≤16","≤ 7","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12333KF",1250,"DC",3.3000000000000002E-2,"±10",26,6.5,16,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12333KF","≤26","≤ 7","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12333JF",1250,"DC",3.3000000000000002E-2,"± 5",26,6.5,16,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12333JF","≤26","≤ 7","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12273KFW",1250,"DC",2.7E-2,"±10",26,6,20.5,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12273KFW",{"$f":"IF(L6692<=9.5,\"≤ \"&ROUNDUP(L6692*1,0)/1,\"≤\"&ROUNDUP(L6692*1,0)/1)","v":"≤26"},{"$f":"IF(M6692<=9,\"≤ \"&ROUNDUP(M6692*1,0)/1,\"≤\"&ROUNDUP(M6692*1,0)/1)","v":"≤ 6"},{"$f":"IF(N6692<=9.5,\"≤ \"&ROUNDUP(N6692*2,0)/2,\"≤\"&ROUNDUP(N6692*2,0)/2)","v":"≤20.5"}]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1225RJF",100,"DC",2.2000000000000002,"± 5",18.5,7,20,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1225RJF","≤19","≤ 7","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1225KF3",100,"DC",2.2000000000000002,"±10",18.5,7,20,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1225KF3","≤19","≤ 7","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12224KFB",1250,"DC",0.22,"±10",31,14.5,31.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12224KFB","≤31","≤15","≤31.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12223KF",1250,"DC",2.1999999999999999E-2,"±10",21,7,15,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12223KF","≤21","≤ 7","≤15"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12223JF",1250,"DC",2.1999999999999999E-2,"± 5",21,7,15,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12223JF","≤21","≤ 7","≤15"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12184JF",1250,"DC",0.18,"± 5",31,13,24.5,27.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12184JF","≤31","≤13","≤24.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12183KFW",1250,"DC",1.7999999999999999E-2,"±10",21,6.5,19.5,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12183KFW","≤21","≤ 7","≤19.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12154KFB",1250,"DC",0.15,"±10",31,12,28,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12154KFB","≤31","≤12","≤28"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12153KF",1250,"DC",1.4999999999999999E-2,"±10",21,6,13.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12153KF","≤21","≤ 6","≤13.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12153JF",1250,"DC",1.4999999999999999E-2,"± 5",21,6,13.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12153JF","≤21","≤ 6","≤13.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12123RKF",1250,"DC",1.2E-2,"±10",21,5.5,18,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12123RKF",{"$f":"IF(L6756<=9.5,\"≤ \"&ROUNDUP(L6756*1,0)/1,\"≤\"&ROUNDUP(L6756*1,0)/1)","v":"≤21"},{"$f":"IF(M6756<=9,\"≤ \"&ROUNDUP(M6756*1,0)/1,\"≤\"&ROUNDUP(M6756*1,0)/1)","v":"≤ 6"},{"$f":"IF(N6756<=9.5,\"≤ \"&ROUNDUP(N6756*2,0)/2,\"≤\"&ROUNDUP(N6756*2,0)/2)","v":"≤18"}]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12104KFB",1250,"DC",0.1,"±10",31,10,24.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12104KFB","≤31","≤10","≤24.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12104JFB",1250,"DC",0.1,"± 5",31,10,24.5,22.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12104JFB","≤31","≤10","≤24.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE12103JFW",1250,"DC",0.01,"± 5",21,5,17.5,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE12103JFW","≤21","≤ 5","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1185RKF",100,"DC",1.8,"±10",18.399999999999999,6.5,19.399999999999999,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1185RKF","≤19","≤ 7","≤19.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1185JFW",100,"DC",1.8,"± 5",18.5,6.5,19.399999999999999,10,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1185JFW","≤19","≤ 7","≤19.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1155KF",100,"DC",1.5,"±10",18.5,6,13.4,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1155KF","≤19","≤ 6","≤13.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1155JF3",100,"DC",1.5,"± 5",18.5,6,18.399999999999999,5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","25.4P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1155JF3","≤19","≤ 6","≤18.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1125KF",100,"DC",1.2,"±10",18.5,5.5,12.8,15,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1125KF","≤19","≤ 6","≤13"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1106JFB",100,"DC",10,"± 5",26,11.5,26,15,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1106JFB","≤26","≤12","≤26"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE1106JF",100,"DC",10,"± 5",26,11.5,21,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE1106JF","≤26","≤12","≤21"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10823RKF",1000,"DC",0.18,"±10",26,10.5,27,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10823RKF","≤26","≤11","≤27"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10823KFB",1000,"DC",8.2000000000000003E-2,"±10",21,9,23.5,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10823KFB","≤21","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10683JFW",1000,"DC",6.8000000000000005E-2,"± 5",21,8.5,23,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10683JFW","≤21","≤ 9","≤23"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10563KFW",1000,"DC",5.6000000000000001E-2,"±10",21,7.5,22,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10563KFW","≤21","≤ 8","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10563JFW",1000,"DC",5.6000000000000001E-2,"± 5",21,7.5,22,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10563JFW","≤21","≤ 8","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10473KF",1000,"DC",4.7E-2,"±10",21,7.5,15.5,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10473KF","≤21","≤ 8","≤15.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10393JFW",1000,"DC",3.9E-2,"± 5",21,7,19.5,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10393JFW","≤21","≤ 7","≤19.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10393JFB",1000,"DC",3.9E-2,"± 5",21,7,19.5,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10393JFB","≤21","≤ 7","≤19.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10333JF",1000,"DC",3.3000000000000002E-2,"± 5",21,6.5,14,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10333JF","≤21","≤ 7","≤14"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10273KFW",1000,"DC",2.7E-2,"±10",21,6,18,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10273KFW","≤21","≤ 6","≤18"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10224KFB",1000,"DC",0.22,"±10",26,12,28,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10224KFB","≤26","≤12","≤28"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10223KF",1000,"DC",2.1999999999999999E-2,"±10",15.5,7.5,15.5,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10223KF","≤16","≤ 8","≤15.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10223JFB",1000,"DC",2.1999999999999999E-2,"± 5",15.5,7.5,22.5,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10223JFB","≤16","≤ 8","≤22.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10223JF",1000,"DC",2.1999999999999999E-2,"± 5",15.5,7.5,13.5,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10223JF","≤16","≤ 8","≤13.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184KFW",1000,"DC",0.18,"±10",26,10.5,27,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184KFW","≤26","≤11","≤27"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184KFB",1000,"DC",0.18,"±10",26,10.5,27,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184KFB","≤26","≤11","≤27"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184KF",1000,"DC",0.18,"±10",26,10.5,22,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184KF","≤26","≤11","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184JFW",1000,"DC",0.18,"± 5",26,10.5,27,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184JFW","≤26","≤11","≤27"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184JFB",1000,"DC",0.18,"± 5",26,10.5,27,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184JFB","≤26","≤11","≤27"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10184JF",1000,"DC",0.18,"± 5",26,10.5,22,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10184JF","≤26","≤11","≤22"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183RKF",1000,"DC",1.7999999999999999E-2,"±10",15.5,7.5,20,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183RKF","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183RJF",1000,"DC",1.7999999999999999E-2,"± 5",15.5,7.5,20,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",400,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183RJF","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183KFW",1000,"DC",1.7999999999999999E-2,"±10",15.5,7.5,20,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183KFW","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183KFB",1000,"DC",1.7999999999999999E-2,"±10",15.5,7.5,20,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183KFB","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183KF",1000,"DC",1.7999999999999999E-2,"±10",15.5,7.5,13,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183KF","≤16","≤ 8","≤13"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183JFW",1000,"DC",1.7999999999999999E-2,"± 5",15.5,7.5,20,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183JFW","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183JFB",1000,"DC",1.7999999999999999E-2,"± 5",15.5,7.5,20,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183JFB","≤16","≤ 8","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10183JF",1000,"DC",1.7999999999999999E-2,"± 5",15.5,7.5,13,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10183JF","≤16","≤ 8","≤13"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154KFW",1000,"DC",0.15,"±10",26,10,25,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154KFW","≤26","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154KFB",1000,"DC",0.15,"±10",26,10,25,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154KFB","≤26","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154KF",1000,"DC",0.15,"±10",26,10,20,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154KF","≤26","≤10","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154JFW",1000,"DC",0.15,"± 5",26,10,25,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154JFW","≤26","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154JFB",1000,"DC",0.15,"± 5",26,10,25,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154JFB","≤26","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10154JF",1000,"DC",0.15,"± 5",26,10,20,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10154JF","≤26","≤10","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153RKF",1000,"DC",1.4999999999999999E-2,"±10",15.5,7,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153RKF","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153RJF",1000,"DC",1.4999999999999999E-2,"± 5",15.5,7,17.5,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153RJF","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153KFW",1000,"DC",1.4999999999999999E-2,"±10",15.5,7,17.5,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153KFW","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153KFB",1000,"DC",1.4999999999999999E-2,"±10",15.5,7,17.5,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153KFB","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153KF",1000,"DC",1.4999999999999999E-2,"±10",15.5,7,12.5,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153KF","≤16","≤ 7","≤12.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153JFW",1000,"DC",1.4999999999999999E-2,"± 5",15.5,7,17.5,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153JFW","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153JFB",1000,"DC",1.4999999999999999E-2,"± 5",15.5,7,17.5,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153JFB","≤16","≤ 7","≤17.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10153JF",1000,"DC",1.4999999999999999E-2,"± 5",15.5,7,12.5,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10153JF","≤16","≤ 7","≤12.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124KFW",1000,"DC",0.12,"±10",26,9,23.5,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124KFW","≤26","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124KFB",1000,"DC",0.12,"±10",26,9,23.5,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124KFB","≤26","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124KF",1000,"DC",0.12,"±10",26,9,18.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124KF","≤26","≤ 9","≤18.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124JFW",1000,"DC",0.12,"± 5",26,9,23.5,17.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124JFW","≤26","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124JFB",1000,"DC",0.12,"± 5",26,9,23.5,17.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124JFB","≤26","≤ 9","≤23.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10124JF",1000,"DC",0.12,"± 5",26,9,18.5,22.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10124JF","≤26","≤ 9","≤18.5"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123RKF",1000,"DC",1.2E-2,"±10",15.5,6,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123RKF","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123RJF",1000,"DC",1.2E-2,"± 5",15.5,6,17,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123RJF","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123KFW",1000,"DC",1.2E-2,"±10",15.5,6,17,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123KFW","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123KFB",1000,"DC",1.2E-2,"±10",15.5,6,17,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123KFB","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123KF",1000,"DC",1.2E-2,"±10",15.5,6,12,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123KF","≤16","≤ 6","≤12"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123JFW",1000,"DC",1.2E-2,"± 5",15.5,6,17,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123JFW","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123JFB",1000,"DC",1.2E-2,"± 5",15.5,6,17,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123JFB","≤16","≤ 6","≤17"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10123JF",1000,"DC",1.2E-2,"± 5",15.5,6,12,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10123JF","≤16","≤ 6","≤12"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104RKF",1000,"DC",0.1,"±10",21,10,25,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104RKF","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104RJF",1000,"DC",0.1,"± 5",21,10,25,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",300,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104RJF","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104KFW",1000,"DC",0.1,"±10",21,10,25,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104KFW","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104KFB",1000,"DC",0.1,"±10",21,10,25,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104KFB","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104KF",1000,"DC",0.1,"±10",21,10,20,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104KF","≤21","≤10","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104JFW",1000,"DC",0.1,"± 5",21,10,25,12.5,"Double crimped lead wire type (Style T)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104JFW","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104JFB",1000,"DC",0.1,"± 5",21,10,25,12.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104JFB","≤21","≤10","≤25"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10104JF",1000,"DC",0.1,"± 5",21,10,20,17.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10104JF","≤21","≤10","≤20"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103RKF",1000,"DC",0.01,"±10",15.5,6,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103RKF","≤16","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103RJF",1000,"DC",0.01,"± 5",15.5,6,16,7.5,"Inner crimped lead wire type (Style B)","-40 to 105 (85)","30.0P crimped lead taping (ammo packing)",500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103RJF","≤16","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103KFW",1000,"DC",0.01,"±10",15.5,6,16,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103KFW","≤16","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103KFB",1000,"DC",0.01,"±10",15.5,6,16,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103KFB","≤16","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103KF",1000,"DC",0.01,"±10",15.5,6,11,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103KF","≤16","≤ 6","≤11"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103JFW",1000,"DC",0.01,"± 5",15.5,6,16,12.5,"Double crimped lead wire type (Style N)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103JFW","≤16","≤ 6","≤16"]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103JFB",1000,"DC",0.01,"± 5",15.5,6,16,12.5,"Crimped lead wire type (Style D)","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103JFB",{"$f":"IF(L6948<=9.5,\"≤ \"&ROUNDUP(L6948*1,0)/1,\"≤\"&ROUNDUP(L6948*1,0)/1)","v":"≤16"},{"$f":"IF(M6948<=9,\"≤ \"&ROUNDUP(M6948*1,0)/1,\"≤\"&ROUNDUP(M6948*1,0)/1)","v":"≤ 6"},{"$f":"IF(N6948<=9.5,\"≤ \"&ROUNDUP(N6948*2,0)/2,\"≤\"&ROUNDUP(N6948*2,0)/2)","v":"≤16"}]
[null,"Std","dip","PET","No","ECQE(F)[DC]","ECQE10103JF",1000,"DC",0.01,"± 5",15.5,6,11,12.5,"Straight lead wire type","-40 to 105 (85)","Bulk (Bag packing)",100,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECQE10103JF","≤16","≤ 6","≤11"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H823JX9",50,"DC",8.2000000000000003E-2,"± 5",4.8,3.3,2.1,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H823JX9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H823GX9",50,"DC",8.2000000000000003E-2,"± 2",4.8,3.3,2.1,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H823GX9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H822JX5",50,"DC",8.2000000000000007E-3,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H822JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H822GX5",50,"DC",8.2000000000000007E-3,"± 2",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H822GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H821JX5",50,"DC",8.1999999999999998E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H821JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H821GX5",50,"DC",8.1999999999999998E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H821GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H683JX9",50,"DC",6.8000000000000005E-2,"± 5",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H683JX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H683GX9",50,"DC",6.8000000000000005E-2,"± 2",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H683GX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H682JX5",50,"DC",6.7999999999999996E-3,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H682JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H682GX5",50,"DC",6.7999999999999996E-3,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H682GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H681JX5",50,"DC",6.8000000000000005E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H681JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H681GX5",50,"DC",6.8000000000000005E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H681GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H563JX9",50,"DC",5.6000000000000001E-2,"± 5",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H563JX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H563GX9",50,"DC",5.6000000000000001E-2,"± 2",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H563GX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H562JX5",50,"DC",5.5999999999999999E-3,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H562JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H562GX5",50,"DC",5.5999999999999999E-3,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H562GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H561JX5",50,"DC",5.5999999999999995E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H561JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H561GX5",50,"DC",5.5999999999999995E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H561GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H473JX9",50,"DC",4.7E-2,"± 5",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H473JX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H473GX9",50,"DC",4.7E-2,"± 2",4.8,3.3,1.5,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H473GX9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H472JX5",50,"DC",4.7000000000000002E-3,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H472JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H472GX5",50,"DC",4.7000000000000002E-3,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H472GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H471JX5",50,"DC",4.6999999999999999E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H471JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H471GX5",50,"DC",4.6999999999999999E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H471GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H393JX5",50,"DC",3.9E-2,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H393JX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H393GX5",50,"DC",3.9E-2,"± 2",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H393GX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H392JX5",50,"DC",3.8999999999999998E-3,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H392JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H392GX5",50,"DC",3.8999999999999998E-3,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H392GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H391JX5",50,"DC",3.8999999999999999E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H391JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H391GX5",50,"DC",3.8999999999999999E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H391GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H333JX5",50,"DC",3.3000000000000002E-2,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H333JX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H333GX5",50,"DC",3.3000000000000002E-2,"± 2",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H333GX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H332JX5",50,"DC",3.3E-3,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H332JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H332GX5",50,"DC",3.3E-3,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H332GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H331JX5",50,"DC",3.3E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H331JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H331GX5",50,"DC",3.3E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H331GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H273JX5",50,"DC",2.7E-2,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H273JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H273GX5",50,"DC",2.7E-2,"± 2",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H273GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H272JX5",50,"DC",2.7000000000000001E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H272JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H272GX5",50,"DC",2.7000000000000001E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H272GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H271JX5",50,"DC",2.7E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H271JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H271GX5",50,"DC",2.7E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H271GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H224JX9",50,"DC",0.22,"± 5",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H224JX9","≤ 6","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H224GX9",50,"DC",0.22,"± 2",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H224GX9","≤ 6","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H223JX5",50,"DC",2.1999999999999999E-2,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H223JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H223GX5",50,"DC",2.1999999999999999E-2,"± 2",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H223GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H222JX5",50,"DC",2.2000000000000001E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H222JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H222GX5",50,"DC",2.2000000000000001E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H222GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H221JX5",50,"DC",2.2000000000000001E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H221JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H221GX5",50,"DC",2.2000000000000001E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H221GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H184JX9",50,"DC",0.18,"± 5",6,4.0999999999999996,2.5,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H184JX9","≤ 6","≤ 5","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H184GX9",50,"DC",0.18,"± 2",6,4.0999999999999996,2.5,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H184GX9","≤ 6","≤ 5","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H183JX5",50,"DC",1.7999999999999999E-2,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H183JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H183GX5",50,"DC",1.7999999999999999E-2,"± 2",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H183GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H182JX5",50,"DC",1.8E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H182JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H182GX5",50,"DC",1.8E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H182GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H181JX5",50,"DC",1.8000000000000001E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H181JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H181GX5",50,"DC",1.8000000000000001E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H181GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H154JX9",50,"DC",0.15,"± 5",6,4.0999999999999996,1.9,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H154JX9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H154GX9",50,"DC",0.15,"± 2",6,4.0999999999999996,1.9,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H154GX9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H153JX5",50,"DC",1.4999999999999999E-2,"± 5",3.2,2.5,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H153JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H153GX5",50,"DC",1.4999999999999999E-2,"± 2",3.2,2.5,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H153GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H152JX5",50,"DC",1.5E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H152JX5",{"$f":"IF(L7012<=9.5,\"≤ \"&ROUNDUP(L7012*1,0)/1,\"≤\"&ROUNDUP(L7012*1,0)/1)","v":"≤ 2"},{"$f":"IF(M7012<=9,\"≤ \"&ROUNDUP(M7012*1,0)/1,\"≤\"&ROUNDUP(M7012*1,0)/1)","v":"≤ 2"},{"$f":"IF(N7012<=9.5,\"≤ \"&ROUNDUP(N7012*2,0)/2,\"≤\"&ROUNDUP(N7012*2,0)/2)","v":"≤ 1"}]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H152GX5",50,"DC",1.5E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H152GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H151JX5",50,"DC",1.4999999999999999E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H151JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H151GX5",50,"DC",1.4999999999999999E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H151GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H124JX9",50,"DC",0.12,"± 5",6,4.0999999999999996,1.9,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H124JX9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H124GX9",50,"DC",0.12,"± 2",6,4.0999999999999996,1.9,"'-","Non lead wire","-55 to 125 (105)","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H124GX9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H123JX5",50,"DC",1.2E-2,"± 5",3.2,2.5,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H123JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H123GX5",50,"DC",1.2E-2,"± 2",3.2,2.5,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H123GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H122JX5",50,"DC",1.1999999999999999E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H122JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H122GX5",50,"DC",1.1999999999999999E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H122GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H121JX5",50,"DC",1.2E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H121JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H121GX5",50,"DC",1.2E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H121GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H104JX9",50,"DC",0.1,"± 5",4.8,3.3,2.1,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H104JX9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H104GX9",50,"DC",0.1,"± 2",4.8,3.3,2.1,"'-","Non lead wire","-55 to 125","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H104GX9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H103JX5",50,"DC",0.01,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H103JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H103GX5",50,"DC",0.01,"± 2",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H103GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H102JX5",50,"DC",1E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H102JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H102GX5",50,"DC",1E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H102GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H101JX5",50,"DC",1E-4,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H101JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1H101GX5",50,"DC",1E-4,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1H101GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C823JX5",16,"DC",8.2000000000000003E-2,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C823JX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C823GX5",16,"DC",8.2000000000000003E-2,"± 2",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C823GX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C822JX5",16,"DC",8.2000000000000007E-3,"± 5",2,1.25,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C822JX5","≤ 2","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C822GX5",16,"DC",8.2000000000000007E-3,"± 2",2,1.25,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C822GX5","≤ 2","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C821JX5",16,"DC",8.1999999999999998E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C821JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C821GX5",16,"DC",8.1999999999999998E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C821GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C683JX5",16,"DC",6.8000000000000005E-2,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C683JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C683GX5",16,"DC",6.8000000000000005E-2,"± 2",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C683GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C682JX5",16,"DC",6.7999999999999996E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C682JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C682GX5",16,"DC",6.7999999999999996E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C682GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C681JX5",16,"DC",6.8000000000000005E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C681JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C681GX5",16,"DC",6.8000000000000005E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C681GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C563JX5",16,"DC",5.6000000000000001E-2,"± 5",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C563JX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C563GX5",16,"DC",5.6000000000000001E-2,"± 2",3.2,2.5,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C563GX5","≤ 4","≤ 3","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C562JX5",16,"DC",5.5999999999999999E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C562JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C562GX5",16,"DC",5.5999999999999999E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C562GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C561JX5",16,"DC",5.5999999999999995E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C561JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C561GX5",16,"DC",5.5999999999999995E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C561GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C473JX5",16,"DC",4.7E-2,"± 5",3.2,1.6,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C473JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C473GX5",16,"DC",4.7E-2,"± 2",3.2,1.6,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C473GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C472JX5",16,"DC",4.7000000000000002E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C472JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C472GX5",16,"DC",4.7000000000000002E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C472GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C471JX5",16,"DC",4.6999999999999999E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C471JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C471GX5",16,"DC",4.6999999999999999E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C471GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C393JX5",16,"DC",3.9E-2,"± 5",3.2,1.6,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C393JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C393GX5",16,"DC",3.9E-2,"± 2",3.2,1.6,1.5,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C393GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C392JX5",16,"DC",3.8999999999999998E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C392JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C392GX5",16,"DC",3.8999999999999998E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C392GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C391JX5",16,"DC",3.8999999999999999E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C391JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C391GX5",16,"DC",3.8999999999999999E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C391GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C333JX5",16,"DC",3.3000000000000002E-2,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C333JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C333GX5",16,"DC",3.3000000000000002E-2,"± 2",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C333GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C332JX5",16,"DC",3.3E-3,"± 5",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C332JX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C332GX5",16,"DC",3.3E-3,"± 2",2,1.25,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C332GX5","≤ 2","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C331JX5",16,"DC",3.3E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C331JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C331GX5",16,"DC",3.3E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C331GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C273JX5",16,"DC",2.7E-2,"± 5",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C273JX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C273GX5",16,"DC",2.7E-2,"± 2",3.2,1.6,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C273GX5","≤ 4","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C272JX5",16,"DC",2.7000000000000001E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C272JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C272GX5",16,"DC",2.7000000000000001E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C272GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C271JX5",16,"DC",2.7E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C271JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C271GX5",16,"DC",2.7E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C271GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C223JX5",16,"DC",2.1999999999999999E-2,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C223JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C223GX5",16,"DC",2.1999999999999999E-2,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C223GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C222JX5",16,"DC",2.2000000000000001E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C222JX5",{"$f":"IF(L7076<=9.5,\"≤ \"&ROUNDUP(L7076*1,0)/1,\"≤\"&ROUNDUP(L7076*1,0)/1)","v":"≤ 2"},{"$f":"IF(M7076<=9,\"≤ \"&ROUNDUP(M7076*1,0)/1,\"≤\"&ROUNDUP(M7076*1,0)/1)","v":"≤ 1"},{"$f":"IF(N7076<=9.5,\"≤ \"&ROUNDUP(N7076*2,0)/2,\"≤\"&ROUNDUP(N7076*2,0)/2)","v":"≤ 1"}]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C222GX5",16,"DC",2.2000000000000001E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C222GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C221JX5",16,"DC",2.2000000000000001E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C221JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C221GX5",16,"DC",2.2000000000000001E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C221GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C183JX5",16,"DC",1.7999999999999999E-2,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C183JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C183GX5",16,"DC",1.7999999999999999E-2,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C183GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C182JX5",16,"DC",1.8E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C182JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C182GX5",16,"DC",1.8E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C182GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C181JX5",16,"DC",1.8000000000000001E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C181JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C181GX5",16,"DC",1.8000000000000001E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C181GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C153JX5",16,"DC",1.4999999999999999E-2,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C153JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C153GX5",16,"DC",1.4999999999999999E-2,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C153GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C152JX5",16,"DC",1.5E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C152JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C152GX5",16,"DC",1.5E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C152GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C151JX5",16,"DC",1.4999999999999999E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C151JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C151GX5",16,"DC",1.4999999999999999E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C151GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C123JX5",16,"DC",1.2E-2,"± 5",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C123JX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C123GX5",16,"DC",1.2E-2,"± 2",3.2,1.6,0.9,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C123GX5","≤ 4","≤ 2","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C122JX5",16,"DC",1.1999999999999999E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C122JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C122GX5",16,"DC",1.1999999999999999E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C122GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C121JX5",16,"DC",1.2E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C121JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C121GX5",16,"DC",1.2E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C121GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C104JX5",16,"DC",0.1,"± 5",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C104JX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C104GX5",16,"DC",0.1,"± 2",3.2,2.5,2.1,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C104GX5","≤ 4","≤ 3","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C103JX5",16,"DC",0.01,"± 5",2,1.25,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C103JX5","≤ 2","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C103GX5",16,"DC",0.01,"± 2",2,1.25,1.1000000000000001,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C103GX5","≤ 2","≤ 2","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C102JX5",16,"DC",1E-3,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C102JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C102GX5",16,"DC",1E-3,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C102GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C101JX5",16,"DC",1E-4,"± 5",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C101JX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(X)","ECHU1C101GX5",16,"DC",1E-4,"± 2",1.6,0.8,0.7,"'-","Non lead wire","-55 to 125","8.0W180A emboss taping (reel packing)",4000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1C101GX5","≤ 2","≤ 1","≤ 1"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1823JC9",100,"DC",8.2000000000000003E-2,"± 5",7.1,5,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1823JC9","≤ 8","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1823GC9",100,"DC",8.2000000000000003E-2,"± 2",7.1,5,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1823GC9","≤ 8","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1683JC9",100,"DC",6.8000000000000005E-2,"± 5",6,4.0999999999999996,3.2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1683JC9","≤ 6","≤ 5","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1683GC9",100,"DC",6.8000000000000005E-2,"± 2",6,4.0999999999999996,3.2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1683GC9","≤ 6","≤ 5","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1563JC9",100,"DC",5.6000000000000001E-2,"± 5",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1563JC9","≤ 6","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1563GC9",100,"DC",5.6000000000000001E-2,"± 2",6,4.0999999999999996,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1563GC9","≤ 6","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1473JC9",100,"DC",4.7E-2,"± 5",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1473JC9","≤ 6","≤ 5","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1473GC9",100,"DC",4.7E-2,"± 2",6,4.0999999999999996,2.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1473GC9","≤ 6","≤ 5","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1393JC9",100,"DC",3.9E-2,"± 5",6,4.0999999999999996,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1393JC9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1393GC9",100,"DC",3.9E-2,"± 2",6,4.0999999999999996,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1393GC9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1333JC9",100,"DC",3.3000000000000002E-2,"± 5",6,4.0999999999999996,1.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1333JC9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1333GC9",100,"DC",3.3000000000000002E-2,"± 2",6,4.0999999999999996,1.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1333GC9","≤ 6","≤ 5","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1273JC9",100,"DC",2.7E-2,"± 5",4.8,3.3,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1273JC9","≤ 5","≤ 4","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1273GC9",100,"DC",2.7E-2,"± 2",4.8,3.3,2.8,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1273GC9","≤ 5","≤ 4","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1224JCV",100,"DC",0.22,"± 5",7.1,6.3,4.8,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1224JCV","≤ 8","≤ 7","≤ 5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1224GCV",100,"DC",0.22,"± 2",7.1,6.3,4.8,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1224GCV","≤ 8","≤ 7","≤ 5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1223JC9",100,"DC",2.1999999999999999E-2,"± 5",4.8,3.3,2.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1223JC9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1223GC9",100,"DC",2.1999999999999999E-2,"± 2",4.8,3.3,2.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",2000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1223GC9","≤ 5","≤ 4","≤ 2.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1184JCV",100,"DC",0.18,"± 5",7.1,6.3,4,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1184JCV","≤ 8","≤ 7","≤ 4"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1184GCV",100,"DC",0.18,"± 2",7.1,6.3,4,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1184GCV","≤ 8","≤ 7","≤ 4"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1183JC9",100,"DC",1.7999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1183JC9","≤ 5","≤ 4","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1183GC9",100,"DC",1.7999999999999999E-2,"± 2",4.8,3.3,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1183GC9","≤ 5","≤ 4","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1154JCV",100,"DC",0.15,"± 5",7.1,6.3,3.4,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1154JCV","≤ 8","≤ 7","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1154GCV",100,"DC",0.15,"± 2",7.1,6.3,3.4,"'-","Non lead wire","-55 to 105","16.0W embossed carrier taping (reel packing)",1000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1154GCV","≤ 8","≤ 7","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1153JC9",100,"DC",1.4999999999999999E-2,"± 5",4.8,3.3,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1153JC9","≤ 5","≤ 4","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1153GC9",100,"DC",1.4999999999999999E-2,"± 2",4.8,3.3,2,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1153GC9","≤ 5","≤ 4","≤ 2"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1124JC9",100,"DC",0.12,"± 5",7.1,5,3.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1124JC9","≤ 8","≤ 5","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1124GC9",100,"DC",0.12,"± 2",7.1,5,3.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1124GC9","≤ 8","≤ 5","≤ 3.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1123JC9",100,"DC",1.2E-2,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1123JC9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1123GC9",100,"DC",1.2E-2,"± 2",4.8,3.3,1.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1123GC9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1104JC9",100,"DC",0.1,"± 5",7.1,5,3,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1104JC9","≤ 8","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1104GC9",100,"DC",0.1,"± 2",7.1,5,3,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",1500,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1104GC9","≤ 8","≤ 5","≤ 3"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1103JC9",100,"DC",0.01,"± 5",4.8,3.3,1.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1103JC9","≤ 5","≤ 4","≤ 1.5"]
[null,"Std","chip","PPS","No","ECHU(C)","ECHU1103GC9",100,"DC",0.01,"± 2",4.8,3.3,1.4,"'-","Non lead wire","-55 to 105","12.0W embossed carrier taping (reel packing)",3000,"https://industrial.panasonic.com/ww/products/pt/film-cap-electroequip/models/ECHU1103GC9","≤ 5","≤ 4","≤ 1.5"]

{"sheet":"Utility","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}